<!-- section: DICT_Q-Z | pages: 341-344 | verified: true -->

# Page 341 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **PROCEDURE (n)** | Steps that are in a THIS SECTION GIVES sequence THE PROCEDURE TO DISASSEMBLE THE COMPONENT FULLY. |
| **proceed (v) — UNNAPROVED** | CONTINUE (v) CONTINUE WITH THE Proceed with the ELECTRICAL TEST. electrical test. process (in the DURING (prep) DURING THIS REPAIR, Apply sufficient heat to process of ) (prep) APPLY SUFFICIENT the unit in the process of HEAT TO THE UNIT. doing this repair. |
| **WHILE (conj)** | WHILE YOU DO THIS Apply sufficient heat to REPAIR, APPLY the unit in the process of SUFFICIENT HEAT TO doing this repair. THE UNIT. |
| **process (n) — UNNAPROVED** | PROCEDURE (n) THESE TWO These two assembly ASSEMBLY processes are almost PROCEDURES ARE the same. ALMOST THE SAME. This word is a CORROSION IS AN technical noun ELECTROLYTIC when it means a PROCESS. sequence of changes that occur and cause a result. |
| **process (v) — UNNAPROVED** | DO (v) THE … PUT THE PARTS IN AN Process the parts in an |
| **PROCEDURE (n)** | ELECTROLYTIC BATH. electrolytic bath. THEN, DO THE ELECTROPLATING PROCEDURE. |
| **produce (v) — UNNAPROVED** | CAUSE (v) ELECTRICAL Electrical equipment can EQUIPMENT CAN produce interference in CAUSE communication. INTERFERENCE IN COMMUNICATION. |
| **GIVE (v)** | A DILUTED SOLUTION A diluted solution does WILL NOT GIVE YOU not produce the correct THE CORRECT results. RESULTS. |
| **MAKE (v)** | WHEN THE LEVER The lever produces a ENGAGES, IT MAKES A click when engaged. CLICK |
| **SUPPLY (v)** | THE POWER UNIT The power unit produces SUPPLIES THE a voltage of 28 V DC. SYSTEM WITH A VOLTAGE OF 28 V DC. |

# Page 342 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **product (n) — UNNAPROVED** | Be accurate. If it WHEN YOU CLEAN When you clean this is possible, use THIS UNIT, USE THE unit, use the correct the name of the CORRECT SOLVENT. product. product. TRICHLOROETHANE This product is IS A DANGEROUS dangerous. MATERIAL. |
| **profile (n) — UNNAPROVED** | CONTOUR (n) MAKE SURE THAT THE Make sure that the CONTOUR OF THE profile of the template is TEMPLATE IS THE the same. SAME. |
| **program (n) — UNNAPROVED** | SEQUENCE (n) DISASSEMBLE THE Disassemble the rotor ROTOR IN THIS according to the SEQUENCE: following program: |
| **progress (n) — UNNAPROVED** | CONTINUE (v) MAKE SURE THAT THE Monitor the progress of TEST CONTINUES the test. Also refer to SATISFACTORILY. IN PROGRESS (adv). |
| **progress (v) — UNNAPROVED** | CONTINUE (v) YOU CAN CONTINUE You can progress with THE TEST. the test. |
| **progressive (adj) — UNNAPROVED** | GRADUALLY (adv) GRADUALLY TORQUE Apply progressive torque THE NUT. to the nut. |
| **progressively (adv) — UNNAPROVED** | GRADUALLY (adv) TORQUE THE BOLTS Torque the bolts GRADUALLY. progressively. |
| **prohibit (v) — UNNAPROVED** | PREVENT (v) PUT A WARNING Display a warning notice NOTICE ON THE on the panel prohibiting PANEL TO PREVENT the operation of the OPERATION OF THE controls. CONTROLS. TELL (NOT TO) (v) TELL THE PERSONNEL Prohibit the use of NOT TO USE asbestos parts. ASBESTOS PARTS. |
| **prolonged (adj) — UNNAPROVED** | LONG (adj) OPERATION OF THE Prolonged motor MOTOR FOR LONG operation can cause PERIODS CAN CAUSE damage. DAMAGE TO IT. |
| **prompt (adj) — UNNAPROVED** | IMMEDIATELY (adv) IF YOU SWALLOW Prompt action is required SOLVENT, DO NOT if you swallow solvent. CAUSE VOMITING. GET MEDICAL AID IMMEDIATELY. |

# Page 343 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **propagation (n) — UNNAPROVED** | INCREASE (v) IF THE DIMENSION OF Crack propagation can A CRACK INCREASES, cause the part to break. THE PART CAN BREAK. If it is possible, IF THE DEPTH OF A Crack propagation can give the CRACK IS MORE THAN cause the rejection of dimensions or 0.2 mm, REJECT THE the part. limits. PART. IF A CRACK IS Crack propagation can LARGER THAN 0.2 mm, cause the rejection of REJECT THE PART. the part. |
| **proper (adj) — UNNAPROVED** | CORRECT (adj) DO A CHECK FOR THE Check the unit for proper CORRECT OPERATION operation. OF THE UNIT. |
| **properly (adv) — UNNAPROVED** | CORRECTLY (adv) CLOSE THE DOORS Close the doors properly. CORRECTLY. |
| **PROPERTY (n)** | A characteristic or THE MAGNETIC attribute of an object PROPERTIES OF THIS METAL DECREASE AT HIGH TEMPERATURES. |
| **PROPORTION (n)** | The ratio of something to ALWAYS MIX something else CLEANING AGENTS WITH COLD WATER IN THE CORRECT For other PROPORTIONS. meanings, use: |
| **RELATION (n)** | THE TEMPERATURE The temperature DECREASES IN decreases in proportion RELATION TO THE to the altitude. ALTITUDE. |
| **proportional (adj) — UNNAPROVED** | RELATION (n) THE CENTER OF Movement of the center GRAVITY MOVES IN of gravity is proportional RELATION TO THE to the loads on the LOADS ON THE wings. WINGS. |
| **PROPORTION (n)** | MIX THE PIGMENT Mix the correct quantity AND SOLVENT IN THE of pigment proportional CORRECT to the quantity of solvent. PROPORTIONS. |

# Page 344 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
proportionally RELATION (n) THE CABLE TENSION The cable tension
(adv) CHANGES IN changes proportionally
RELATION TO THE with temperature.

### TEMPERATURE.

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **protect (v) — UNNAPROVED** | PREVENT (v) USE CELLOPHANE TO Use cellophane to PREVENT DAMAGE TO protect the surface from THE SURFACE. damage. |
| **PROTECTION (n)** | MAKE SURE THAT ALL Make sure that all sharp SHARP EDGES HAVE edges are protected with VINYL TAPE vinyl tape. PROTECTION. |
| **PROTECTION (n)** | Something to prevent APPLY TWO LAYERS injury, damage, or OF SEALING failure COMPOUND ON THE SURFACES THAT HAVE NO PROTECTION. |
| **PROTECTIVE (adj)** | That gives protection REMOVE THE PROTECTIVE LAYER. |
| **PROTRUDE (v)** | To be farther forward or IF THE POP-OUT PROTRUDES out from an adjacent INDICATOR PROTRUDED surface PROTRUDES, PROTRUDED REPLACE THE FILTER ELEMENT. |
| **provide (v) — UNNAPROVED** | GIVE (v) THIS SECTION GIVES This section provides the THE PROCEDURES procedures for the storage FOR THE STORAGE of the component. FO THE COMPONENT. |
| **SUPPLY (v)** | THE HYDRAULIC The hydraulic system SYSTEM SUPPLIES provides pressure for PRESSURE FOR THE operating the flight OPERATION OF THE controls. FLIGHT CONTROLS. |
| **provided (that) — UNNAPROVED** | IF (conj) IF A REPLACEMENT Provided that a (conj) PART IS AVAILABLE, replacement part is REPLACE THE available, replace the DAMAGED SHIELD. damaged shield. |
