<!-- section: DICT_G-P | pages: 273-276 | verified: true -->

# Page 273 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **huge (adj) — UNNAPROVED** | LARGE (adj) TO REMOVE THE To remove the paint PAINT STRIPPER, stripper, flush the FLUSH THE SURFACE surface with huge WITH LARGE quantities of water. QUANTITIES OF WATER. |
| **hum (v) — UNNAPROVED** | HUM (TN) ADJUST THE Adjust the potentiometer POTENTIOMETER until the loudspeaker no UNTIL YOU DO NOT longer hums. HEAR A HUM FROM THE LOUDSPEAKER. |
| **hurt (v) — UNNAPROVED** | INJURY (n) BE CAREFUL WHEN Be careful when you do YOU DO THIS this procedure. If the unit PROCEDURE. IF THE falls, it can hurt persons. UNIT FALLS, IT CAN CAUSE INJURY TO PERSONS. |
| **HYDRAULIC (adj)** | Related to, or operated CONNECT THE by, pressurized liquid FITTINGS TO THE HYDRAULIC TEST BENCH. HYDRAULICALLY With hydraulic power MAKE SURE THAT THE (adv) LINES ARE HYDRAULICALLY OPERATED. |

---

# Page 274 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example
Blank Page
Page 2-1-H8 Part 2 - Dictionary Issue 9
2025-01-15

---

# Page 275 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **identical (adj) — UNNAPROVED** | SAME (adj) THE SAME The procedure is PROCEDURE IS identical for both VHF APPLICABLE TO THE sets. TWO VHF SETS. IDENTIFICATION Something that identifies MAKE SURE THAT THE (n) an object NAMEPLATE SHOWS THE CORRECT IDENTIFICATION OF THE UNIT. |
| **IDENTIFY (v)** | , 1. To use a specified IDENTIFY THE WIRES IDENTIFIES, code or marking to WITH SLEEVES OF IDENTIFIED, supply with an DIFFERENT COLORS. IDENTIFIED identity 2. To show an identity A 406 MHz DIGITAL SIGNAL IDENTIFIES THE EMERGENCY LOCATOR TRANSMITTER AND For other ITS LOCATION. meanings, use: |
| **FIND (v)** | FIND THE DAMAGED Identify the damaged AREAS. areas. |
| **idle (v) — UNNAPROVED** | IDLE (TN) OPERATE THE Idle the engine for ENGINE AT IDLE FOR 20 minutes. 20 MINUTES. |
| **IF (conj)** | In the event that, on the IF YOU USE A condition that, in case of REPLACEMENT FAIRING PLATE, CUT IT UNTIL YOU GET THE CORRECT MATING DIMENSION. |
| **ignite (v) — UNNAPROVED** | IGNITION (TN) FUEL GOES THROUGH Fuel passes through the THE ATOMIZERS INTO atomizers to the THE COMBUSTION combustion chamber, CHAMBER, WHERE where it is ignited. IGNITION OCCURS. |
| **IGNORE (v)** | , Not to think about IGNORE THE IGNORES, something, not to do VIBRATION IGNORED, something about INDICATIONS. IGNORED SELECT “CANCEL” TO IGNORE ALL CHANGES. |

---

# Page 276 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **ILLUMINATE (v)** | , To make something THE EMERGENCY ILLUMINATES, visible with an external LIGHTS COME ON TO ILLUMINATED, light source ILLUMINATE THE ILLUMINATED EVACUATION PATH. For lights or lamps, use: COME ON WHEN THE PRESSURE When the pressure light LIGHT COMES ON, illuminates, read the READ THE VALUE ON value on the pressure THE PRESSURE gauge. GAUGE. MAKE SURE THAT THE Ensure the lamp LAMP COMES ON. illuminates. BE ON MAKE SURE THAT THE Ensure the lamp is LAMP IS ON. illuminated. |
| **immediate (adj) — UNNAPROVED** | IMMEDIATELY (adv) MAKE SURE THAT THE Check the speedbrake SPEEDBRAKE for immediate retraction. RETRACTS IMMEDIATELY. IMMEDIATELY Without a gap of time or MAKE SURE THAT THE (adv) space EMERGENCY LIGHT IMMEDIATELY GOES BACK TO ”OFF.” |
| **immerse (v) — UNNAPROVED** | SOAK (v) SOAK THE FILTER IN Immerse the filter in the THE CLEANING cleaning solution for SOLUTION FOR 4 hours. 4 HOURS. PUT FULLY INTO PUT THE FILTER Immerse the filter in FULLY INTO THE solvent. SOLVENT. |
| **immobilize (v) — UNNAPROVED** | LOCK (v) LOCK THE PULLEY Immobilize the pulley WITH THE RIGGING with the rigging pin. PIN. PREVENT MOVEMENT WHEN YOU REPAIR Immobilize the THE UNIT, PREVENT assemblies when MOVEMENT OF THE repairing the unit. ASSEMBLIES. |
| **impact (n) — UNNAPROVED** | HIT (v) MAKE SURE THAT Avoid impact between METAL OBJECTS DO metal objects and the NOT HIT THE MATING mating surface. SURFACE. |
