<!-- GROUP: 024-appendix -->
<!-- PAGES: 427-434 -->
<!-- SECTION: APPENDIX -->
<!-- KEY:  -->
<!-- WORKERS: R107, R108, R109 -->
<!-- PAGE_COUNT: 8 -->

# Appendix

> **Source:** ASD-STE100 Issue 9, January 2025
> **Section:** APPENDIX
> **Pages:** 427-434 of 434 (8 pages)

# Page 429 of 434

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **whose (pron) — UNNAPROVED** | Use a different THE GENERATORS The generators produce construction. SUPPLY A THREE- a three-phase voltage PHASE VOLTAGE. THE whose frequency is FREQUENCY OF THIS proportional to the VOLTAGE INCREASES generator rotor speed. WHEN THE GENERATOR ROTOR SPEED INCREASES. |
| **WIDE (adj)** | That has a specified or REPAIR ALL CRACKS (WIDER, large width THAT ARE WIDER WIDEST) THAN 0,05 mm. |
| **WIDTH (n)** | The smaller of two MEASURE THE WIDTH dimensions, the second- OF THE CRACK AT largest of three THE WIDEST POINT. dimensions |
| **WILL (v)** | Auxiliary modal verb that WARNINGS AND shows simple future CAUTIONS IN THIS No other verb tense MANUAL WILL HELP forms. YOU TO DO THE WORK SAFELY AND CORRECTLY. |
| **WIND (v)** | , To move around and WIND THE TAPE ON WINDS, around an object THE REEL. WOUND, WOUND |
| **windy (adj) — UNNAPROVED** | WIND (TN) WHEN THERE ARE Take special precautions STRONG WINDS, in very windy conditions. OBEY THESE SPECIAL PRECAUTIONS. |
| **wipe (v) — UNNAPROVED** | CLEAN (v) BEFORE EACH CYCLE, Wipe the indicator CLEAN THE surfaces before each INDICATOR. cycle. |
| **wire (v) — UNNAPROVED** | ATTACH (v) ATTACH THE HOSE TO Wire the hose to the (WITH WIRE [TN]) THE FIXTURE WITH fixture. WIRE. |
| **wire-lock (v) — UNNAPROVED** | LOCK (v) LOCK THE FOUR Wire-lock the four bolts (WITH LOCKWIRE [TN]) BOLTS TO EACH to each other. OTHER WITH LOCKWIRE. |
| **SAFETY (v)** | SAFETY THE FOUR Wire-lock the four bolts (WITH SAFETY WIRE BOLTS TO EACH to each other. [TN]) OTHER WITH SAFETY WIRE. |

<!-- Page 430 of 434 -->

| **WITH (prep)** | Function word that ALIGN THE MARK shows association or WITH THE relationship, help or LONGITUDINAL AXIS. sharing, a means or instrument Refer to ATTACH THE FLANGE section 9, GR-2. (10) WITH THE FOUR BOLTS (15). REMOVE THE VALVE (2) WITH THE EXTRACTOR. |
| **withdraw (v) — UNNAPROVED** | REMOVE (v) REMOVE THE Withdraw the indicator INDICATOR FROM THE from the instrument INSTRUMENT PANEL. panel. |
| **within (prep) — UNNAPROVED** | IN (prep) A FILTER PREVENTS A filter prevents CONTAMINATION OF contamination of the THE COMPONENTS IN components within the THE SYSTEM. system. IN ... OR LESS LIGHT L4 COMES ON Light L4 illuminates IN 5 SECONDS OR within 5 seconds. LESS. IN LESS THAN MAKE SURE THAT THE Make sure that the WARNING LIGHT warning light illuminates COMES ON IN LESS within 3 seconds. THAN 3 SECONDS. |
| **WITHOUT (prep)** | Not with SMALL DAMAGE IS PERMITTED WITHOUT REPAIR. REFER TO TABLE 1 FOR THE APPLICABLE LIMITS. |
| **withstand (v) — UNNAPROVED** | RESISTANT (adj) THIS MATERIAL IS This material can RESISTANT TO FIRE. withstand fire. |
| **WORK (n)** | That which you do when DO THE WORK IN A you use physical CLEAN AREA. strength, or mental power |
| **work (v) — UNNAPROVED** | WORK (n) BE CAREFUL WHEN Be careful when you YOU DO WORK NEAR work near fuel tanks. FUEL TANKS. |
| **would (v) — UNNAPROVED** | CAN (v) SOLVENTS THAT STAY Solvents left on the part ON THE PART CAN would corrode the part. CAUSE CORROSION. |

<!-- Page 431 of 434 -->

| **wrap (v) — UNNAPROVED** | PUT (v) PUT THE PART IN Wrap the part in OILPAPER. oilpaper. |
| **WIND (v)** | WIND MASKING TAPE Wrap masking tape AROUND THE PART. around the part. |
| **WRITE (v)** | , To record data or WRITE THE TEST WRITES, information as words, DATE ON THE WROTE, letters, or symbols CERTIFICATE. WRITTEN |
| **wrong (adj) — UNNAPROVED** | INCORRECT (adj) IDENTIFY THE Mark the bellcrank and BELLCRANK AND shaft to prevent wrong SHAFT WITH MARKS. installation. THESE MARKS WILL PREVENT AN INCORRECT INSTALLATION. |
| **wrongly (adv) — UNNAPROVED** | INCORRECTLY (adv) IF THE HOSES ARE Damage can occur if INCORRECTLY hoses are wrongly INSTALLED, DAMAGE installed. CAN OCCUR. |

# Page 432 of 434

Blank Page

# Page 433 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 433–434 of 434

## Unapproved Words

#### yet (conj) — unapproved

- **Approved alternative:** BUT (conj)

> **STE:** TIGHTEN THE NUTS, BUT KEEP THEM SUFFICIENTLY LOOSE TO REMOVE THEM WITH YOUR HAND.
> **Non-STE:** The nuts should be tightened, yet loose enough to remove by hand.

> **See:** Dictionary entry for BUT (conj).

#### yet (adv) — unapproved

- **Approved alternative:** AT THIS TIME

> **STE:** DO NOT REMOVE THE FIXTURE COVER AT THIS TIME.
> **Non-STE:** Do not remove the fixture cover yet.

#### yourself (pron) — unapproved

- **Approved alternative:** YOU (pron)

> **STE:** DO NOT USE YOUR HANDS TO PREVENT MOVEMENT OF THE LP COMPRESSOR. IF YOU DO, THE LP COMPRESSOR CAN CAUSE YOU INJURY AND CAN CAUSE DAMAGE TO THE EQUIPMENT.
> **Non-STE:** Do not use your hands to prevent movement of the LP compressor. If you do, you can cause injury to yourself and damage to the equipment.

> **See:** Dictionary entry for YOU (pron).

#### zero (v) — unapproved

- **Approved alternative:** ZERO (TN)

> **STE:** ADJUST THE METER TO ZERO.
> **Non-STE:** Zero the meter.

> **See:** Dictionary entry for ZERO (TN).

## Approved Words

#### YES (adv) — APPROVED

- **Meaning:** Function word that shows the positive answer to a question.
- **Example:**

> **STE:** DOES THE LIGHT COME ON? YES OR NO?

#### YOU (pron) — APPROVED

- **Meaning:** The reader or the user.
- **Examples:**

> **STE:** YOU CAN CONTINUE THE TEST.
> **STE:** HOT SURFACES CAN BURN YOU.

#### YOUR (adj) — APPROVED

- **Meaning:** Related to the reader or the user.
- **Example:**

> **STE:** IF YOU GET SOLVENT IN YOUR EYES, FLUSH THEM IMMEDIATELY WITH WATER.

---

*Page 434 is intentionally blank (end of Part 2 – Dictionary, Issue 9, 2025-01-15).*
