# Page 161–164 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 161–164 of 434

# Page 161 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| associated (adj) — UNNAPPROVED | CORRECT (adj) | INSTALL THE DUMP VALVE AND THE CORRECT GASKET. | Install the dump valve with the associated gasket. |
|  | RELATED (adj) | REMOVE THE RELATED DOORS. | Remove the panels from the associated doors. |
|  | ITS (adj) | REMOVE THE BOLT AND ITS WASHER. | Remove the bolt and the associated washer. |
|  | THEIR (adj) | REMOVE THE EIGHT BOLTS AND THEIR WADGERS. | Remove the eight bolts and the associated washers. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | <p>If damage is assumed to</p> <p>be repairable, refer to</p> <p>the repair section.</p> |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |

# Page 162 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| ATTACH (v), ATTACHES, ATTACHED, ATTACHED | To stay together or to cause different items to stay together | MAKE SURE THAT THE LABEL FULLY ATTACHES TO THE SURFACE AND THAT THERE ARE NO BUBBLES. |  |
| ATTACH (v), ATTACHES, ATTACHED, ATTACHED |  | TEMPORARILY ATTACH THE CABLE TO THE ADJACENT STRUCTURE. |  |
| attachment (n) — UNNAPPROVED | ATTACH (v) | MAKE SURE THAT THE DUCT IS CORRECTLY ATTACHED TO THE FILTER. | Make sure that the attachment of the duct to the filter is correct. |
| attain (v) — UNNAPPROVED | SHOW (v) | WHEN THE VOLTMETER SHOWS 28 VOLTS DC, THE RELAY CLOSES. | When 28 volts DC is attained, the relay closes. |
|  | BE (v) | WHEN THE VOLTAGE IS 28 VOLTS DC, THE RELAY CLOSES. | When 28 volts DC is attained, the relay closes. |
|  | GET (v) | WHEN YOU GET 28 VOLTS DC, THE RELAY CLOSES. | When 28 volts DC is attained, the relay closes. |
| attempt (n) — UNNAPPROVED | TRY (v) | TRY TO LIFT THE COVER MANUALLY. | Make an attempt to lift the cover manually. |
| attempt (v) — UNNAPPROVED | TRY (v) | TRY TO FIND THE DEFECT. | Attempt to find the defect. |
| attention (n) — UNNAPPROVED | AID (n) | IF YOU GET PAINT SPRAY IN YOUR EYES, GET MEDICAL AID. | If you get paint spray in your eyes, get medical attention. |
|  | CAREFUL (adj) | BE CAREFUL WHEN YOU REMOVE THE CONTROL UNIT. | Pay attention when you remove the control unit. |
|  | MONITOR (v) | MONITOR THE RESULTS. | Pay attention to the results. |

# Page 163 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| audible (adj) — UNNAPPROVED | HEAR (v) | IF YOU CANNOT HEAR THE ALARM, ADJUST THE VOLUME CONTROL. | If the alarm is not audible, adjust the volume control. |
|  | LISTEN (v) | LISTEN FOR AIR LEAKAGE FROM THE LINES. | Check the lines for audible air leakage. |
| augment (v) — UNNAPPROVED | INCREASE (v) | A MIXTURE OF WATER AND METHANOL INCREASES THE POWER OF THE ENGINE. | A mixture of water and methanol augments the power of the engine. |
| aurally (adv) — UNNAPPROVED | LISTEN (v) | LISTEN TO MAKE SURE THAT THE FLUID FLOWS. | Check aurally to ensure fluid flow. |
|  | HEAR (v) | YOU CAN HEAR THE WARNING IN THE COCKPIT. | The warning is given aurally in the cockpit. |
| authentic (adj) — UNNAPPROVED | ACCURATE (adj) | IF THE ADJUSTMENT OF THE STOPS IS NOT CORRECT, THE RESULTS OF THE TEST WILL NOT BE ACCURATE. | If the adjustment of the stops is not correct, the results of the test will not be authentic. |
| AUTHORITY (n) | An official organization that gives approval to something | BEFORE YOU CHANGE THE PROCEDURE, GET THE APPROVAL OF THE DESIGN AUTHORITY. |  |
| authorized (adj) — UNNAPPROVED | APPROVED (adj) | ONLY APPROVED PERSONS ARE PERMITTED TO STAY IN THIS AREA. | Only authorized persons are permitted to stay in this area. |
| AUTOMATIC (adj) | That operates without other input | THE AUTOMATIC SYSTEM WILL OPEN THE DOORS. |  |
| AUTOMATICALLY (adv) | That operates without other input | THE FUEL FLOW STOPS AUTOMATICALLY. |  |

# Page 164 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| AUXILIARY (adj) | 1. That operates in a secondary function | LUBRICANTS FOR THE ENGINE AND THE AUXILIARY EQUIPMENT ARE THE SAME. |  |
| AUXILIARY (adj) | 2. That gives help | USE AUXILIARY SCREWS TO ASSEMBLE THE UNIT TEMPORARILY. |  |
| AVAILABLE (adj) | Prepared or supplied for you to use | IF ELECTRICAL POWER IS AVAILABLE, DO A CONTINUITY CHECK. |  |
| avert (v) — UNNAPPROVED | PREVENT (v) | IF THE MICROSWITCH BECOMES UNSERVICEABLE, DEACTIVATE THE ACTUATOR TO PREVENT DAMAGE TO THE VALVE. | If the microswitch becomes unserviceable, deactivate the actuator to avert damage to the valve. |
| avoid (v) — UNNAPPROVED | PREVENT (v) | TURN THE CONTROLS SLOWLY TO PREVENT DAMAGE. | Turn the controls slowly to avoid damage. |
|  | DO NOT | DO NOT PUSH ON THE SEALS. | Avoid pushing on the seals. |
| aware (adj) — UNNAPPROVED | KNOW (v) | ALL PERSONNEL MUST KNOW THE HEALTH RISKS. | All personnel must be aware of the health risks. |
|  | TELL (v) | TELL ALL PERSONNEL ABOUT THE NEW RULES. | All personnel must be aware of the new rules. |
| AWAY FROM (prep) | In or to a different position or direction | DO THE WORK IN AN AREA AWAY FROM EQUIPMENT OR METAL FRAME BUILDINGS. |  |
| AXIAL (adj) | Related to an axis | DO STEPS 1 THRU 4 TO MAKE SURE THAT NO AXIAL LOAD IS ON THE ROD. |  |
| AXIALLY (adv) | Related to an axis | APPLY THE LOAD AXIALLY. |  |
