# Page 249–252 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 249–252 of 434

# Page 249 of 434

|||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|||**fulfill (v) — UNNAPPROVED**|ABEY (v)|ABEY THE<br>INSTRUCTIONS IN THE<br>TEST PROCEDURE.|Fulfill the instructions in<br>the test procedure.|
|||THIS PROCEDURE<br>ABEYS ALL THE<br>REQUIREMENTS OF<br>SERVICE BULLETIN<br>No. 97.|This procedure fulfills all<br>the requirements of<br>Service Bulletin No. 97.|
|||**FULL (adj)**<br>**(FULLER,**<br>**FULLEST)**|At or related to<br>maximum travel, length,<br>quantity, or detail|MAKE SURE THAT THE<br>RESERVOIR IS FULL.|
|||**FULLY (adv)**|At or related to<br>maximum travel, length,<br>quantity, or detail|TURN THE CONTROL<br>TO THE FULLY<br>CLOSED POSITION.|
|||**FUNCTION (n)**|Action or activity that a<br>person or thing does|THE PRIMARY<br>FUNCTION OF THIS<br>UNIT IS TO CONTROL<br>THE FUEL FLOW.|
|||**function (v) — UNNAPPROVED**|OPERATE (v)|THE ELEVATOR<br>CONTROLS MUST<br>OPERATE SMOOTHLY.|The elevator controls<br>must function smoothly.|
|||MOVE (v)|THE SYSTEM<br>CONTROLS MUST<br>MOVE FREELY.|The system controls<br>must function freely.|
|||**fundamental (adj) — UNNAPPROVED**|IMPORTANT (adj)|DURING THIS<br>PROCEDURE, IT IS<br>IMPORTANT TO KEEP<br>ALL PARTS CLEAN.|Cleanliness of all parts is<br>fundamental in this<br>procedure.|
|||**further (adj) — UNNAPPROVED**|MORE (adj)|IF YOU DO NOT GET<br>THE CORRECT<br>DIMENSION, ADD<br>MORE GASKETS.|If you do not get the<br>correct dimension, add<br>further gaskets.|
|||**further (adv) — UNNAPPROVED**|MORE (adv)|IF IT IS NECESSARY<br>TO DECREASE THE<br>CABLE TENSION<br>MORE, USE THE<br>TURNBUCKLE.|Cable tension can be<br>further reduced if<br>necessary by means of<br>the turnbuckle.|

# Page 250 of 434

|||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|||**gain (n) — UNNAPPROVED**|INCREASE (v)|AFTER THE LAST<br>MODIFICATION, THE<br>SYSTEM'S<br>EFFICIENCY<br>INCREASED.|The system's efficiency<br>showed a gain after the<br>last modification.|
|||**gain (v) — UNNAPPROVED**|GET (v)|GET ACCESS TO THE<br>CONNECTORS AT THE<br>REAR OF THE<br>INSTRUMENT.|Gain access to the<br>connectors at the back<br>of the Instrument.|
|||**gall (v) — UNNAPPROVED**|GALLING (TN)|THERE MUST BE NO<br>SCRATCHES OR<br>GALLING ON THE<br>SURFACE.|The surface must not be<br>scratched or galled.|
|||**gap (n) — UNNAPPROVED**|CLEARANCE (n)|MEASURE THE<br>CLEARANCE<br>BETWEEN THE<br>IMPELLER AND THE<br>BODY.|Measure the gap<br>between the impeller<br>and the body.|
|||DISTANCE (n)|MEASURE THE<br>DISTANCE BETWEEN<br>THE ROTARY<br>ACTUATOR AND THE<br>STOP BOLT.|Measure the gap<br>between the rotary<br>actuator and the stop<br>bolt.|
|||SPACE (n)|PUT THE BLADE OF A<br>SMALL SCREWDRIVER<br>INTO THE SPACE<br>BETWEEN THE COVER<br>AND THE HOUSING.|Put the blade of a small<br>screwdriver into the gap<br>between the cover and<br>the housing.|
|||**garbled (adj) — UNNAPPROVED**|CLEAR (adj)|IF THE RADIO SIGNAL<br>IS NOT CLEAR,<br>ADJUST THE<br>FREQUENCY.|If the radio signal is<br>garbled, adjust the<br>frequency.|
|||CLEARLY (adv)|MAKE SURE THAT<br>YOU TRANSMIT THE<br>ANNOUNCEMENT<br>CLEARLY.|Make sure that the<br>announcement is not<br>garbled.|

# Page 251 of 434

|||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|||**garner (v) — UNNAPPROVED**|COLLECT (v)|THESE COMPUTERS<br>COLLECT DATA FROM<br>THE VHF SYSTEM.|These computers garner<br>data from the VHF<br>system.|
|||THE BITE FUNCTION<br>COLLECTS THE<br>FAILURES AND SENDS<br>THE FAILURE<br>MESSAGE TO THE<br>CENTRAL<br>MAINTENANCE<br>COMPUTER.|The BITE function<br>garners the failures and<br>sends the failure<br>message to the Central<br>Maintenance Computer.|
|||**GAS (n)**|A fluid that has no shape<br>or volume and that can<br>expand|<br>THE TEMPERATURE<br>SENSING UNIT IS A<br>CAPILLARY TUBE<br>FILLED WITH GAS.|
|||**gaseous (adj) — UNNAPPROVED**|GAS (n)|THE TOOL CYLINDER<br>CONTAINS A MIXTURE<br>OF GASES<br>(10% HELIUM AND<br>90% NITROGEN).|The tool cylinder<br>contains a gaseous<br>mixture of 10% helium<br>and 90% nitrogen.|
|||**gash (v) — UNNAPPROVED**|DAMAGED (adj)|IF THE THERMAL<br>BLANKET IS<br>DAMAGED, DO<br>REPAIR No. 9.|If the thermal blanket is<br>gashed, do repair No. 9.|
|||**gather (v) — UNNAPPROVED**|COLLECT (v)|ALL FLUIDS COLLECT<br>AT THE LOWEST<br>POINT IN THE<br>COMPARTMENT.|All fluids gather at the<br>lowest point in the<br>compartment.|
|||THREE COMPUTERS<br>COLLECT DATA AND<br>PARAMETERS FROM<br>THE SYSTEMS AND<br>PUT THEM TOGETHER<br>ON THE DATA LINK TO<br>THE DISPLAY UNIT.|Three computers gather<br>data and parameters<br>from the systems and<br>put them together on the<br>data link to the display<br>unit.|
|||**gauge (v) — UNNAPPROVED**|MEASURE (v)|MEASURE THE<br>DISTANCE BETWEEN<br>THE TOP EDGE AND<br>THE BOTTOM<br>SURFACE.|Gauge the width of the<br>gap between the top<br>edge and the bottom<br>surface.|
|||**GENERAL (adj)**|Of, or related to<br>something as a whole,<br>not detailed|THIS SECTION GIVES<br>GENERAL<br>MAINTENANCE<br>PROCEDURES.|

# Page 252 of 434

|||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|||**generally (adv) — UNNAPPROVED**|USUALLY (adv)|YOU USUALLY<br>REPLACE MEMORY<br>MODULES DURING<br>MAINTENANCE.|Memory modules are<br>generally replaced<br>during Maintenance.|
|||**generate (v) — UNNAPPROVED**|BE (v)|THERE MUST BE NO<br>ERRORS WHEN YOU<br>OPEN THE FILE.|The file opening must<br>not generate errors.|
|||GIVE (v)|IF THE HYDRAULIC<br>PUMP DOES NOT GIVE<br>A PRESSURE OF<br>3000 psi, USE THE<br>ELECTRIC PUMP.|If the hydraulic pump<br>fails to generate a<br>pressure of 3000 Psi,<br>use the electric pump.|
|||SUPPLY (v)|THE BATTERIES<br>SUPPLY 28 V DC.|The batteries generate<br>28 V DC.|
|||**generous (adj) — UNNAPPROVED**|LARGE (adj)|A LARGE QUANTITY<br>OF COMPOUND IS<br>NECESSARY.|A generous amount of<br>compound will be<br>necessary.|
|||THICK (adj)<br>If it is possible, be<br>accurate.|APPLY A THICK LAYER<br>OF GREASE.|Apply a generous<br>amount of grease.|
|||**generously (adv) — UNNAPPROVED**|LARGE (adj)|APPLY A LARGE<br>QUANTITY OF<br>SEALANT TO THE<br>REPAIR PATCH.|Apply sealant<br>generously to the repair<br>patch.|
|||THICK (adj)<br>If it is possible, be<br>accurate.|APPLY A THICK LAYER<br>OF GREASE.|Apply grease<br>generously.|
|||**gentle (adj) — UNNAPPROVED**|CAREFULLY (adv)|TURN THE<br>POTENTIOMETER<br>CAREFULLY.|Rotate the potentiometer<br>with a gentle movement.|
|||LIGHTLY (adv)|TAP THE SURFACE<br>LIGHTLY.|Give the surface a gentle<br>tap.|
|||**gently (adv) — UNNAPPROVED**|CAREFULLY (adv)|CAREFULLY PULL THE<br>ELECTRICAL WIRE<br>OUT FROM THE<br>RUBBER SEAL.|Gently pull out the<br>electrical wire from the<br>rubber seal.|
|||LIGHTLY (adv)|LIGHTLY TAP THE TOP<br>SURFACE UNTIL THE<br>PARTS ALIGN.|Gently tap the top<br>surface until the parts<br>align.|
