<!-- section: DICT_A-F | pages: 233-236 | verified: true -->

# Page 233 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **enough (adj) — UNNAPROVED** | SUFFICIENT (adj) MAKE SURE THAT Make sure that there is THERE IS SUFFICIENT enough pressure in the PRESSURE IN THE accumulator. ACCUMULATOR. |
|| **ensue (v) — UNNAPROVED** | CAUSE (v) INCORRECT Damage will ensue from INSTALLATION WILL incorrect installation. CAUSE DAMAGE. |
|| **ensure (v) — UNNAPROVED** | MAKE SURE (v) MAKE SURE THAT THE Ensure that the correct CORRECT SEALS ARE seals are installed. INSTALLED. |
|| **enter (v) — UNNAPROVED** | GO INTO DO NOT GO INTO THE Do not enter the LABORATORY laboratory without WITHOUT APPROVAL. approval. |
|| **RECORD (v)** | RECORD THE DATA IN Enter the data in the THE LOGBOOK. logbook. |
|| **ENTRY (n)** | MAKE AN ENTRY IN Enter in the logbook that THE LOGBOOK TO you did the deactivation SHOW THAT YOU DID procedure. THE DEACTIVATION PROCEDURE. |
|| **entire (adj) — UNNAPROVED** | FULL (adj) THE ANTENNA MAKES The antenna makes a A SCAN OF THE FULL scan of the entire range RANGE OF of frequencies. FREQUENCIES. |
|| **ALL (adj)** | EXAMINE ALL OF THE Check the entire system SYSTEM TO FIND THE to determine the cause CAUSE OF THE of interference. INTERFERENCE. |
|| **entirely (adv) — UNNAPROVED** | FULLY (adv) THE SYSTEM IS FULLY The system is entirely AUTOMATIC. automatic. |
|| **ENTRANCE (n)** | An opening to go into a PUT SAFETY space BARRIERS AT THE ENTRANCE TO THE WORK AREA. |

# Page 234 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **ENTRY (n)** | A record of an MAKE AN ENTRY IN occurrence THE LOG CARD. |
|| **EQUAL (adj)** | The same dimension, MAKE SURE THAT quality, quantity, or THERE IS AN EQUAL number DISTANCE BETWEEN THE HOLES. |
|| **equal (v) — UNNAPROVED** | SAME (adj) DIMENSION "X" MUST Dimension X must equal BE THE SAME AS dimension Z. DIMENSION "Z." |
|| **EQUAL (adj)** | DIMENSION "X" MUST Dimension X must equal BE EQUAL TO dimension Y. DIMENSION "Y." |
|| **EQUALLY (adv)** | The same dimension, ADJUST THE quality, quantity, or TURNBUCKLES number EQUALLY. |
|| **equip (v) — UNNAPROVED** | INSTALL (v) INSTALL THE Equip each HP manifold SHUTOFF VALVES ON with shutoff valves. EACH HP MANIFOLD. |
|| **EQUIPMENT (n)** | The objects or tools REMOVE ALL THE used for operation and EQUIPMENT FROM maintenance THE WORK AREA. |
|| **equipped (adj) — UNNAPROVED** | HAVE (v) BE CAREFUL WHEN Be careful when YOU MOVE JET PIPES handling jet pipes or OR EXHAUST CONES exhaust cones equipped THAT HAVE with insulating blankets. INSULATING BLANKETS. |
|| **EQUIVALENT (adj)** | Has the same MATERIALS properties, functions, or (REF. No. 2) AND values (REF. No. 18) ARE EQUIVALENT. |
|| **EQUIVALENT (n)** | Something that has the USE CLEANING same properties, COMPOUND ARDROX functions, or values 6025, OR AN EQUIVALENT. |
|| **ERASE (v)** | , To remove data from a ERASE THE TAPE. ERASES, medium ERASED, ERASED |

# Page 235 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **erect (v) — UNNAPROVED** | ASSEMBLE (v) BEFORE YOU LIFT THE Erect the movable hoist GEARBOX, ASSEMBLE before lifting the THE MOVABLE HOIST. gearbox. BECOME STABLE LET THE VERTICAL Give the vertical gyro GYRO BECOME time to erect. STABLE. |
|| **erratic (adj) — UNNAPROVED** | IRREGULAR (adj) THE OPERATION OF The compass is erratic. THE COMPASS IS IRREGULAR. |
|| **ERROR (n)** | The difference from that IF THE ERROR IS which is correct or MORE THAN 3 DEG., accurate CALIBRATE THE COMPASS. |
|| **escape (v) — UNNAPROVED** | DEFLATE (v) DEFLATE THE TIRE. Let the air escape from the tire. |
|| **RELEASE (v)** | RELEASE ALL THE Allow all the nitrogen to NITROGEN. escape. |
|| **establish (v) — UNNAPROVED** | MAKE SURE (v) IN THE STEP THAT In the following step, FOLLOWS, MAKE establish the correct SURE THAT THE FUEL functioning of the fuel PUMP OPERATES pump. CORRECTLY. |
|| **ESTIMATE (n)** | A calculated, MAKE AN ESTIMATE approximate result OF THE NECESSARY QUANTITY OF PAINT. |
|| **estimate (v) — UNNAPROVED** | ESTIMATE (n) MAKE AN ESTIMATE Estimate the amount of OF THE QUANTITY OF cleaning fluid that is CLEANING FLUID THAT necessary. IS NECESSARY. |
|| **evaluate (v) — UNNAPROVED** | EXAMINE (v) EXAMINE THE Evaluate the damage DAMAGE AFTER AN after an accident. ACCIDENT. ANALYSIS (TN) MAKE AN ANALYSIS Evaluate the test results. OF THE TEST RESULTS. |

# Page 236 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

|| Word (POS) | Meaning & Examples |
||------------|-------------------|
|| **evaluation (n) — UNNAPROVED** | EXAMINE (v) EXAMINE THE Do an evaluation of the DAMAGE. damage. ANALYSIS (TN) MAKE AN ANALYSIS Do an evaluation of the OF THE TEST test results. RESULTS. |
|| **evaporate (v) — UNNAPROVED** | DRY (v) LET THE COMPOUND Allow the solvent to DRY. evaporate from the compound. |
|| **even (adj) — UNNAPROVED** | SMOOTH (adj) A GUIDE ROD IS A guide rod is attached ATTACHED TO THE to the metal bellows disc METAL BELLOWS for an even movement of DISC FOR A SMOOTH the bellows. MOVEMENT OF THE BELLOWS. |
|| **SAME (adj)** | APPLY THE SAME Braking must be even on LOAD ON THE TWO the two brakes. BRAKES. |
|| **FLAT (adj)** | MAKE SURE THAT Ensure the surface is THE SURFACE IS even. FLAT. |
|| **FLUSH (adj)** | MAKE SURE THAT Make sure that the THE FASTENER fastener heads are even HEADS ARE FLUSH with the skin. WITH THE SKIN. |
|| **LEVEL (adj)** | MAKE SURE THAT Make sure that the mark THE MARK ON THE on the bolt is even with BOLT IS LEVEL WITH the mark on the handle. THE MARK ON THE HANDLE. |
|| **evenly (adv) — UNNAPROVED** | GRADUALLY (adv) INCREASE THE Increase the TEMPERATURE temperature evenly. GRADUALLY. |
|| **EQUALLY (adv)** | APPLY THE LOAD Apply the load evenly on EQUALLY ON THE the area. AREA. |
|| **event (n) — UNNAPROVED** | IF (conj) IF THE PRESSURE In the event of a sudden DECREASES dropping of pressure, SUDDENLY, CLOSE close the valve. THE VALVE. |
|| **eventually (adv) — UNNAPROVED** | SOME TIME IF THE CABLE RUBS, If the cable chafes, it will IT WILL BREAK AFTER eventually break. SOME TIME. |
