<!-- GROUP: 014-dict-a-b -->
<!-- PAGES: 142-174 -->
<!-- SECTION: DICT -->
<!-- KEY: A-B -->
<!-- WORKERS: R036, R037, R038, R039, R040, R041, R042, R043, R044 -->
<!-- PAGE_COUNT: 33 -->

# Dict A B

> **Source:** ASD-STE100 Issue 9, January 2025
> **Section:** DICT (A-B)
> **Pages:** 142-174 of 434 (33 pages)

<!-- Page 142 of 434 -->

| Word (POS) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| ABOUT (prep) | Concerned with For other meanings, use: | FOR DATA ABOUT THE LOCATION OF CIRCUIT BREAKERS, REFER TO THE WIRING LIST. |  |
| ABOUT (prep) | APPROXIMATELY (adv) | DRAIN APPROXIMATELY 2 LITERS OF FUEL FROM THE TANK. | Drain about 2 liters of fuel from the tank. |
| ABOUT (prep) | AROUND (prep) | TURN THE SHAFT AROUND ITS AXIS. | Rotate the shaft about its axis. |
| ABOVE (prep) | In (or to) a position farther up than something | LIFT THE CYLINDER ABOVE ITS INSTALLED POSITION. |  |
| ABOVE (prep) | For other meanings, use: |  |  |
| ABOVE (prep) | MORE THAN | THE PRESSURE VALUE MUST BE MORE THAN 800 kPa. | The pressure value must be above 800 kPa. |
| ABRASIVE (adj) | That can remove material by friction | POLISH THE SURFACE WITH AN ABRASIVE PAPER. |  |
| abrupt (adj) — UNNAPPROVED | SUDDEN (adj) | THE DAMPER PREVENTS SUDDEN MOVEMENT OF THE CONTROL. | The damper prevents abrupt movement of the control. |
| abrupt (adj) — UNNAPPROVED | SUDDENLY (adv) | IF THE ROTORS STOP SUDDENLY, EXAMINE THE INTAKE FOR UNWANTED MATERIAL. | If the rotors come to an abrupt stop, examine the intake for unwanted material. |

<!-- Page 143 of 434 -->

|---|---|---|---|
| absence (n) — UNNAPPROVED | NONE (pron) | IF NONE OF THE BRACKETS ARE DAMAGED, CONTINUE THE PROCEDURE. | In the absence of damage to the brackets, continue the procedure. |
| absence (n) — UNNAPPROVED | NOT (adv) | IF THE BRACKETS ARE NOT DAMAGED, CONTINUE THE PROCEDURE. | In the absence of damage to the brackets, continue the procedure. |
| absence (n) — UNNAPPROVED | NO (adj) | IF THERE IS NO CONTAMINATION IN THE FUEL SAMPLE, CONTINUE THE PROCEDURE. | In the absence of contamination in the fuel sample, continue the procedure. |
| absent (adj) — UNNAPPROVED | MISSING (adj) | IF ONE OR MORE BLADES ARE MISSING, MAKE AN ENTRY IN THE ENGINE LOGBOOK. | If one or more blades are absent, make an entry in the engine logbook. |
| absent (adj) — UNNAPPROVED | NO (adj) | IF THERE IS NO CONTAMINATION IN THE FUEL SAMPLE, CONTINUE THE PROCEDURE. | If contamination is absent from the fuel sample, continue the procedure. |
| absolutely (adv) — UNNAPPROVED | FULLY (adv) | MAKE SURE THAT THE LATCH IS FULLY ENGAGED. | Ensure the latch is absolutely engaged. |
| ABSORB (v), ABSORBS, ABSORBED, ABSORBED | 1. To take up or into | ABSORB THE FLUID WITH A CLEAN CLOTH. |  |
| ABSORB (v), ABSORBS, ABSORBED, ABSORBED | 2. To decrease the effect of | THE SHOCK MOUNT ABSORBS THE VIBRATION. |  |
| absorption (n) — UNNAPPROVED | ABSORB (v) | MEASURE THE TIME THAT IS NECESSARY FOR THE SILICA GEL TO ABSORB THE MOISTURE. | Measure the rate of absorption of the moisture by the silica gel. |
| abundant (adj) — UNNAPPROVED | LARGE (adj) | CLEAN YOUR SKIN WITH A LARGE QUANTITY OF CLEAN WATER. | Clean your skin with abundant clean water. |

<!-- Page 144 of 434 -->

|---|---|---|---|
| abut (v) — UNNAPPROVED | TOUCH (v) | THE BIN TOUCHES THE FORWARD HINGE SURFACE. | The bin abuts the forward hinge surface. |
| accelerate (v) — UNNAPPROVED | INCREASE (v) | A HIGHER TEMPERATURE INCREASES THE SPEED OF EVAPORATION. | Evaporation is accelerated by a higher temperature. |
| accelerate (v) — UNNAPPROVED | FASTER (adj) | TO MAKE THE CURING PROCESS FASTER, APPLY HEAT TO THE COMPOUND. | The curing process of the compound can be accelerated by heating. |
| ACCEPT (v), ACCEPTS, ACCEPTED, ACCEPTED | To make a decision that something is satisfactory | ACCEPT THE RELAY IF IT IS SERVICEABLE. |  |
| acceptable (adj) — UNNAPPROVED | PERMITTED (adj) | A VALUE OF 2 mm IS PERMITTED. | A value of 2 mm is acceptable. |
| acceptable (adj) — UNNAPPROVED | SATISFACTORY (adj) | IF THE CONDITION OF THE CAP IS NOT SATISFACTORY, REPLACE IT. | Replace the cap if its condition is not acceptable. |
| acceptable (adj) — UNNAPPROVED | SERVICEABLE (adj) | BEFORE YOU INSTALL THE UNIT, MAKE SURE THAT IT IS SERVICEABLE. | Before installation, make sure that the unit is acceptable. |
| acceptance (n) — UNNAPPROVED | ACCEPT (v) | BEFORE YOU ACCEPT THE UNIT, DO THE SPECIFIED TEST PROCEDURE. | Before acceptance of the unit, do the specified test procedure. |
| ACCESS (n) | The ability to go into or near | GET ACCESS TO THE ACCUMULATOR FOR THE No. 1 HYDRAULIC SYSTEM. |  |
| accessible (adj) — UNNAPPROVED | ACCESS (n) | TURN THE COVER UNTIL YOU CAN GET ACCESS TO THE JACKS THAT HAVE + AND - MARKS. | Rotate the cover until the jacks marked by + and - are accessible. |
| ACCIDENT (n) | An occurrence that causes injury or damage | TO PREVENT ACCIDENTS, MAKE SURE THAT THE PINS ARE INSTALLED. |  |

<!-- Page 145 of 434 -->

|---|---|---|---|
| ACCIDENTAL (adj) | That does not occur on purpose | TO PREVENT ACCIDENTAL OPERATION OF THE SYSTEM, INSTALL THE SAFETY LOCK. |  |
| ACCIDENTALLY (adv) | That does not occur on purpose | IF YOU ACCIDENTALLY MOVE THE LEVER, SET THE SYSTEM TO THE NEUTRAL POSITION AGAIN. |  |
| accommodate (v) — UNNAPPROVED | LET (v) | DIFFERENT LENGTHS OF STUDS LET YOU ATTACH DIFFERENT THICKNESSES OF SKIN. | Studs are available in different lengths to accommodate different thicknesses of skin. |
| accomplish (v) — UNNAPPROVED | DO (v) You can use a more accurate verb. | DO THIS TASK FIRST. | This task must be accomplished first. |
| accomplish (v) — UNNAPPROVED | COMPLETE (v) | THE PERSONNEL MUST COMPLETE THIS TASK IN 30 MINUTES. | The personnel must accomplish this task in 30 minutes. |
| according to (prep) | REFER (v) | TO CALIBRATE THE TEST SET, REFER TO THE MANUFACTURER'S INSTRUCTIONS. | Calibrate the test set according to the manufacturer's instructions. |
| account for (v) — UNNAPPROVED | MAKE SURE (v) | MAKE SURE THAT YOU REMOVE ALL TOOLS AND EQUIPMENT. | All tools and equipment must be accounted for. |
| accumulate (v) — UNNAPPROVED | COLLECT (v) | IF WATER COLLECTS IN THE FILLER LINE, DRAIN IT. | If water accumulates in the filler line, drain it. |
| accumulation (n) — UNNAPPROVED | QUANTITY (n) | REMOVE LARGE QUANTITIES OF CONTAMINATION. | Large accumulations of contamination must be removed. |
| accumulation (n) — UNNAPPROVED | COLLECT (v) | IF FUEL COLLECTS FREQUENTLY, EXAMINE THE PIPE FOR LEAKS. | If accumulation of fuel is frequent, examine the pipe for leaks. |

<!-- Page 146 of 434 -->

|---|---|---|---|
| accuracy (n) — UNNAPPROVED | PRECISION (n) | THE PRECISION OF THE ADJUSTMENT CAN CHANGE. | The accuracy of the adjustment can vary. |
| ACCURATE (adj) | Exact | THE ADJUSTMENT MUST BE ACCURATE. |  |
| ACCURATELY (adv) | Exactly | PUT THE REPAIR SHEET ACCURATELY ON THE DAMAGED AREA. |  |
| achieve (v) — UNNAPPROVED | GET (v) | SET THE CONTROL TO GET MAXIMUM THRUST. | Set the control to achieve maximum thrust. |
| acquire (v) — UNNAPPROVED | GET (v) | THE COMPUTER GETS THIS DATA FROM FIVE SENSORS. | The computer acquires this data from five sensors. |
| acrid (adj) — UNNAPPROVED | DANGEROUS (adj) | THIS MATERIAL RELEASES DANGEROUS FUMES WHEN IT TOUCHES HOT SURFACES. | On contact with hot surfaces, this material produces acrid fumes. |
| ACROSS (prep) | From one side to the other side | SAFETY THE CLAMP BLOCK ACROSS THE CONTROL LEVER FORKS WITH SAFETY WIRE. |  |
| act (v) — UNNAPPROVED | Use an accurate verb. | THE HYDRAULIC FLUID FLOW OPENS THE VALVE. | The hydraulic fluid flow acts on the valve. |
| action (n) — UNNAPPROVED | STEP (n) | DO THE STEPS THAT FOLLOW: | Do the following actions: |
| action (n) — UNNAPPROVED | PROCEDURE (n) | DO NOT DO THIS PROCEDURE IN THE HANGAR. | This action must not be done in the hangar: |
| action (n) — UNNAPPROVED | TASK (n) | DO THIS TASK OUTDOORS. | Do this action outdoors. |
| ACTIVATE (v) | To make a system, function, or feature ready for operation | THE AUTOPILOT ACTIVATES THE APPROACH MODE. |  |
| ACTIVATE (v) | For other meanings, use: |  |  |
| ACTIVATE (v) | START (v) | START THE MOTOR. | Activate the motor. |

<!-- Page 147 of 434 -->

|---|---|---|---|
| ACTIVE (adj) | A system, function, or feature in a state of action | DOWNLOAD THE EXPORT FILE FROM THE ACTIVE SERVER UNIT. |  |
| activity (n) — UNNAPPROVED | TASK (n) | A SUBCONTRACTOR CAN DO THESE MAINTENANCE TASKS. | These maintenance activities can be done by a subcontractor. |
| activity (n) — UNNAPPROVED | PROCEDURE (n) | DO THIS PROCEDURE AT THE AMBIENT TEMPERATURE. | Do this activity at the ambient temperature. |
| activity (n) — UNNAPPROVED | WORK (n) | DO THIS WORK IN A CLEAN AREA. | Do this activity in a clean area. |
| actuate (v) — UNNAPPROVED | START (v) | START THE MOTOR. | Actuate the motor. |
| actuate (v) — UNNAPPROVED | OPERATE (v) | OPERATE THE HAND PUMP. | Actuate the hand pump. |
| actuate (v) — UNNAPPROVED | PUSH (v) | PUSH THE PUSHBUTTON SWITCH. | Actuate the pushbutton switch. |
| actuation (n) — UNNAPPROVED | OPERATION (n) | MONITOR THE OPERATION OF THE STEERING MOTOR. | Monitor the actuation of the steering motor. |
| ADAPT (v), ADAPTS, ADAPTED, ADAPTED | To change or adjust to that which is necessary | ADAPT THE PRESSURE CONNECTION TO THE PITOT HEAD. THE SYSTEM INTERFACE CIRCUITS ADAPT TO THE PHYSICAL PROPERTIES OF THE CONNECTED SYSTEMS. |  |
| ADD (v), ADDS, ADDED, ADDED | To increase the number, dimension, or quantity | ADD 5 ml OF HARDENER TO THE COMPOUND. |  |
| addition (n) — UNNAPPROVED | ADD (v) | TO GET THE CORRECT CLEARANCE, ADD SPECIAL SHIMS, AS NECESSARY. | Adjust the clearance by the addition of special shims, as necessary. |

<!-- Page 148 of 434 -->

|---|---|---|---|
| additional (adj) — UNNAPPROVED | MORE (adj) | THIS CHAPTER GIVES MORE INFORMATION ABOUT SAFETY. | This chapter gives additional information about safety. |
| adequate (adj) — UNNAPPROVED | SUFFICIENT (adj) | MAKE SURE THAT CONTAINERS HAVE SUFFICIENT CAPACITY AND DIAMETER. | Make sure that containers have adequate capacity and diameter. |
| adhere (v) — UNNAPPROVED | BOND (v) | THE SEAL MUST BOND CORRECTLY. | The seal must adhere correctly. |
| adhere (v) — UNNAPPROVED | OBEY (v) | OBEY THE SAFETY INSTRUCTIONS. | Adhere to the safety instructions. |
| adhesion (n) — UNNAPPROVED | BOND (n) | CLEAN THE SURFACE TO MAKE SURE THAT THE BOND IS SATISFACTORY. | Clean the surface to ensure there will be good adhesion. |
| ADJACENT (adj) | That which is near to an object, with no other object of the same type between the two | DO NOT OPERATE THE ADJACENT CONTROL. |  |
| ADJACENT TO (prep) | To be near to an object, with no other object of the same type between the two | THE FUEL PUMP IS INSTALLED ADJACENT TO THE BULKHEAD. |  |
| adjoining (adj) — UNNAPPROVED | ADJACENT (adj) | ALIGN THE BRACKETS WITH THE ADJACENT COMPONENTS. | Align the brackets with the adjoining components. |
| ADJUST (v), ADJUSTS, ADJUSTED, ADJUSTED | To put in or come to a specified position or value | ADJUST THE FREQUENCY TO THE VALUE GIVEN IN TABLE 1. THE INTERNAL LOGIC ADJUSTS TO SUDDEN CHANGES IN TEMPERATURE. |  |
| ADJUSTABLE (adj) | That you can adjust | THE TWO STOP BOLTS ARE ADJUSTABLE. |  |
| ADJUSTMENT (n) | The effect of adjusting | MAKE SURE THAT THE ADJUSTMENT IS IN THE LIMITS GIVEN IN TABLE 1. |  |

<!-- Page 149 of 434 -->

|---|---|---|---|
| admit (v) — UNNAPPROVED | LET (v) | OPEN THE VALVE TO LET NITROGEN GO INTO THE OLEO STRUT. | Open the valve to admit nitrogen into the oleo strut. |
| adopt (v) — UNNAPPROVED | USE (v) | IF THE UNIT IS DAMAGED, USE THIS PROCEDURE. | Adopt this procedure if the unit is damaged. |
| advance (n) — UNNAPPROVED | FORWARD (adj) | THE FORWARD MOVEMENT OF THE CONTROL LEVER MUST BE SLOW AND CONTINUOUS. | The advance of the control lever must be slow and continuous. |
| advance (v) — UNNAPPROVED | SET (v) | SET THE THROTTLE TO MAXIMUM POWER. | Advance the throttle to maximum power. |
| advance (v) — UNNAPPROVED | FORWARD (adv) | MOVE THE LEVER FORWARD. | Advance the lever. |
| adverse (adj) — UNNAPPROVED | BAD (adj) | REFER TO CHAPTER 6 FOR INSTRUCTIONS ABOUT HOW TO PARK IN BAD WEATHER CONDITIONS. | For parking in adverse weather conditions, refer to Chapter 6. |
| adverse (adj) — UNNAPPROVED | If it is possible, give accurate and correct conditions. | THIS MEDICATION CAN CAUSE DERMATITIS. | This medication can cause adverse reactions. |
| advisable (adj) — UNNAPPROVED | RECOMMEND (v) | THE DESIGN AUTHORITY RECOMMENDS THAT YOU TORQUE THE BOLTS AGAIN AT INTERVALS OF SIX MONTHS. | According to the Design Authority, it is advisable to retorque the bolts at intervals of six months. |
| advise (v) — UNNAPPROVED | TELL (v) | TELL THE RAMP AGENT THAT THE BRAKES ARE SET. | Advise the ramp agent that the brakes are set. |
| advise (v) — UNNAPPROVED | RECOMMEND (v) | THE SAFETY OFFICER RECOMMENDS THE APPLICABLE PERSONAL PROTECTIVE EQUIPMENT. | The safety officer advises on applicable personal protective equipment. |

<!-- Page 150 of 434 -->

|---|---|---|---|
| affect (v) — UNNAPPROVED | EFFECT (n) | MAGNETIC TOOLS HAVE AN UNWANTED EFFECT ON THE COMPASS SYSTEM. | Magnetic tools affect the compass system. |
| affect (v) — UNNAPPROVED | If it is possible, be accurate. | THIS MEDICATION CAN CAUSE DERMATITIS. | This medication can affect your skin. |
| AFT (adj) | At or nearer to the rear of an air or sea vehicle | THE PUMP IS IN THE AFT CELL OF THE FUSELAGE TANK. |  |
| AFT (adv) | In the direction of the rear of an air or sea vehicle | MOVE THE THROTTLE AFT. |  |
| AFTER (conj) | That follows a specified time, sequence, or operation | AFTER YOU INSTALL THE COMPONENT, DO A FUNCTIONAL TEST. |  |
| AFTER (prep) | That follows a specified time, sequence, or operation | THE BAR MOVES DOWN AFTER 20 SECONDS. |  |
| AFT OF (prep) | At a position nearer to the rear | THE CONTROL UNIT IS INSTALLED AFT OF THE FLIGHT COMPARTMENT. |  |
| AGAIN (adv) | One more occurrence | MOVE THE CONTROL STICK BACK TO THE CENTER, AND THEN MOVE IT FORWARD AGAIN. |  |
| AGAINST (prep) | In contact with | PUT THE ADAPTER IN POSITION AGAINST ITS SUPPORT. |  |
| AGENT (n) | One of a group of materials made to do a specified task | DO NOT USE THESE CLEANING AGENTS ON HOT SURFACES. |  |
| aggravate (v) — UNNAPPROVED | INCREASE (v) | TIRE WEAR INCREASES WITH HIGH SPEED. | Tire wear is aggravated by high speed. |
| agitate (v) — UNNAPPROVED | SHAKE (v) | SHAKE THE SOLUTION. | Agitate the solution. |
| agitation (n) — UNNAPPROVED | SHAKE (v) | IF YOU SHAKE THE SOLUTION, DO NOT USE IT FOR ONE HOUR. | After agitation, do not use the solution for one hour. |

<!-- Page 151 of 434 -->

|---|---|---|---|
| AGREE (v), AGREES, AGREED, AGREED | To be consistent with | THE INDICATIONS MUST AGREE WITH THE VALUES IN TABLE 1001. |  |
| ahead (adv) — UNNAPPROVED | FORWARD (adv) | WHEN YOU INSTALL THE ANTENNA, THE ALIGNMENT ARROW MUST POINT FORWARD. | When you install the antenna, the alignment arrow must point ahead. |
| AID (n) | Help that is given | IF YOU GET THIS CHEMICAL SOLUTION INTO YOUR EYES, GET MEDICAL AID IMMEDIATELY. |  |
| aid (v) — UNNAPPROVED | HELP (v) | APPLY SAND TO THE PLANKS TO HELP WITH TIRE TRACTION. | Apply sand to the planks to aid tire traction. |
| aim (v) — UNNAPPROVED | POINT (v) | DO NOT POINT THE HOSE AT PERSONS. | Do not aim the hose at persons. |
| AIRBORNE (adj) | In, or used in, flight | POSITION 2 OF THE SWITCH GIVES A SIGNAL OF THE AIRCRAFT AIRBORNE CONDITION. |  |
| air-dry (v) — UNNAPPROVED | DRY (v) | DRY THE FILTER IN THE AIR. | Air-dry the filter. |
| AIRFLOW (n) | A flow of air | MAKE SURE THAT THE AIRFLOW IS NOT MORE THAN 10 LITERS/MINUTE. |  |
| alert (v) — UNNAPPROVED | TELL (v) | TELL ALL PERSONS TO GO AWAY FROM THE AREA. | Alert all persons to go away from the area. |
| ALIGN (v), ALIGNS, ALIGNED, ALIGNED | To put or come into a specified position in relation to a line | ALIGN THE FLANGE HOLES WITH THE STUDS. |  |
| ALIGN (v), ALIGNS, ALIGNED, ALIGNED |  | ALL THREE BRACKET HOLES MUST ALIGN WITH THE FUEL TUBE. |  |

<!-- Page 152 of 434 -->

|---|---|---|---|
| alignment (n) — UNNAPPROVED | ALIGN (v) | MAKE SURE THAT THE KEYWAY IS AT THE TOP AND ALIGNS WITH THE PEG. | Ensure that the keyway is at the top and in alignment with the peg. |
| ALL (adj) | Full quantity | DRAIN ALL THE FLUIDS. |  |
| allocate (v) — UNNAPPROVED | GIVE (v) | GIVE THE DIFFERENT MAINTENANCE TASKS TO THE APPROVED TECHNICIANS. | Allocate the different maintenance tasks to the approved technicians. |
| allow (v) — UNNAPPROVED | LET (v) | DO NOT LET THE CABLE TOUCH THE FLOOR. | Do not allow the cable to touch the floor. |
| allowable (adj) — UNNAPPROVED | PERMITTED (adj) | THE MAXIMUM PERMITTED DIFFERENCE IS 5 mm. | The maximum allowable difference is 5 mm. |
| allowable (adj) — UNNAPPROVED | APPROVED (adj) | THE VALUES MUST NOT BE MORE THAN THE APPROVED DIFFERENCES GIVEN IN TABLE 1. | The values must not be more than the allowable differences given in table 1. |
| ALMOST (adv) | Near the limit or the value | MAKE SURE THAT THE PRESSURE IN THE CABIN IS ALMOST ZERO. |  |
| ALONG (prep) | In a line parallel with the length or direction of | MOVE THE TENSIOMETER ALONG THE CABLE. |  |
| already (adv) — UNNAPPROVED | IN PROGRESS (adv) | THE DATABASE SYNCHRONIZATION IS IN PROGRESS. | The database is already synchronizing. |
| already (adv) — UNNAPPROVED | NO OTHER | YOU CAN DO THIS REPAIR PROCEDURE ONLY IF THERE IS NO OTHER DAMAGE. | Only do this repair procedure if there is not already damage. |
| already (adv) — UNNAPPROVED | Frequently, an alternative for this word is not necessary. | MAKE SURE THAT THE SOFTWARE IS INSTALLED IN THE REPOSITORY. | Make sure that the software is already installed in the repository. |
| ALSO (adv) | In addition | ALSO DO THE APPLICABLE STEPS OF THIS PROCEDURE. |  |

<!-- Page 153 of 434 -->

|---|---|---|---|
| alter (v) — UNNAPPROVED | CHANGE (v) | IT IS POSSIBLE THAT THE INSTALLATION OF THE CONNECTOR PINS CHANGED THE ROUTING OF THE CABLE LOOM. | It is possible that the installation of the connector pins altered the routing of the cable loom. |
| alteration (n) — UNNAPPROVED | CHANGE (v) | IF YOU CHANGE THIS REPAIR PROCEDURE, GET APPROVAL OF THE DESIGN AUTHORITY. | The alteration to this repair procedure must get approval of the Design Authority. |
| alternate (adj) — UNNAPPROVED | ALTERNATIVE (adj) | AN ALTERNATIVE REPAIR IS AVAILABLE. | An alternate repair is available. |
|  | EACH SECOND | EACH SECOND SQUARE IS RED. | Alternate squares are red. |
| alternate (v) — UNNAPPROVED | THEN (adv) | DO THE PILOT'S INSTRUMENT TEST AND THEN THE COPILOT'S TEST. | Alternate between pilot's and copilot's instrument test. |
| alternately (adv) — UNNAPPROVED | IN ONE (TN) … AND THEN THE OTHER | TO MAKE PIN REMOVAL EASIER, MANUALLY TURN THE CANOPY IN ONE DIRECTION AND THEN IN THE OTHER. | To make pin removal easier, manually turn the canopy alternately in the two directions. |
| ALTERNATIVE (adj) | That gives a choice | YOU CAN USE ALTERNATIVE MATERIALS. |  |
| ALTERNATIVE (n) | One of two or more objects or processes that have the same or almost the same properties or functions | A BIO-BASED FUEL CAN BE AN ALTERNATIVE TO FUELS JET-A1 AND JET-A. |  |
| alternatively (adv) — UNNAPPROVED | ALTERNATIVE (n) | YOU CAN DO TEST B AS AN ALTERNATIVE. | Alternatively, you can do test B. |
| ALTHOUGH (conj) | In spite of the fact that | ALTHOUGH THE PRESSURE DECREASES, THE VALVE MUST STAY CLOSED. |  |
| ALWAYS (adv) | At all times | ALWAYS KEEP THE BRIGHTNESS CONTROL ON THE LCD DISPLAY AT MAXIMUM. |  |

<!-- Page 154 of 434 -->

|---|---|---|---|
| amend (v) — UNNAPPROVED | CHANGE (v) | IF IT IS NECESSARY TO CHANGE THE REPAIR SCHEME, GET THE APPROVAL OF THE DESIGN AUTHORITY. | If it is necessary to amend the Repair Scheme, get the approval of the Design Authority. |
| amendment (n) — UNNAPPROVED | CHANGE (n) | THE DESIGN AUTHORITY MUST GIVE APPROVAL TO THE CHANGES THAT YOU MAKE TO THE REPAIR SCHEME. | The Design Authority must approve the amendments that you make to the Repair Scheme. |
|  | CHANGE (v) | IF IT IS NECESSARY TO CHANGE THE REPAIR SCHEME, GET THE APPROVAL OF THE DESIGN AUTHORITY. | If an amendment to the Repair Scheme is necessary, get the approval of the Design Authority. |
| among (prep) — UNNAPPROVED | IN (prep) | IF THERE ARE METAL PARTICLES IN THE SAMPLES, REPLACE THE PUMP. | If there are metal particles among the samples, replace the pump. |
| amount (n) — UNNAPPROVED | QUANTITY (n) | MAKE SURE THAT THE QUANTITY OF FUEL IN THE TANK IS NOT MORE THAN 500 LITERS. | Make sure that the amount of fuel in the tank is not more than 500 liters. |
| AN (art) | Function word: indefinite article | MAKE AN ENTRY IN THE LOGBOOK. |  |
| ANALOG (adj) | Of data given by pointers and dials | THE PRE-MOD UNIT HAS ANALOG INDICATORS. |  |
| analyze (v) — UNNAPPROVED | ANALYSIS (TN) | MAKE AN ANALYSIS OF THE OIL. | Analyze the oil sample. |
| anchor (v) — UNNAPPROVED | ATTACH (v) | THE STRAPS ARE ATTACHED TO A FULL-LENGTH RAIL. | The straps are anchored to a full-length rail. |

<!-- Page 155 of 434 -->

|---|---|---|---|
| ancillary (adj) — UNNAPPROVED | AUXILIARY (adj) | THE ENGINE AND ALL AUXILIARY EQUIPMENT USE THE SAME LUBRICANT. | The engine and all ancillary equipment use the same lubricant. |
|  | SECONDARY (adj) | DO AN OPERATIONAL CHECK OF THE SECONDARY CONTROLS. | Do an operational check of the ancillary controls. |
| AND (conj) | Function word used to connect words, phrases, or clauses | MAKE SURE THAT THE FLAPS ARE RETRACTED AND THE AILERON TRIM HANDWHEEL IS IN THE ZERO POSITION. |  |
| ANGULAR (adj) | That has one or more angles | MAKE SURE THAT THE ANGULAR POSITION IS CORRECT. |  |
| annotation (n) — UNNAPPROVED | WRITE (v) | WRITE THE TEMPERATURE VALUE ON THE ENGINE LOG CARD. | Make an annotation of the temperature on the Engine Log Card. |
|  | RECORD (v) | RECORD THE TEMPERATURE VALUE ON THE ENGINE LOG CARD. | Make an annotation of the temperature on the Engine Log Card. |
| annunciate (v) — UNNAPPROVED | SHOW (v) | THE DISPLAY SHOWS A FAULT MESSAGE. | The display annunciates a fault message. |
| another (adj) — UNNAPPROVED | ONE (TN) MORE | INSTALL ONE MORE WASHER BETWEEN THE NUT AND THE SURFACE. | Install another washer between the nut and the surface. |
|  | DIFFERENT (adj) | REFER TO DETAIL C ON FIG. 4 FOR A DIFFERENT PROCEDURE TO ATTACH THE CABLE. | Refer to detail C on Fig. 4 for another way of attaching the cable. |
|  | AGAIN (adv) | BEFORE YOU TRY TO START THE ENGINE AGAIN, MAKE SURE THAT THE AREA IS SAFE. | Before you try another engine start, make sure that the area is safe. |
| anticlockwise (adv) | COUNTERCLOCKWISE (adv) | COUNTERCLOCKWISE. | Turn the cap anticlockwise. |

<!-- Page 156 of 434 -->

|---|---|---|---|
| any (adj) — UNNAPPROVED | Frequently, an alternative for this word is not necessary. | IF YOU HAVE QUESTIONS ABOUT THIS DOCUMENT, SEND AN E-MAIL TO THE ADDRESS THAT FOLLOWS: | If you have any questions about this document, send an e-mail to the address that follows: |
| any (pron) — UNNAPPROVED | ONE (TN) | REMOVE ONE OF THE FOUR BOLTS. | Remove any of the four bolts. |
| anytime (adv) — UNNAPPROVED | WHEN (conj) | WHEN YOU USE THE EMERGENCY PUMP, RECORD THE TIME OF OPERATION. | Anytime you use the emergency pump, record the time of operation. |
| APART (adv) | At a distance (not specified) from | MOVE THE CABLE STRANDS APART. |  |
| aperture (n) — UNNAPPROVED | OPENING (n) | GET ACCESS TO THE CONTROL UNIT THROUGH THE OPENING IN THE SIDE OF THE TANK. | Get access to the control unit through the aperture in the side of the tank. |
| apparent (adj) — UNNAPPROVED | SEE (v) | IF YOU SEE DISCOLORATION, REPLACE THE PART. | If discoloration is apparent, replace the part. |
|  | FIND (v) | IF YOU FIND A CRACK, DO THE APPLICABLE REPAIR PROCEDURE. | If a crack is apparent, do the applicable repair procedure. |
| appear (v) — UNNAPPROVED | SHOW (v) | A WARNING FLAG SHOWS IN THE WINDOW. | A warning flag appears in the window. |
| (v) | THINK (v) | IF YOU THINK THAT THE ENGINE IS TOO HOT, TURN THE SWITCH TO "OFF." | If the engine appears to be too hot, turn the switch to off. |
|  | POSSIBLE (adj) | IF IT IS POSSIBLE THAT THE TEMPERATURE VALUES ARE INCORRECT, DECREASE THE POWER. | If it appears that the temperature values are incorrect, decrease the power. |

<!-- Page 157 of 434 -->

|---|---|---|---|
| APPLICABLE (adj) | Correct or satisfactory for the task | REFER TO THE TABLE THAT FOLLOWS FOR THE APPLICABLE TORQUE VALUES. |  |
| application (n) — UNNAPPROVED | APPLY (v) | APPLY THE SEALANT WITH A WOODEN SPATULA. | The application of sealant must be carried out with a wooden spatula. |
| APPLY (v), APPLIES, APPLIED, APPLIED | 1. To put or spread something on | APPLY THE SEALING COMPOUND. |  |
| APPLY (v), APPLIES, APPLIED, APPLIED | 2. To use something (for example, pressure, force, load) to cause an effect | APPLY A FORCE OF 100 N ON THE END OF THE LEVER. |  |
| appoint (v) — UNNAPPROVED | TELL (v) | TELL TWO PERSONS TO BE PREPARED TO OPERATE THE FIRE EXTINGUISHERS. | Appoint two persons to be prepared to operate the fire extinguishers. |
| approach (v) — UNNAPPROVED | GO NEAR | IF IT IS NECESSARY TO GO NEAR THE ENGINE EXHAUST, USE EAR PROTECTION. | If it is necessary to approach the engine exhaust, use ear protection. |
| appropriate (adj) — UNNAPPROVED | APPLICABLE (adj) | LOCK THE WASHER WITH THE APPLICABLE TABS. | Lock the washer with the appropriate tabs. |
| APPROVAL (n) | That which permits a person or a thing to do something | BEFORE YOU REPAIR THIS UNIT, GET THE APPROVAL OF THE MANUFACTURER. |  |
| approve (v) — UNNAPPROVED | APPROVAL (n) | APPROVAL FROM THE DESIGN AUTHORITY IS MANDATORY FOR ALL MODIFICATIONS. | All modifications must be approved by the Design Authority. |
| APPROVED (adj) | Permitted by an authority | DO THE PROCEDURE IN AN APPROVED AREA. |  |
| APPROXIMATE (adj) | Almost correct or accurate | AN APPROXIMATE VALUE IS SATISFACTORY. |  |

<!-- Page 158 of 434 -->

|---|---|---|---|
| APPROXIMATELY (adv) | Almost correct or accurate | DRAIN APPROXIMATELY 2 LITERS OF FUEL. |  |
| AREA (n) | A specified surface or location | DO NOT SMOKE IN THE WORK AREA. |  |
| arise (v) — UNNAPPROVED | OCCUR (v) | SHOCK LOADING OF THE ENGINE CAN OCCUR DURING A HEAVY LANDING. | Shock loading of the engine can arise from a heavy landing. |
| arise (v) — UNNAPPROVED | CAUSE (v) | A HEAVY LANDING CAN CAUSE SHOCK LOADING OF THE ENGINE. | Shock loading of the engine can arise from a heavy landing. |
| ARM (v), ARMS, ARMED, ARMED | 1. To install armaments | ARM THE AIRCRAFT. |  |
| ARM (v), ARMS, ARMED, ARMED | 2. To prepare for automatic operation | SET THE SWITCH TO "CLOSE" TO ARM THE CIRCUIT. |  |
| AROUND (prep) | On all sides of For other meanings, use: | PUT THE STRAP CLAMPS AROUND THE CYLINDER. |  |
| AROUND (prep) | APPROXIMATELY (adv) | THE TEST BENCH IS APPROXIMATELY 10 FEET FROM THE DOOR. | The test bench is around 10 feet from the door. |
| arrange (v) — UNNAPPROVED | PUT (v) | PUT THE COMPONENTS IN THIS SEQUENCE: | Arrange the components in this order. |
| arrangement (n) — UNNAPPROVED | CONFIGURATION (TN) | THE CONFIGURATION OF THE INSERTS IS RELATED TO THE DIMENSIONS OF THE CONNECTOR SHELL. | The arrangement of the inserts is related to the dimensions of the connector shell. |
| arrangement (n) — UNNAPPROVED | PREPARE (v) | PREPARE FOR THE LEAK TEST. | Make the arrangements for the leak test. |
| arrest (v) — UNNAPPROVED | STOP (v) | STOP THE FLOW FOR 10 SECONDS. | Arrest the flow for 10 seconds. |
| arrest (v) — UNNAPPROVED | HOLD (v) | A COTTER PIN HOLDS THE ATTACHMENT BAR. | A cotter pin arrests the attachment bar. |

<!-- Page 159 of 434 -->

|---|---|---|---|
| arrive (v) — UNNAPPROVED | GET (v) | TO GET THE CORRECT VALUE, SET THE SWITCH TO POSITION 2. | To arrive at the correct value, set the switch to position 2. |
| ARROW (n) | A mark that has a point to show direction | MAKE SURE THAT THE ARROW POINTS IN THE DIRECTION OF THE FUEL FLOW. |  |
| article (n) — UNNAPPROVED | OBJECT (n) | MAKE SURE THAT THERE ARE NO LOOSE OBJECTS IN THE ENGINE AIR INTAKES. | Ensure that there are no loose articles in the engine air intakes. |
| AS (prep) | In the manner of, to the same quantity, equally | DO NOT USE THE CYLINDER AS A SUPPORT. |  |
| as (conj) — UNNAPPROVED | BECAUSE (conj) | THE PUMP DID NOT OPERATE BECAUSE THE SHAFT WAS BROKEN. | The pump did not operate as the shaft was broken. |
| as (conj) — UNNAPPROVED | WHILE (conj) You can use: | WHILE YOU DO EACH STEP OF THE VALVE TEST, MAKE SURE THAT THERE IS NO LEAKAGE. | As you do each step of the valve test, make sure that there is no leakage. |
| as (conj) — UNNAPPROVED | AS FOLLOWS | ASSEMBLE THE VALVE AS FOLLOWS: |  |
| as (conj) — UNNAPPROVED | AS NECESSARY | SET THE LENGTH OF THE CONTROL ROD AS NECESSARY. |  |
| as (conj) — UNNAPPROVED | AS SHOWN | MEASURE THE DEPTH OF THE DENT AS SHOWN IN FIGURE 4. |  |
| AS ... AS (conj) | Construction used to show comparison or relation | MOVE THE LEVER AS FAST AS POSSIBLE. |  |
| AS ... AS (conj) | For "as long as," refer to "long (as long as)." |  |  |
| ascertain (v) — UNNAPPROVED | MAKE SURE (v) | MAKE SURE THAT THE LIGHT IS OFF. | Ascertain that the light is off. |

<!-- Page 160 of 434 -->

|---|---|---|---|
| ask (v) — UNNAPPROVED | TELL (v) | TELL THE DRIVER TO SET THE SWITCH TO OFF. | Ask the driver to set the switch to off. |
| ask (v) — UNNAPPROVED | SPEAK (v) | SPEAK TO THE LOCAL AIR TRAFFIC CONTROLLER. | Ask the local air traffic controller. |
| ASSEMBLE (v), ASSEMBLES, ASSEMBLED, ASSEMBLED | To attach, connect, or put together the parts of something | ASSEMBLE THE VALVE AS FOLLOWS: |  |
| ASSEMBLY (n) | Items that are connected for a specified function | REMOVE THE WHEEL BRAKE ASSEMBLY FROM THE AXLE. |  |
| assess (v) — UNNAPPROVED | CALCULATE (v) | CALCULATE THE QUANTITY OF FUEL THAT IS NECESSARY. | Assess the quantity of fuel that is necessary. |
| assess (v) — UNNAPPROVED | ESTIMATE (n) | MAKE AN ESTIMATE OF THE DAMAGE. | Assess the damage. |
| assessment (n) — UNNAPPROVED | ESTIMATE (n) | MAKE AN ESTIMATE OF THE DAMAGE. | Carry out an assessment of the damage. |
| assessment (n) — UNNAPPROVED | CALCULATE (v) | CALCULATE THE NUMBER OF SHIMS THAT ARE NECESSARY. | Do an assessment of the number of shims that are necessary. |
| assign (v) — UNNAPPROVED | GIVE (v) | GIVE A CODE TO EACH CONNECTOR. | Assign a code to each connector. |
| assist (v) — UNNAPPROVED | HELP (v) | KEEP THE DATA TO HELP YOU WITH SUBSEQUENT PROCEDURES. | Keep the data to assist subsequent procedures. |
| assistance (n) — UNNAPPROVED | AID (n) | FOR THIS STEP, MAKE SURE THAT YOU HAVE THE AID OF ONE MORE PERSON. | For this step, you must have the assistance of one more person. |
| assistance (n) — UNNAPPROVED | HELP (v) | FOR THIS STEP, MAKE SURE THAT ONE PERSON HELPS YOU. | For this step, you must have the assistance of one person. |

<!-- Page 161 of 434 -->

|---|---|---|---|
| associated (adj) — UNNAPPROVED | CORRECT (adj) | INSTALL THE DUMP VALVE AND THE CORRECT GASKET. | Install the dump valve with the associated gasket. |
|  | RELATED (adj) | REMOVE THE RELATED DOORS. | Remove the panels from the associated doors. |
|  | ITS (adj) | REMOVE THE BOLT AND ITS WASHER. | Remove the bolt and the associated washer. |
|  | THEIR (adj) | REMOVE THE EIGHT BOLTS AND THEIR WADGERS. | Remove the eight bolts and the associated washers. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |
| assume (v) — UNNAPPROVED | THINK (v) | IF YOU THINK THAT YOU CAN REPAIR THE DAMAGE, REFER TO THE REPAIR SECTION. | If damage is assumed to be repairable, refer to the repair section. |

<!-- Page 162 of 434 -->

|---|---|---|---|
| ATTACH (v), ATTACHES, ATTACHED, ATTACHED | To stay together or to cause different items to stay together | MAKE SURE THAT THE LABEL FULLY ATTACHES TO THE SURFACE AND THAT THERE ARE NO BUBBLES. |  |
| ATTACH (v), ATTACHES, ATTACHED, ATTACHED |  | TEMPORARILY ATTACH THE CABLE TO THE ADJACENT STRUCTURE. |  |
| attachment (n) — UNNAPPROVED | ATTACH (v) | MAKE SURE THAT THE DUCT IS CORRECTLY ATTACHED TO THE FILTER. | Make sure that the attachment of the duct to the filter is correct. |
| attain (v) — UNNAPPROVED | SHOW (v) | WHEN THE VOLTMETER SHOWS 28 VOLTS DC, THE RELAY CLOSES. | When 28 volts DC is attained, the relay closes. |
|  | BE (v) | WHEN THE VOLTAGE IS 28 VOLTS DC, THE RELAY CLOSES. | When 28 volts DC is attained, the relay closes. |
|  | GET (v) | WHEN YOU GET 28 VOLTS DC, THE RELAY CLOSES. | When 28 volts DC is attained, the relay closes. |
| attempt (n) — UNNAPPROVED | TRY (v) | TRY TO LIFT THE COVER MANUALLY. | Make an attempt to lift the cover manually. |
| attempt (v) — UNNAPPROVED | TRY (v) | TRY TO FIND THE DEFECT. | Attempt to find the defect. |
| attention (n) — UNNAPPROVED | AID (n) | IF YOU GET PAINT SPRAY IN YOUR EYES, GET MEDICAL AID. | If you get paint spray in your eyes, get medical attention. |
|  | CAREFUL (adj) | BE CAREFUL WHEN YOU REMOVE THE CONTROL UNIT. | Pay attention when you remove the control unit. |
|  | MONITOR (v) | MONITOR THE RESULTS. | Pay attention to the results. |

<!-- Page 163 of 434 -->

|---|---|---|---|
| audible (adj) — UNNAPPROVED | HEAR (v) | IF YOU CANNOT HEAR THE ALARM, ADJUST THE VOLUME CONTROL. | If the alarm is not audible, adjust the volume control. |
|  | LISTEN (v) | LISTEN FOR AIR LEAKAGE FROM THE LINES. | Check the lines for audible air leakage. |
| augment (v) — UNNAPPROVED | INCREASE (v) | A MIXTURE OF WATER AND METHANOL INCREASES THE POWER OF THE ENGINE. | A mixture of water and methanol augments the power of the engine. |
| aurally (adv) — UNNAPPROVED | LISTEN (v) | LISTEN TO MAKE SURE THAT THE FLUID FLOWS. | Check aurally to ensure fluid flow. |
|  | HEAR (v) | YOU CAN HEAR THE WARNING IN THE COCKPIT. | The warning is given aurally in the cockpit. |
| authentic (adj) — UNNAPPROVED | ACCURATE (adj) | IF THE ADJUSTMENT OF THE STOPS IS NOT CORRECT, THE RESULTS OF THE TEST WILL NOT BE ACCURATE. | If the adjustment of the stops is not correct, the results of the test will not be authentic. |
| AUTHORITY (n) | An official organization that gives approval to something | BEFORE YOU CHANGE THE PROCEDURE, GET THE APPROVAL OF THE DESIGN AUTHORITY. |  |
| authorized (adj) — UNNAPPROVED | APPROVED (adj) | ONLY APPROVED PERSONS ARE PERMITTED TO STAY IN THIS AREA. | Only authorized persons are permitted to stay in this area. |
| AUTOMATIC (adj) | That operates without other input | THE AUTOMATIC SYSTEM WILL OPEN THE DOORS. |  |
| AUTOMATICALLY (adv) | That operates without other input | THE FUEL FLOW STOPS AUTOMATICALLY. |  |

<!-- Page 164 of 434 -->

|---|---|---|---|
| AUXILIARY (adj) | 1. That operates in a secondary function | LUBRICANTS FOR THE ENGINE AND THE AUXILIARY EQUIPMENT ARE THE SAME. |  |
| AUXILIARY (adj) | 2. That gives help | USE AUXILIARY SCREWS TO ASSEMBLE THE UNIT TEMPORARILY. |  |
| AVAILABLE (adj) | Prepared or supplied for you to use | IF ELECTRICAL POWER IS AVAILABLE, DO A CONTINUITY CHECK. |  |
| avert (v) — UNNAPPROVED | PREVENT (v) | IF THE MICROSWITCH BECOMES UNSERVICEABLE, DEACTIVATE THE ACTUATOR TO PREVENT DAMAGE TO THE VALVE. | If the microswitch becomes unserviceable, deactivate the actuator to avert damage to the valve. |
| avoid (v) — UNNAPPROVED | PREVENT (v) | TURN THE CONTROLS SLOWLY TO PREVENT DAMAGE. | Turn the controls slowly to avoid damage. |
|  | DO NOT | DO NOT PUSH ON THE SEALS. | Avoid pushing on the seals. |
| aware (adj) — UNNAPPROVED | KNOW (v) | ALL PERSONNEL MUST KNOW THE HEALTH RISKS. | All personnel must be aware of the health risks. |
|  | TELL (v) | TELL ALL PERSONNEL ABOUT THE NEW RULES. | All personnel must be aware of the new rules. |
| AWAY FROM (prep) | In or to a different position or direction | DO THE WORK IN AN AREA AWAY FROM EQUIPMENT OR METAL FRAME BUILDINGS. |  |
| AXIAL (adj) | Related to an axis | DO STEPS 1 THRU 4 TO MAKE SURE THAT NO AXIAL LOAD IS ON THE ROD. |  |
| AXIALLY (adv) | Related to an axis | APPLY THE LOAD AXIALLY. |  |

<!-- Page 165 of 434 -->

|---|---|---|---|
| back (adj) — UNNAPPROVED | REAR (adj) | DISCONNECT THE CABLE FROM THE REAR SIDE OF THE INSTRUMENT. | Disconnect the cable from the back side of the instrument. |
| BACK (adv) | To an initial condition | MOVE THE ENGINE THROTTLE BACK TO 60% RPM. |  |
| back (n) — UNNAPPROVED | REAR (n) | THE CONTROL UNIT IS AT THE REAR. | The control unit is at the back. |
| back and forth (adv) | DIRECTION (n) | MOVE THE SLEEVE IN THE PISTON TO ONE DIRECTION AND THEN BACK AGAIN. | Move the sleeve back and forth in the piston. |
| back off (v) — UNNAPPROVED | LOOSEN (v) | DO NOT LOOSEN THE NUT TO ALIGN IT. | Do not back off the nut to obtain alignment. |
| backup (n) — UNNAPPROVED | EMERGENCY (n) | IN AN EMERGENCY, THE ONE-SHOT BATTERY SUPPLIES DC POWER. | The one-shot battery is a backup for the DC electrical supply. |
| backup (n) — UNNAPPROVED | AUXILIARY (adj) | USE AUXILIARY SCREWS TO ASSEMBLE THE UNIT TEMPORARILY. | Use some screws as a backup to assemble the unit temporarily. |
| backward (adv) — UNNAPPROVED | REARWARD (adv) | MOVE THE LEVER REARWARD. | Move the lever backward. |
| BAD (adj) (WORSE, WORST) | Not satisfactory. Do not use this word if more accurate and clear words are available. | REFER TO CHAPTER 6 FOR INSTRUCTIONS ABOUT HOW TO PARK IN BAD WEATHER CONDITIONS. |  |
| BAD (adj) (WORSE, WORST) |  | IF THE LENGTH OF THE CRACK IS MORE THAN THE PERMITTED LIMIT, REPLACE THE PART. | If the crack is bad, replace the part. |

<!-- Page 166 of 434 -->

|---|---|---|---|
| badly (adv) — UNNAPPROVED | INCORRECTLY (adv) | IF THE SLEEVE IS INCORRECTLY ATTACHED, ADJUST IT. | If the sleeve is badly attached, adjust it. |
| badly (adv) — UNNAPPROVED | UNSATISFACTORILY (adv) | DISCARD ALL SEALS WHICH ARE UNSATISFACTORILY BONDED. | Discard all seals which are badly bonded. |
| badly (adv) — UNNAPPROVED | DECREASE (v) | FUEL LEAKS CAN DECREASE ENGINE PERFORMANCE. | A fuel leak can cause the engine to operate badly. |
| BALANCE (v), BALANCES, BALANCED, BALANCED | To make equal | BALANCE THE ELECTRICAL LOADS ON EACH GENERATOR. |  |
| bank (v) — UNNAPPROVED | BANK (TN) | THE V-BARS GIVE THE INDICATION FOR A BANK. | The V-bars indicate the command to bank. |
| BARE (adj) | Without a surface layer or protection | BARE METAL SURFACES ARE USUALLY SATISFACTORY FOR AN ELECTRICAL BOND. |  |
| bared (adj) — UNNAPPROVED | BARE (adj) | GIVE TEMPORARY PROTECTION TO AREAS OF BARE METAL. | Give temporary protection to areas of bared metal. |
| base (n) — UNNAPPROVED | BOTTOM (n) | MAKE SURE THAT THE TWO SPIGOTS AT THE BOTTOM OF THE UNIT ENGAGE. | Make sure that the two spigots at the base of the unit engage. |
| base (v) — UNNAPPROVED | USE (v) | USE THE TORQUE VALUES GIVEN IN CHAPTER 10. | Base the torque values on those given in Chapter 10. |
| BASIC (adj) | Approved minimum | THIS MODIFICATION CHANGES THE BASIC CONFIGURATION OF THE SYSTEM. |  |

<!-- Page 167 of 434 -->

|---|---|---|---|
| BE (v), IS, WAS, (also ARE, WERE) No other verb forms. | 1. To occur, exist | IF THERE IS CORROSION ON THE PUMP VANES, REPLACE THE PUMP. |  |
| BE (v), IS, WAS, (also ARE, WERE) No other verb forms. | 2. To have a property, to be equal to | ACID SOLUTIONS ARE DANGEROUS. |  |
| BECAUSE (conj) | As a result of | BECAUSE THE FLUID LEVEL IS INCORRECT, THE SYSTEM WILL NOT OPERATE. |  |
| BECAUSE OF (prep) | As a result of | IF YOU CANNOT REMOVE A BOLT BECAUSE OF CORROSION, APPLY PENETRATING OIL. |  |
| BECOME (v), BECOMES, BECAME No other verb forms. | To come to be | THE SCREEN BECOMES AVAILABLE. |  |
| BEFORE (conj) | That precedes a specified time, sequence, or operation | BEFORE YOU DISCONNECT THE COMPONENTS, BLEED THE SYSTEM. |  |
| BEFORE (prep) | That precedes a specified time, sequence, or operation | THE BAR MOVES DOWN BEFORE 20 SECONDS. |  |
| begin (v) — UNNAPPROVED | START (v) | INCREASE THE PRESSURE UNTIL THE FLOW STARTS AGAIN. | Increase pressure until the flow begins again. |

<!-- Page 168 of 434 -->

|---|---|---|---|
| beginning (n) — UNNAPPROVED | START (n) | YOU CAN GET SLOW MOVEMENT AT THE START. | You can get slow movement at the beginning. |
| beginning (n) — UNNAPPROVED | SOURCE (n) | FIND THE SOURCE OF THE FUEL LEAKAGE. | Find the beginning of the fuel leak. |
| beginning (n) — UNNAPPROVED | START (v) | WHEN THE LEVER STARTS TO MOVE, THE MICROSWITCH OPERATES. | At the beginning of the lever movement, the microswitch will operate. |
| BEHIND (prep) | In a position at the rear of | THE PUMP IS INSTALLED BEHIND THE HYDRAULIC MOTOR. |  |
| below (adv) — UNNAPPROVED | FOLLOW (v) | OBEY THE SAFETY PRECAUTIONS THAT FOLLOW: | Obey the safety precautions below: |
| below (adv) — UNNAPPROVED | THESE (adj) | OBEY THESE SAFETY PRECAUTIONS: | Obey the safety precautions below: |
| BELOW (prep) | In (or to) a position farther down than something | THE DATE IS WRITTEN BELOW THE CYLINDER NECK. |  |
| BELOW (prep) | For other meanings, use LESS THAN | MAKE SURE THAT THE DIAMETER OF THE HOLE IS LESS THAN THE SPECIFIED VALUE. | Make sure that the diameter of the hole is below the specified value. |
| BEND (n) | The area where something is bent | EXAMINE THE BENDS FOR CRACKS. |  |
| BEND (v), BENDS, BENT, BENT | To change or cause to change from straight to curved | BEND THE PIPE CAREFULLY. |  |
| BEND (v), BENDS, BENT, BENT |  | THESE PARTS CAN EASILY BEND, BREAK OR BECOME INCORRECTLY ALIGNED. |  |
| beneath (prep) — UNNAPPROVED | BELOW (prep) | PUT THE JACK BELOW THE AXLE. | Put the jack beneath the axle. |

<!-- Page 169 of 434 -->

|---|---|---|---|
| beside (prep) — UNNAPPROVED | ADJACENT TO | THE FUEL PUMP IS ADJACENT TO THE STRUCTURAL SUPPORT. | The fuel pump is beside the structural support. |
| BETWEEN (prep) | Related to something before and after in time or position | MAKE SURE THAT THE STOPWATCH INDICATION IS BETWEEN 2 AND 4 MINUTES. |  |
| beware (v) — UNNAPPROVED | CAREFUL (adj) | BE CAREFUL OF DANGEROUS VOLTAGES. | Beware of dangerous voltages. |
| beyond (prep) — UNNAPPROVED | MORE THAN | REPLACE ALL COMPONENTS THAT ARE WORN MORE THAN THE MAXIMUM LIMITS. | Replace all components that are worn beyond their maximum limits. |
| big (adj) — UNNAPPROVED | LARGE (adj) If it is possible, give an accurate value. | INSTALL THE LARGER BOLTS. | Install the bigger bolts. |
| bind (v) — UNNAPPROVED | FREELY (adv) | MAKE SURE THAT THE VALVES MOVE FREELY. | Check that valves do not bind. |
| bind (v) — UNNAPPROVED | WIND AROUND | WIND TWO LAYERS OF TAPE AROUND THE PIPE JOINTS. | Bind the pipe joints with two layers of tape. |
| blank (v) — UNNAPPROVED | SEAL (v) | SEAL THE HOSE. | Blank the hose. |
| blank (v) — UNNAPPROVED | CAP (TN) | PUT A CAP ON THE CONNECTOR. | Blank the connector. |
| blank (v) — UNNAPPROVED | COVER (TN) | PUT A COVER ON THE OUTLET PORT. | Blank the outlet port. |
| BLEED (v), BLEEDS, BLED, BLED | To let a gas out of | BLEED THE SPEEDBRAKE HYDRAULIC SYSTEM. |  |
| blend (v) — UNNAPPROVED | MIX (v) | MIX THE ADHESIVE WITH THE HARDENER. | Blend the adhesive with the hardener. |

<!-- Page 170 of 434 -->

|---|---|---|---|
| block (v) — UNNAPPROVED | CAUSE A BLOCKAGE | MAKE SURE THAT THE SEALANT DOES NOT CAUSE A BLOCKAGE OF THE DRAIN. | Check that the sealant does not block the drain. |
| BLOCKAGE (n) | That which prevents correct operation | MAKE SURE THAT THERE IS NO BLOCKAGE OF THE PIPE. |  |
| BLOCKED (adj) | That prevents correct operation | A BLOCKED OIL JET CAN CAUSE INCORRECT OPERATION. |  |
| blot (v) — UNNAPPROVED | DRY (v) | DRY THE SURFACE WITH A TOWEL. | Blot the surface with a towel. |
| BLOW (v), BLOWS, BLEW, BLOWN | To cause gas to move | BLOW DRY AIR THROUGH THE FEED TUBES. |  |
| BLUNT (adj) | Not sharp | REMOVE THE SEALANT WITH A BLUNT SCRAPER. |  |
| blunted (adj) — UNNAPPROVED | BLUNT (adj) | EXAMINE THE STATIC DISCHARGERS FOR BENT AND BLUNT PINS. | Inspect the static dischargers for bent and blunted pins. |
| bolt (v) — UNNAPPROVED | ATTACH (v) (WITH A BOLT [TN] OR BOLTS [TN]) | ATTACH THE TRACK TO THE CHANNELS WITH THE BOLTS. | Bolt the track to the channels. |
| BOND (n) | 1. A connection between structural components for electrical continuity | DO A RESISTANCE CHECK OF THE PRIMARY BONDS. |  |
| BOND (n) | 2. A firm connection with another material | MAKE SURE THAT THE BOND BETWEEN THE HONEYCOMB CORE AND THE SKIN IS CORRECT. |  |

<!-- Page 171 of 434 -->

|---|---|---|---|
| BOND (v), BONDS, BONDED, BONDED | 1. To make an electrical bond | THE STATIC DISCHARGER IS ELECTRICALLY BONDED TO THE FRAME. |  |
| BOND (v), BONDS, BONDED, BONDED | 2. To attach firmly or become firmly attached with another material | IF THE FILLER BONDS TO THE TOOL, MAKE THE TOOL MOIST WITH COLD WATER. |  |
| BOND (v), BONDS, BONDED, BONDED | 3. | WHEN YOU BOND THE MATERIALS, APPLY A THIRD LAYER OF ADHESIVE. |  |
| both (adj) — UNNAPPROVED | THE TWO (TN) | ATTACH THE TWO ENDS OF THE HOSE. | Attach both ends of the hose. |
| BOTTOM (adj) | That is lowermost | REMOVE THE BOTTOM BOLT. |  |
| BOTTOM (n) | The lowermost position | THE DRAIN PLUG IS AT THE BOTTOM OF THE UNIT. |  |
| bottom (v) — UNNAPPROVED | TOUCH (v) | OPEN THE DOOR UNTIL IT TOUCHES THE FLOOR. | Open the door until it bottoms on the floor. |
| bounds (n) — UNNAPPROVED | LIMIT (n) | MAKE SURE THAT THE CLEARANCE IS IN THE LIMITS. | Make sure that the clearance is in bounds. |
| brace (v) — UNNAPPROVED | HOLD (v) | SUPPORT STRUTS HOLD THE FLOOR STRUCTURE IN POSITION. | Support struts brace the floor structure. |
| brace (v) — UNNAPPROVED | STRONG (adj) | REINFORCEMENT PLATES MAKE THE LAP JOINTS STRONGER. | Reinforcement plates brace the lap joints. |
| branch (v) — UNNAPPROVED | DIVIDE (v) | THE PRESSURE LINES DIVIDE IN DIFFERENT DIRECTIONS. | The pressure lines branch in different directions. |
| breadth (n) — UNNAPPROVED | WIDTH (n) | THE WIDTH OF THE MATERIAL MUST BE LARGER THAN 10 mm. | The breadth of the material must be larger than 10 mm. |

<!-- Page 172 of 434 -->

|---|---|---|---|
| break (n) — UNNAPPROVED | STOP (v) | IF THERE TRANSMISSION STOPS, CANCEL THE TEST. | If there is a break in the transmission, cancel the test. |
| BREAK (v), BREAKS, BROKE, BROKEN | To cause to separate or become separated into parts by force | BREAK THE BOND OF THE SEALANT. |  |
| BREAK (v), BREAKS, BROKE, BROKEN | 3. | IF THE SHEAR PIN BREAKS, DO AN INSPECTION OF THE TOWBAR. |  |
| breakdown (n) — UNNAPPROVED | STOP (v) | IF THE PRESSURE SUPPLY STOPS, CANCEL THE TEST. | If there is a breakdown in the pressure supply, cancel the test. |
| BREATHE (v), BREATHES, BREATHED, BREATHED | To get gas into or out of the lungs | DO NOT BREATHE THE SOLVENT FUMES. |  |
| BREATHE (v), BREATHES, BREATHED, BREATHED | 2. | BREATHE INTO THE OXYGEN MASK. |  |
| BRIGHT (adj) (BRIGHTER, BRIGHTEST) | That gives much light | THE NAVIGATION LIGHTS CHANGE FROM DIM TO BRIGHT. |  |
| BRIGHTLY (adv) | In a bright manner | THE LIGHTS COME ON BRIGHTLY. |  |
| brilliance (n) — UNNAPPROVED | INTENSITY (n) | SET THE INTENSITY TO THE MINIMUM. |  |
| brilliance (n) — UNNAPPROVED | BRIGHT (adj) | TURN THE BRT CONTROL CLOCKWISE TO MAKE THE DISPLAY BRIGHTER. | Turn the BRT CONTROL clockwise to increase the display brilliance. |

<!-- Page 173 of 434 -->

|---|---|---|---|
| bring (v) — UNNAPPROVED | MOVE (v) | MOVE THE PANEL INTO POSITION. | Bring the panel into place. |
| bring (v) — UNNAPPROVED | PUT (v) | PUT THE PANEL IN POSITION. |  |
| briskly (adv) — UNNAPPROVED | QUICKLY (adv) | RUB THE SURFACE QUICKLY WITH A SOFT, DRY CLOTH. | Rub the surface briskly with a soft, dry cloth. |
| broadcast (v) — UNNAPPROVED | TRANSMIT (v) | TRANSMIT THE DATA ON THE TWO CHANNELS. | Broadcast the data on both channels. |
| brush (v) — UNNAPPROVED | BRUSH (TN) | CLEAN THE FILTER ELEMENT WITH A BRUSH. | Brush the filter element to clean it. |
| brush (v) — UNNAPPROVED |  | USE A BRUSH TO CLEAN THE FILTER ELEMENT. |  |
| brush on (v) — UNNAPPROVED | BRUSH (TN) | APPLY THE PAINT WITH A BRUSH. | Brush the paint on. |
| BUBBLE (n) | A small quantity of gas in a liquid or a solid | ADJUST THE CLINOMETER UNTIL THE BUBBLE IS IN THE CENTER. |  |
| build (n) — UNNAPPROVED | STRUCTURE (n) | THE WING STRUCTURE GIVES MAXIMUM FUEL CAPACITY. | The build of the wing allows maximum fuel storage. |
| build (v) — UNNAPPROVED | ASSEMBLE (v) | ASSEMBLE THE UNIT. | Build the unit. |
| bump (v) — UNNAPPROVED | HIT (v) | THE FUELING HOSE MUST NOT HIT THE EDGE OF THE TANK. | The fueling hose must not bump the edge of the tank. |
| BURN (v), BURNS, BURNED, BURNED | 1. To cause or undergo combustion | TURBINE BURNS FUEL. |  |
| BURN (v), BURNS, BURNED, BURNED |  | SEALANT BURNS AT 109 DEG. F. |  |
| BURN (v), BURNS, BURNED, BURNED | 2. To cause injury or damage through heat | HOT SURFACES CAN BURN YOU. |  |

<!-- Page 174 of 434 -->

|---|---|---|---|
| burst (v) — UNNAPPROVED | BREAK (v) | IF THE DISK BREAKS, STOP THE SUPPLY. | If the disk bursts, switch off the supply. |
| BUT (conj) | On the contrary | TIGHTEN THE NUTS, BUT DO NOT TORQUE THEM AT THIS TIME. |  |
| butt (v) — UNNAPPROVED | TOUCH (v) | THE WIRE MUST TOUCH THE REAR OF THE CONTACT. | The wire must butt against the rear of the contact. |
| BY (prep) | Mathematical function word | DIVIDE THE VALUE BY TWO. |  |
| BY (prep) |  | INCREASE THE TEMPERATURE BY 10 DEGREES. |  |
| by means of (prep) — UNNAPPROVED | WITH (prep) | PRESSURIZE THE SYSTEM TO 150 bar WITH THE HAND PUMP. | By means of the hand pump, pressurize the system to 150 bar. |
| BYPASS (v), BYPASSES, BYPASSED, BYPASSED | To change a circuit so that it goes past something instead of through it | IN THIS CONFIGURATION, THE HYDRAULIC PRESSURE BYPASSES THE VALVE. |  |
