# Page 225 of 434

**Page 2-1-E7**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**ENTRY (n)**|A record of an<br>occurrence|MAKE AN ENTRY IN<br>THE LOG CARD.||
|**EQUAL (adj)**|The same dimension,<br>quality, quantity, or<br>number|MAKE SURE THAT<br>THERE IS AN EQUAL<br>DISTANCE BETWEEN<br>THE HOLES.||
|**equal (v) — UNNAPPROVED**|SAME (adj)|DIMENSION "X" MUST<br>BE THE SAME AS<br>DIMENSION "Z."|Dimension X must equal<br>dimension Z.|
|||EQUAL (adj)|DIMENSION "X" MUST<br>BE EQUAL TO<br>DIMENSION "Y."|Dimension X must equal<br>dimension Y.|
|**EQUALLY (adv)**|The same dimension,<br>quality, quantity, or<br>number|ADJUST THE<br>TURNBUCKLES<br>EQUALLY.||
|**equip (v) — UNNAPPROVED**|INSTALL (v)|INSTALL THE<br>SHUTOFF VALVES ON<br>EACH HP MANIFOLD.|Equip each HP manifold<br>with shutoff valves.|
|**EQUIPMENT (n)**|The objects or tools<br>used for operation and<br>maintenance|REMOVE ALL THE<br>EQUIPMENT FROM<br>THE WORK AREA.||
|**equipped (adj) — UNNAPPROVED**|HAVE (v)|BE CAREFUL WHEN<br>YOU MOVE JET PIPES<br>OR EXHAUST CONES<br>THAT HAVE<br>INSULATING<br>BLANKETS.|Be careful when<br>handling jet pipes or<br>exhaust cones equipped<br>with insulating blankets.|
|**EQUIVALENT (adj)**|Has the same<br>properties, functions, or<br>values|MATERIALS<br>(REF. No. 2) AND<br>(REF. No. 18) ARE<br>EQUIVALENT.||
|**EQUIVALENT (n)**|Something that has the<br>same properties,<br>functions, or values|USE CLEANING<br>COMPOUND ARDROX<br>6025, OR AN<br>EQUIVALENT.||
|**ERASE (v),**<br>**ERASES,**<br>**ERASED,**<br>**ERASED**|To remove data from a<br>medium|ERASE THE TAPE.||

# Page 226 of 434

**Page 2-1-E8**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**erect (v) — UNNAPPROVED**|ASSEMBLE (v)|BEFORE YOU LIFT THE<br>GEARBOX, ASSEMBLE<br>THE MOVABLE HOIST.|Erect the movable hoist<br>before lifting the<br>gearbox.|
|||BECOME STABLE|LET THE VERTICAL<br>GYRO BECOME<br>STABLE.|Give the vertical gyro<br>time to erect.|
|**erratic (adj) — UNNAPPROVED**|IRREGULAR (adj)|THE OPERATION OF<br>THE COMPASS IS<br>IRREGULAR.|The compass is erratic.|
|**ERROR (n)**|The difference from that<br>which is correct or<br>accurate|IF THE ERROR IS<br>MORE THAN 3 DEG.,<br>CALIBRATE THE<br>COMPASS.||
|**escape (v) — UNNAPPROVED**|DEFLATE (v)|DEFLATE THE TIRE.|Let the air escape from<br>the tire.|
|||RELEASE (v)|RELEASE ALL THE<br>NITROGEN.|Allow all the nitrogen to<br>escape.|
|**establish (v) — UNNAPPROVED**|MAKE SURE (v)|IN THE STEP THAT<br>FOLLOWS, MAKE<br>SURE THAT THE FUEL<br>PUMP OPERATES<br>CORRECTLY.|In the following step,<br>establish the correct<br>functioning of the fuel<br>pump.|
|**ESTIMATE (n)**|A calculated,<br>approximate result|MAKE AN ESTIMATE<br>OF THE NECESSARY<br>QUANTITY OF PAINT.||
|**estimate (v) — UNNAPPROVED**|ESTIMATE (n)|MAKE AN ESTIMATE<br>OF THE QUANTITY OF<br>CLEANING FLUID THAT<br>IS NECESSARY.|Estimate the amount of<br>cleaning fluid that is<br>necessary.|
|**evaluate (v) — UNNAPPROVED**|EXAMINE (v)|EXAMINE THE<br>DAMAGE AFTER AN<br>ACCIDENT.|Evaluate the damage<br>after an accident.|
|||ANALYSIS (TN)|MAKE AN ANALYSIS<br>OF THE TEST<br>RESULTS.|Evaluate the test results.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 227 of 434

**Page 2-1-E9**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**evaluation (n) — UNNAPPROVED**|EXAMINE (v)|EXAMINE THE<br>DAMAGE.|Do an evaluation of the<br>damage.|
|||ANALYSIS (TN)|MAKE AN ANALYSIS<br>OF THE TEST<br>RESULTS.|Do an evaluation of the<br>test results.|
|**evaporate (v) — UNNAPPROVED**|DRY (v)|LET THE COMPOUND<br>DRY.|Allow the solvent to<br>evaporate from the<br>compound.|
|**even (adj) — UNNAPPROVED**|SMOOTH (adj)|A GUIDE ROD IS<br>ATTACHED TO THE<br>METAL BELLOWS<br>DISC FOR A SMOOTH<br>MOVEMENT OF THE<br>BELLOWS.|A guide rod is attached<br>to the metal bellows disc<br>for an even movement of<br>the bellows.|
|||SAME (adj)|APPLY THE SAME<br>LOAD ON THE TWO<br>BRAKES.|Braking must be even on<br>the two brakes.|
|||FLAT (adj)|MAKE SURE THAT<br>THE SURFACE IS<br>FLAT.|Ensure the surface is<br>even.|
|||FLUSH (adj)|MAKE SURE THAT<br>THE FASTENER<br>HEADS ARE FLUSH<br>WITH THE SKIN.|Make sure that the<br>fastener heads are even<br>with the skin.|
|||LEVEL (adj)|MAKE SURE THAT<br>THE MARK ON THE<br>BOLT IS LEVEL WITH<br>THE MARK ON THE<br>HANDLE.|Make sure that the mark<br>on the bolt is even with<br>the mark on the handle.|
|**evenly (adv) — UNNAPPROVED**|GRADUALLY (adv)|INCREASE THE<br>TEMPERATURE<br>GRADUALLY.|Increase the<br>temperature evenly.|
|||EQUALLY (adv)|APPLY THE LOAD<br>EQUALLY ON THE<br>AREA.|Apply the load evenly on<br>the area.|
|**event (n) — UNNAPPROVED**|IF (conj)|IF THE PRESSURE<br>DECREASES<br>SUDDENLY, CLOSE<br>THE VALVE.|In the event of a sudden<br>dropping of pressure,<br>close the valve.|
|**eventually (adv) — UNNAPPROVED**|SOME TIME|IF THE CABLE RUBS,<br>IT WILL BREAK AFTER<br>SOME TIME.|If the cable chafes, it will<br>eventually break.|

# Page 228 of 434

**Page 2-1-E10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**every (adj) — UNNAPPROVED**|ALL (adj)|REMOVE ALL SAFETY<br>PINS BEFORE FLIGHT.|Every safety pin must be<br>removed before flight.|
|||EACH (adj)|SET THE BTRY<br>SWITCH TO "ON"<br>EACH TIME.|It is necessary to set the<br>BTRY switch to ON<br>every time.|
|||INTERVAL (n)|DO AN INSPECTION<br>AT INTERVALS OF<br>20 000 FLIGHT<br>HOURS.|Do an inspection every<br>20 000 flight hours.|
|**evidence (n) — UNNAPPROVED**|INDICATION (n)|IF THERE IS AN<br>INDICATION OF A<br>LEAK, REPLACE THE<br>VALVE.|If there is evidence of a<br>leak, replace the valve.|
|||SIGN (n)|ONE SIGN OF A LEAK<br>OF HOT AIR FROM A<br>JOINT IS THAT THE<br>TEMPERATURE<br>INDICATION<br>DECREASES.|Evidence of a leak of hot<br>air from a joint is that the<br>temperature reading<br>drops.|
|**evidence (v) — UNNAPPROVED**|SHOW (v)|IF THE TEST SHOWS<br>NO FAULT, CONTINUE<br>THE PROCEDURE.|If no fault is evidenced<br>by the test, continue the<br>procedure.|
|||FIND (v)|IF YOU DO NOT FIND<br>DAMAGE DURING THE<br>INSPECTION<br>PROCEDURE,<br>ASSEMBLE THE UNIT.|If the inspection does<br>not evidence any<br>damage, assemble the<br>unit.|
|**evident (adj) — UNNAPPROVED**|FIND (v)|IF YOU DO NOT FIND<br>DAMAGE, CONTINUE<br>THE INSPECTION.|If no damage is evident,<br>continue the inspection.|
|**exact (adj) — UNNAPPROVED**|ACCURATE (adj)|IF THE INDICATION IS<br>NOT ACCURATE, DO<br>THE TEST AGAIN.|If the indication is not<br>exact, do the test again.|
|||CORRECT (adj)|IF THE INDICATION IS<br>NOT CORRECT, DO<br>THE TEST AGAIN.|If the indication is not<br>exact, do the test again.|

**Issue 9 Part 2 - Dictionary 2025-01-15**
