# Page 153–156 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 153–156 of 434

# Page 153 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| alter (v) — UNNAPPROVED | CHANGE (v) | IT IS POSSIBLE THAT THE INSTALLATION OF THE CONNECTOR PINS CHANGED THE ROUTING OF THE CABLE LOOM. | It is possible that the installation of the connector pins altered the routing of the cable loom. |
| alteration (n) — UNNAPPROVED | CHANGE (v) | IF YOU CHANGE THIS REPAIR PROCEDURE, GET APPROVAL OF THE DESIGN AUTHORITY. | The alteration to this repair procedure must get approval of the Design Authority. |
| alternate (adj) — UNNAPPROVED | ALTERNATIVE (adj) | AN ALTERNATIVE REPAIR IS AVAILABLE. | An alternate repair is available. |
|  | EACH SECOND | EACH SECOND SQUARE IS RED. | Alternate squares are red. |
| alternate (v) — UNNAPPROVED | THEN (adv) | DO THE PILOT'S INSTRUMENT TEST AND THEN THE COPILOT'S TEST. | Alternate between pilot's and copilot's instrument test. |
| alternately (adv) — UNNAPPROVED | IN ONE (TN) … AND THEN THE OTHER | TO MAKE PIN REMOVAL EASIER, MANUALLY TURN THE CANOPY IN ONE DIRECTION AND THEN IN THE OTHER. | To make pin removal easier, manually turn the canopy alternately in the two directions. |
| ALTERNATIVE (adj) | That gives a choice | YOU CAN USE ALTERNATIVE MATERIALS. |  |
| ALTERNATIVE (n) | One of two or more objects or processes that have the same or almost the same properties or functions | A BIO-BASED FUEL CAN BE AN ALTERNATIVE TO FUELS JET-A1 AND JET-A. |  |
| alternatively (adv) — UNNAPPROVED | ALTERNATIVE (n) | YOU CAN DO TEST B AS AN ALTERNATIVE. | Alternatively, you can do test B. |
| ALTHOUGH (conj) | In spite of the fact that | ALTHOUGH THE PRESSURE DECREASES, THE VALVE MUST STAY CLOSED. |  |
| ALWAYS (adv) | At all times | ALWAYS KEEP THE BRIGHTNESS CONTROL ON THE LCD DISPLAY AT MAXIMUM. |  |

# Page 154 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| amend (v) — UNNAPPROVED | CHANGE (v) | IF IT IS NECESSARY TO CHANGE THE REPAIR SCHEME, GET THE APPROVAL OF THE DESIGN AUTHORITY. | If it is necessary to amend the Repair Scheme, get the approval of the Design Authority. |
| amendment (n) — UNNAPPROVED | CHANGE (n) | THE DESIGN AUTHORITY MUST GIVE APPROVAL TO THE CHANGES THAT YOU MAKE TO THE REPAIR SCHEME. | The Design Authority must approve the amendments that you make to the Repair Scheme. |
|  | CHANGE (v) | IF IT IS NECESSARY TO CHANGE THE REPAIR SCHEME, GET THE APPROVAL OF THE DESIGN AUTHORITY. | If an amendment to the Repair Scheme is necessary, get the approval of the Design Authority. |
| among (prep) — UNNAPPROVED | IN (prep) | IF THERE ARE METAL PARTICLES IN THE SAMPLES, REPLACE THE PUMP. | If there are metal particles among the samples, replace the pump. |
| amount (n) — UNNAPPROVED | QUANTITY (n) | MAKE SURE THAT THE QUANTITY OF FUEL IN THE TANK IS NOT MORE THAN 500 LITERS. | Make sure that the amount of fuel in the tank is not more than 500 liters. |
| AN (art) | Function word: indefinite article | MAKE AN ENTRY IN THE LOGBOOK. |  |
| ANALOG (adj) | Of data given by pointers and dials | THE PRE-MOD UNIT HAS ANALOG INDICATORS. |  |
| analyze (v) — UNNAPPROVED | ANALYSIS (TN) | MAKE AN ANALYSIS OF THE OIL. | Analyze the oil sample. |
| anchor (v) — UNNAPPROVED | ATTACH (v) | THE STRAPS ARE ATTACHED TO A FULL-LENGTH RAIL. | The straps are anchored to a full-length rail. |

# Page 155 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| ancillary (adj) — UNNAPPROVED | AUXILIARY (adj) | THE ENGINE AND ALL AUXILIARY EQUIPMENT USE THE SAME LUBRICANT. | The engine and all ancillary equipment use the same lubricant. |
|  | SECONDARY (adj) | DO AN OPERATIONAL CHECK OF THE SECONDARY CONTROLS. | Do an operational check of the ancillary controls. |
| AND (conj) | Function word used to connect words, phrases, or clauses | MAKE SURE THAT THE FLAPS ARE RETRACTED AND THE AILERON TRIM HANDWHEEL IS IN THE ZERO POSITION. |  |
| ANGULAR (adj) | That has one or more angles | MAKE SURE THAT THE ANGULAR POSITION IS CORRECT. |  |
| annotation (n) — UNNAPPROVED | WRITE (v) | WRITE THE TEMPERATURE VALUE ON THE ENGINE LOG CARD. | Make an annotation of the temperature on the Engine Log Card. |
|  | RECORD (v) | RECORD THE TEMPERATURE VALUE ON THE ENGINE LOG CARD. | Make an annotation of the temperature on the Engine Log Card. |
| annunciate (v) — UNNAPPROVED | SHOW (v) | THE DISPLAY SHOWS A FAULT MESSAGE. | The display annunciates a fault message. |
| another (adj) — UNNAPPROVED | ONE (TN) MORE | INSTALL ONE MORE WASHER BETWEEN THE NUT AND THE SURFACE. | Install another washer between the nut and the surface. |
|  | DIFFERENT (adj) | REFER TO DETAIL C ON FIG. 4 FOR A DIFFERENT PROCEDURE TO ATTACH THE CABLE. | Refer to detail C on Fig. 4 for another way of attaching the cable. |
|  | AGAIN (adv) | BEFORE YOU TRY TO START THE ENGINE AGAIN, MAKE SURE THAT THE AREA IS SAFE. | Before you try another engine start, make sure that the area is safe. |
| anticlockwise (adv) | COUNTERCLOCKWISE (adv) | COUNTERCLOCKWISE. | Turn the cap anticlockwise. |

# Page 156 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| any (adj) — UNNAPPROVED | Frequently, an alternative for this word is not necessary. | IF YOU HAVE QUESTIONS ABOUT THIS DOCUMENT, SEND AN E-MAIL TO THE ADDRESS THAT FOLLOWS: | If you have any questions about this document, send an e-mail to the address that follows: |
| any (pron) — UNNAPPROVED | ONE (TN) | REMOVE ONE OF THE FOUR BOLTS. | Remove any of the four bolts. |
| anytime (adv) — UNNAPPROVED | WHEN (conj) | WHEN YOU USE THE EMERGENCY PUMP, RECORD THE TIME OF OPERATION. | Anytime you use the emergency pump, record the time of operation. |
| APART (adv) | At a distance (not specified) from | MOVE THE CABLE STRANDS APART. |  |
| aperture (n) — UNNAPPROVED | OPENING (n) | GET ACCESS TO THE CONTROL UNIT THROUGH THE OPENING IN THE SIDE OF THE TANK. | Get access to the control unit through the aperture in the side of the tank. |
| apparent (adj) — UNNAPPROVED | SEE (v) | IF YOU SEE DISCOLORATION, REPLACE THE PART. | If discoloration is apparent, replace the part. |
|  | FIND (v) | IF YOU FIND A CRACK, DO THE APPLICABLE REPAIR PROCEDURE. | If a crack is apparent, do the applicable repair procedure. |
| appear (v) — UNNAPPROVED | SHOW (v) | A WARNING FLAG SHOWS IN THE WINDOW. | A warning flag appears in the window. |
| (v) | THINK (v) | IF YOU THINK THAT THE ENGINE IS TOO HOT, TURN THE SWITCH TO "OFF." | If the engine appears to be too hot, turn the switch to off. |
|  | POSSIBLE (adj) | IF IT IS POSSIBLE THAT THE TEMPERATURE VALUES ARE INCORRECT, DECREASE THE POWER. | If it appears that the temperature values are incorrect, decrease the power. |
