<!-- section: DICT_A-F | pages: 161-164 | verified: true -->

# Page 161 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/

| ALTERNATIVE |
| --- |
| (adj) |

THE INSTALLATION OF installation of the
THE CONNECTOR connector pins altered
PINS CHANGED THE the routing of the cable
ROUTING OF THE loom.

### CABLE LOOM.

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **alteration (n) — UNNAPROVED** | CHANGE (v) IF YOU CHANGE THIS The alteration to this REPAIR PROCEDURE, repair procedure must GET APPROVAL OF get approval of the THE DESIGN Design Authority. AUTHORITY. |
| **alternate (adj) — UNNAPROVED** | ALTERNATIVE (adj) AN ALTERNATIVE An alternate repair is REPAIR IS AVAILABLE. available. EACH SECOND EACH SECOND Alternate squares are SQUARE IS RED. red. |
| **alternate (v) — UNNAPROVED** | THEN (adv) DO THE PILOT’S Alternate between pilot’s INSTRUMENT TEST and copilot’s instrument AND THEN THE test. COPILOT’S TEST. |
| **alternately (adv) — UNNAPROVED** | IN ONE (TN) … AND TO MAKE PIN To make pin removal THEN THE OTHER REMOVAL EASIER, easier, manually turn the MANUALLY TURN THE canopy alternately in the CANOPY IN ONE two directions. DIRECTION AND THEN IN THE OTHER. ALTERNATIVE That gives a choice YOU CAN USE (adj) ALTERNATIVE MATERIALS. |
| **ALTERNATIVE (n)** | One of two or more A BIO-BASED FUEL objects or processes that CAN BE AN have the same or almost ALTERNATIVE TO the same properties or FUELS JET-A1 AND functions JET-A. |
| **alternatively (adv) — UNNAPROVED** | ALTERNATIVE (n) YOU CAN DO TEST B Alternatively, you can do AS AN ALTERNATIVE. test B. |
| **ALTHOUGH (conj)** | In spite of the fact that ALTHOUGH THE PRESSURE DECREASES, THE VALVE MUST STAY CLOSED. |
| **ALWAYS (adv)** | At all times ALWAYS KEEP THE BRIGHTNESS CONTROL ON THE LCD DISPLAY AT MAXIMUM. |

# Page 162 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **amend (v) — UNNAPROVED** | CHANGE (v) IF IT IS NECESSARY If it is necessary to TO CHANGE THE amend the Repair REPAIR SCHEME, GET Scheme, get the THE APPROVAL OF approval of the Design THE DESIGN Authority. AUTHORITY. |
| **amendment (n) — UNNAPROVED** | CHANGE (n) THE DESIGN The Design Authority AUTHORITY MUST must approve the GIVE APPROVAL TO amendments that you THE CHANGES THAT make to the Repair YOU MAKE TO THE Scheme. REPAIR SCHEME. |
| **CHANGE (v)** | IF IT IS NECESSARY If an amendment to the TO CHANGE THE Repair Scheme is REPAIR SCHEME, GET necessary, get the THE APPROVAL OF approval of the Design THE DESIGN Authority. AUTHORITY. |
| **among (prep) — UNNAPROVED** | IN (prep) IF THERE ARE METAL If there are metal PARTICLES IN THE particles among the SAMPLES, REPLACE samples, replace the THE PUMP. pump. |
| **amount (n) — UNNAPROVED** | QUANTITY (n) MAKE SURE THAT THE Make sure that the QUANTITY OF FUEL IN amount of fuel in the THE TANK IS NOT tank is not more than MORE THAN 500 500 liters. LITERS. |
| **AN (art)** | Function word: MAKE AN ENTRY IN indefinite article THE LOGBOOK. |
| **ANALOG (adj)** | Of data given by pointers THE PRE-MOD UNIT and dials HAS ANALOG INDICATORS. |
| **analyze (v) — UNNAPROVED** | ANALYSIS (TN) MAKE AN ANALYSIS Analyze the oil sample. OF THE OIL. |
| **anchor (v) — UNNAPROVED** | ATTACH (v) THE STRAPS ARE The straps are anchored ATTACHED TO A to a full-length rail. FULL-LENGTH RAIL. |

# Page 163 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **ancillary (adj) — UNNAPROVED** | AUXILIARY (adj) THE ENGINE AND ALL The engine and all AUXILIARY ancillary equipment use EQUIPMENT USE THE the same lubricant. SAME LUBRICANT. |
| **SECONDARY (adj)** | DO AN OPERATIONAL Do an operational check CHECK OF THE of the ancillary controls. SECONDARY CONTROLS. |
| **AND (conj)** | Function word used to MAKE SURE THAT THE connect words, phrases, FLAPS ARE or clauses RETRACTED AND THE AILERON TRIM HANDWHEEL IS IN THE ZERO POSITION. |
| **ANGULAR (adj)** | That has one or more MAKE SURE THAT THE angles ANGULAR POSITION IS CORRECT. |
| **annotation (n) — UNNAPROVED** | WRITE (v) WRITE THE Make an annotation of TEMPERATURE VALUE the temperature on the ON THE ENGINE LOG Engine Log Card. CARD. |
| **RECORD (v)** | RECORD THE Make an annotation of TEMPERATURE VALUE the temperature on the ON THE ENGINE LOG Engine Log Card. CARD. |
| **annunciate (v) — UNNAPROVED** | SHOW (v) THE DISPLAY SHOWS The display annunciates A FAULT MESSAGE. a fault message. |
| **another (adj) — UNNAPROVED** | ONE (TN) MORE INSTALL ONE MORE Install another washer WASHER BETWEEN between the nut and the THE NUT AND THE surface. SURFACE. |
| **DIFFERENT (adj)** | REFER TO DETAIL C Refer to detail C on Fig. ON FIG. 4 FOR A 4 for another way of DIFFERENT attaching the cable. PROCEDURE TO ATTACH THE CABLE. |
| **AGAIN (adv)** | BEFORE YOU TRY TO Before you try another START THE ENGINE engine start, make sure AGAIN, MAKE SURE that the area is safe. THAT THE AREA IS SAFE. anticlockwise COUNTERCLOCKWISE TURN THE CAP Turn the cap (adv) (adv) COUNTERCLOCKWISE. anticlockwise. |

# Page 164 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **any (adj) — UNNAPROVED** | Frequently, an IF YOU HAVE If you have any alternative for this QUESTIONS ABOUT questions about this word is not THIS DOCUMENT, document, send an necessary. SEND AN E-MAIL TO e-mail to the address THE ADDRESS THAT that follows: FOLLOWS: |
| **any (pron) — UNNAPROVED** | ONE (TN) REMOVE ONE OF THE Remove any of the four FOUR BOLTS. bolts. |
| **anytime (adv) — UNNAPROVED** | WHEN (conj) WHEN YOU USE THE Anytime you use the EMERGENCY PUMP, emergency pump, record RECORD THE TIME OF the time of operation. OPERATION. |
| **APART (adv)** | At a distance (not MOVE THE CABLE specified) from STRANDS APART. |
| **aperture (n) — UNNAPROVED** | OPENING (n) GET ACCESS TO THE Get access to the control CONTROL UNIT unit through the aperture THROUGH THE in the side of the tank. OPENING IN THE SIDE OF THE TANK. |
| **apparent (adj) — UNNAPROVED** | SEE (v) IF YOU SEE If discoloration is DISCOLORATION, apparent, replace the REPLACE THE PART. part. |
| **FIND (v)** | IF YOU FIND A CRACK, If a crack is apparent, do DO THE APPLICABLE the applicable repair REPAIR PROCEDURE. procedure. |
| **appear (v) — UNNAPROVED** | SHOW (v) A WARNING FLAG A warning flag appears SHOWS IN THE in the window. WINDOW. |
| **VIEW (n)** | WHEN YOU PULL THE The lower seal appears LOWER BEARING when you pull the lower DOWN, THE LOWER bearing down. SEAL COMES INTO VIEW. |
| **THINK (v)** | IF YOU THINK THAT If the engine appears to THE ENGINE IS TOO be too hot, turn the HOT, TURN THE switch to off. SWITCH TO “OFF.” |
| **POSSIBLE (adj)** | IF IT IS POSSIBLE If it appears that the THAT THE temperature values are TEMPERATURE incorrect, decrease the VALUES ARE power. INCORRECT, DECREASE THE POWER. |
