<!-- section: DICT_G-P | pages: 269-272 | verified: true -->

# Page 269 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **HAVE (v)** | , To possess as a part or THE SYSTEM HAS AN HAS, quality EMERGENCY HAD WARNING DEVICE. No other verb forms. |
| **have to (v) — UNNAPROVED** | Use a verb in the WHEN ENGINES ARE When engines are in imperative form IN OPERATION, PUT operation, you have to ON A HEARING put on a hearing PROTECTION DEVICE. protection device. |
| **hazard (n) — UNNAPROVED** | DANGEROUS (adj) TRICHLORO- Trichloroethylene is a ETHYLENE IS health hazard. “hazard” can be DANGEROUS. part of safety regulations. |
| **hazardous (adj) — UNNAPROVED** | DANGEROUS (adj) ALL PERSONNEL WHO All personnel who work DO WORK WITH with hazardous materials “hazardous” can DANGEROUS must obey the following be part of safety MATERIALS MUST safety instructions. regulations. OBEY THE SAFETY INSTRUCTIONS THAT FOLLOW. |
| **hazy (adj) — UNNAPROVED** | HAZE (TN) IF THERE IS HAZE, DO If the weather is hazy, do NOT DO THE TEST. not do the test. |
| **HEAD (n)** | The top of something MAKE SURE THAT THE HEAD OF THE BOLT IS DOWN. |
| **head (v) — UNNAPROVED** | POINT (v) POINT THE AIRCRAFT Head the aircraft into the INTO THE WIND. wind. |
| **HEAR (v)** | , To know by sound in the MAKE SURE THAT HEARS, ear YOU HEAR THE AUDIO HEARD, SIGNALS IN ALL THE HEARD CREW HEADSETS. |
| **HEAT (n)** | The condition or quality USE HEAT TO CURE of being hot THE POLYSULPHIDE SEALANT. |

# Page 270 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **heat (v) — UNNAPROVED** | HEAT (n) USE HEAT TO Heat the oil to 40 C. INCREASE THE TEMPERATURE OF THE OIL TO 40 C. |
| **HOT (adj)** | WHEN THE OIL IS HOT, When you heat the oil, it IT FLOWS FREELY. flows freely. |
| **HEAVY (adj)** | That has a large mass, A SUPPORT WILL BE (HEAVIER, weight, or force NECESSARY HEAVIEST) BECAUSE THE CONTROL UNIT IS HEAVY. |
| **HEIGHT (n)** | The vertical distance THE HEIGHT FROM THE GROUND TO THE TOP OF THE FIN CAN CHANGE. |
| **heighten (v) — UNNAPROVED** | INCREASE (v) STRONG WINDS WILL Strong winds will INCREASE THE RISK heighten the risk of OF DAMAGE. damage. |
| **help (n) — UNNAPROVED** | AID (n) GET MEDICAL AID You must get medical IMMEDIATELY. help immediately. |
| **HELP (v)** | , To make something PETROLATUM HELPS HELPS, easier or better TO PREVENT HELPED, CORROSION OF THE HELPED TERMINALS. |
| **helpful (adj) — UNNAPROVED** | HELP (v) RECORD THE Record the lockwire LOCKWIRE positions. This will be POSITIONS. THIS helpful during the INFORMATION WILL assembly procedure. HELP YOU DURING THE ASSEMBLY PROCEDURE. |
| **HERE (adv)** | In this position TO DOWNLOAD THE FILE, CLICK HERE. |
| **hesitation (n) — UNNAPROVED** | SMOOTHLY (adv) MAKE SURE THAT THE Make sure that the SOLENOID OPERATES solenoid operates SMOOTHLY. without hesitation. |
| **CORRECTLY (adv)** | THE VALVE MUST The valve must operate OPERATE without hesitation. CORRECTLY. |
| **IMMEDIATELY (adv)** | WHEN YOU OPEN THE When you open the CIRCUIT BREAKER, circuit breaker, the light THE LIGHT MUST must come on without COME ON hesitation. IMMEDIATELY. |

# Page 271 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **HIGH (adj)** | That is of large value USE THE SPECIAL (HIGHER, PROTECTION FOR HIGHEST) STORAGE IN HIGH TEMPERATURES. |
| **highly (adv) — UNNAPROVED** | VERY (adv) TOLUENE IS VERY Toluene is highly FLAMMABLE. flammable. |
| **hinder (v) — UNNAPROVED** | PREVENT (v) SCRATCHES CAN Scratches can hinder the PREVENT THE FREE movement of the piston MOVEMENT OF THE in the sleeve. PISTON IN THE SLEEVE. |
| **DECREASE (v)** | A CLOGGED DUCT A clogged duct will WILL DECREASE hinder airflow. AIRFLOW. |
| **BLOCKAGE (n)** | MAKE SURE THAT Make sure that there is THERE IS NO nothing in the pipe to BLOCKAGE IN THE hinder airflow. PIPE THAT PREVENTS AIRFLOW. |
| **CLOGGED (adj)** | MAKE SURE THAT THE Make sure that there is PIPE IS NOT nothing in the pipe to CLOGGED. hinder airflow. |
| **hinge (v) — UNNAPROVED** | TURN (v) THE PANELS TURN ON Panels hinge on two TWO NYLON STRAPS. nylon straps. |
| **HIT (v)** | , To touch suddenly and DO NOT HIT THE HITS, with much force CARTRIDGE. HIT, HIT |
| **hitch (v) — UNNAPROVED** | CONNECT (v) CONNECT THE Hitch the towing arm to TOWING ARM TO THE the nosewheel. NOSEWHEEL. |
| **hoist (v) — UNNAPROVED** | LIFT (v) LIFT THE MODULE. Hoist the module. |
| **hold (n) — UNNAPROVED** | HOLD (v) MAKE SURE THAT Make sure that you have YOU HOLD THE ROD a tight hold on the rod. TIGHTLY. |
| **HOLD (v)** | , 1. To continue to have HOLD THE ROD HOLDS, in the hand or grip TIGHTLY. HELD, HELD 2. To continue to have HOLD THE AIRSPEED in a specified INDICATION AT THE location, position, or SAME VALUE FOR condition 2 MINUTES. |

# Page 272 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **hold back (v) — UNNAPROVED** | PREVENT (v) AT FULL THRUST, THE At full thrust, the brakes BRAKES MUST must hold the aircraft PREVENT MOVEMENT back. OF THE AIRCRAFT. |
| **hold off (v) — UNNAPROVED** | PREVENT (v) THE PROTECTIVE The protective paint will PAINT WILL PREVENT hold off corrosion for six CORROSION FOR SIX months. MONTHS. |
| **HOLE (n)** | An empty space in a MAKE SURE THAT THE solid object HOLES IN THE BUSHING ALIGN WITH THOSE IN THE HOUSING. |
| **hook (v) — UNNAPROVED** | PUT (v) PUT THE SLING ON Hook the sling on the THE SHACKLE. shackle. |
| **hook up (v) — UNNAPROVED** | CONNECT (v) CONNECT THE Hook the towing arm up TOWING ARM TO THE to the nose gear. NOSE GEAR. |
| **HORIZONTAL (adj)** | Parallel to the horizon or ADJUST THE SLING a baseline UNTIL THE FLAP IS HORIZONTAL. HORIZONTALLY In a horizontal position THE VALVE IS (adv) INSTALLED HORIZONTALLY. |
| **HOT (adj)** | At a high temperature DRY THE SURFACE (HOTTER, WITH HOT AIR. HOTTEST) |
| **house (v) — UNNAPROVED** | CONTAIN (v) THE MODULE The module houses five CONTAINS FIVE components. COMPONENTS. |
| **HOW (adv)** | By which manner PARAGRAPH 7.0 TELLS YOU HOW TO INSTALL THE UNIT. |
| **however (adv) — UNNAPROVED** | BUT (conj) THE DRYING TIME IS The drying time is USUALLY 24 HOURS. usually 24 hours. BUT THE PROCEDURE However, the procedure IN THIS STEP WILL in this step will decrease DECREASE THE the drying time to DRYING TIME TO 12 hours. 12 HOURS. |
