# Page 305 of 434

# Page 305 of 434

**Page 2-1-M9**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**MOVE (v),**<br>**MOVES,**<br>**MOVED,**<br>**MOVED**|To change or cause to<br>change position or<br>location|MAKE SURE THAT THE<br>POINTER MOVES<br>FREELY.|
|||MOVE THE VALVE<br>UNTIL IT ALIGNS WITH<br>THE ACTUATOR<br>SHAFT.|
|**MOVEMENT (n)**|A change of position or<br>location|SUDDEN OPERATION<br>OF THE GYRO CAN<br>CAUSE UNWANTED<br>MOVEMENT OF THE<br>HORIZONTAL<br>STABILIZER.|
|**MUCH (adj)**<br>**(MORE, MOST)**|Of relatively large<br>dimension, value,<br>quantity, or volume|DO NOT APPLY TOO<br>MUCH PRESSURE.|
|**MUCH (adv)**|To a great degree or<br>extent|BE CAREFUL THAT<br>YOU DO NOT TURN<br>THE INNER RACES<br>TOO MUCH.|
|**MULTIPLY (v),**<br>**MULTIPLIES,**<br>**MULTIPLIED,**<br>**MULTIPLIED**|To use multiplication to<br>get a result<br>For other<br>meanings, use:|MULTIPLY THE<br>INDICATOR VALUE BY<br>THE SCALE VALUE.|
|||INCREASE (v)|THE NUMBER OF<br>CRACKS CAN<br>INCREASE.|Cracks can multiply.|
|**MUST (v)**|Auxiliary modal verb that<br>shows obligation|THE BAT 1 SWITCH<br>MUST BE IN THE ON<br>POSITION.|

# Page 306 of 434

**Page 2-1-M10**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**NAME (n)**|The identification you<br>give to a person or an<br>object|PUSH THE BUTTON<br>ADJACENT TO THE<br>NAME OF THE<br>SYSTEM.|
|||WRITE YOUR NAME<br>ON THE<br>REGISTRATION FORM.|
|**NEAR (adj)**<br>**(NEARER,**<br>**(NEAREST)**|At or to a relatively short<br>distance|PUT THE SYRINGE ON<br>THE NEAREST<br>SURFACE OF THE<br>EXAMINATION TABLE.|
|**NEAR (prep)**|Approaching in space or<br>condition|BALANCE THE<br>ELEVATOR NEAR ITS<br>MAXIMUM LIMIT.|
|||MAKE SURE THAT THE<br>COMPUTER SCREEN<br>IS NOT NEAR THE<br>WINDOW.|
|**nearly (adv) — UNNAPPROVED**|ALMOST (adv)|MOVE THE POINTER<br>UNTIL IT IS ALMOST IN<br>THE GREEN BAND.|Move the pointer until<br>nearly in the green band.|
|**NECESSARY (adj)**|That must be|TWO HOURS ARE<br>NECESSARY TO<br>COMPLETE THE<br>EXAM.|
|**need (v) — UNNAPPROVED**|NECESSARY (adj)|DURING THIS<br>PROCEDURE, IT IS<br>NOT NECESSARY TO<br>REPLACE THE<br>BACKING RINGS.|The backing rings do not<br>need to be replaced<br>during this procedure.|
|**neither (adj) — UNNAPPROVED**|TWO (TN) … NOT|THE TWO UNITS MUST<br>NOT OPERATE.|Neither unit must<br>operate.|
|**neither (pron) — UNNAPPROVED**|TWO (TN) … NOT|THE TWO UNITS MUST<br>NOT OPERATE.|Neither of the units must<br>operate.|
|**NEUTRAL (adj)**|1.<br>That has no effect|MAKE SURE THAT THE<br>CONTROLS ARE IN<br>THE NEUTRAL<br>POSITION.|
|||2.<br>That is not acid or<br>alkaline|CLEAN THE SCREEN<br>WITH A NEUTRAL<br>SOLUTION.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 307 of 434

**Page 2-1-N1**

**ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**neutralize (v) — UNNAPPROVED**|NEUTRAL (adj)|MAKE THE BASIC<br>ELECTROLYTE<br>NEUTRAL WITH<br>VINEGAR OR BORIC<br>ACID.| Neutralize the basic<br>electrolyte with vinegar<br>or boric acid.|
|**never (adv) — UNNAPPROVED**|DO NOT|DO NOT LET THE<br>LEVEL IN THE TANK<br>DECREASE TO LESS<br>THAN HALF.|Never allow the level in<br>the tank to drop below<br>half.|
|**NEW (adj)**<br>**(NEWER,**<br>**(NEWEST)**|Not used before|INSTALL A NEW<br>GASKET ON THE<br>FLANGE.|
|**NEXT (adj)**|The first occurrence that<br>follows immediately after<br>in time or sequence.|REMOVE THE UNIT<br>BEFORE THE NEXT<br>OPERATING CYCLE.|
|**next (adv) — UNNAPPROVED**|THEN (adv)|HOLD THE FLANGE IN<br>ITS POSITION. THEN,<br>INSTALL THE BOLT.|Hold the flange in its<br>position. Next, install the<br>bolt.|
|**next to (prep) — UNNAPPROVED**|ADJACENT TO (prep)|THE PUMP IS<br>ADJACENT TO THE<br>CENTRAL RIB.|The pump is next to the<br>central rib.|
|**NO (adj)**|Not any|MAKE SURE THAT<br>THERE IS NO FUEL<br>LEAKAGE.|
|**NO (adv)**|Function word that<br>shows the negative<br>answer to a question|DOES THE LIGHT<br>COME ON?<br>YES OR NO?|
|**NOISE (n)**|An unwanted sound|WHILE THE ENGINE<br>CONTINUES TO TURN,<br>LISTEN FOR UNUSUAL<br>NOISES.|
|**noisy (adj) — UNNAPPROVED**|NOISE (n)|IF THERE IS NOISE<br>WHEN THE PUMP<br>OPERATES, EXAMINE<br>THE FILTER FOR<br>UNWANTED<br>PARTICLES.|If pump operation is<br>noisy, check the pump<br>filter for unwanted<br>particles.|
|**NONE (pron)**|Not one, not anyone|IF NONE OF THE<br>BRACKETS ARE<br>DAMAGED, CONTINUE<br>THE INSPECTION.|

# Page 308 of 434

**Page 2-1-N2**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

##### **ASD-STE100 Simplified Technical English**

|**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
|---|---|---|---|
|**nor (conj) — UNNAPPROVED**|NOT (adv)|IN THESE<br>CONDITIONS, THE<br>MECHANICAL AND<br>ELECTRICAL PITCH<br>TRIM SYSTEMS WILL<br>NOT OPERATE.|In these conditions,<br>neither the mechanical<br>nor the electrical pitch<br>trim systems will<br>operate.|
|**normal (adj) — UNNAPPROVED**|USUAL (adj)|THE "ARMED"<br>POSITION IS THE<br>USUAL POSITION OF<br>THE SWITCH.|The ARMED position is<br>the normal position of<br>the switch.|
|||CORRECT (adj)|THE CORRECT<br>PRESSURE FOR<br>OPERATION IS<br>3000 psi.|Normal operating<br>pressure is 3000 psi.|
|**normally (adv) — UNNAPPROVED**|USUALLY (adv)|THE SWITCH IS<br>USUALLY IN THE<br>"STANDBY" POSITION.|The switch is normally in<br>the STANDBY position.|
|||CORRECTLY (adv)|IF THE SYSTEM DOES<br>NOT OPERATE<br>CORRECTLY, REFER<br>TO THE FAULT<br>ISOLATION<br>PROCEDURE.|If the system does not<br>operate normally, refer<br>to the fault isolation<br>procedure.|
|**NOSE (n)**|The front end or part, a<br>part that protrudes|PULL THE<br>TRANSPARENT<br>PLASTIC COLLAR<br>AWAY FROM THE<br>NOSE OF THE<br>ELECTRICAL LATCH.|
|**NOT (adv)**|Adverb of negation|DO NOT LET THE<br>PRESSURE INCREASE<br>TO MORE THAN<br>3000 psi.|
|**NOTCH (n)|An area in the shape of<br>a "V"|MAKE SURE THAT THE<br>BOGIE ROLLERS ARE<br>ALIGNED WITH THE<br>NOTCHES IN THE<br>TRACK.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
