<!-- section: DICT_Q-Z | pages: 313-316 | verified: true -->

# Page 313 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **MOOR (v)** | , To hold something in IN BAD WEATHER MOORS, position with ropes and CONDITIONS, MOOR MOORED, cables THE BOAT. MOORED |
| **MORE (adj)** | A large quantity of ADD MORE SHIMS UNTIL YOU GET THE SPECIFIED CLEARANCE. |
| **MORE (adv)** | To a larger degree CORROSION CAN OCCUR MORE EASILY IN THIS AREA THAN IN OTHER AREAS. |
| **MOST (adj)** | To the largest quantity of MOST MANUFACTURERS RECOMMEND SYNTHETIC LUBRICANTS. |
| **MOST (adv)** | To the largest degree FAULT MESSAGES THAT SHOW IN RED ARE THE MOST IMPORTANT. |
| **motion (n) — UNNAPROVED** | MOVEMENT (n) MAKE SURE THAT THE Check that the stabilizer STABILIZER motion continues. MOVEMENT CONTINUES. |
| **motor (v) — UNNAPROVED** | DRY-MOTOR (TV) DRY-MOTOR THE Motor the engine without ENGINE. fuel. WET-MOTOR (TV) WET-MOTOR THE Motor the engine without ENGINE. ignition. MOTORING (TN) DO A MOTORING Motor the engine. PROCEDURE. |
| **mount (v) — UNNAPROVED** | INSTALL (v) INSTALL THE Mount the manifold. MANIFOLD. |
| **ATTACH (v)** | ATTACH THE SEATS Mount the seats on the TO THE SEAT seat tracks. TRACKS. |
| **PUT (v)** | PUT THE WHEEL ON Mount the wheel on the THE AXLE. axle. |
| **MOVABLE (adj)** | That can move if TURN THE MOVABLE necessary HALF-COLLAR OF THE SUPPORT. |

# Page 314 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **MOVE (v)** | , To change or cause to MAKE SURE THAT THE MOVES, change position or POINTER MOVES MOVED, location FREELY. MOVED MOVE THE VALVE UNTIL IT ALIGNS WITH THE ACTUATOR SHAFT. |
| **MOVEMENT (n)** | A change of position or SUDDEN OPERATION location OF THE GYRO CAN CAUSE UNWANTED MOVEMENT OF THE HORIZONTAL STABILIZER. |
| **MUCH (adj)** | Of relatively large DO NOT APPLY TOO (MORE, MOST) dimension, value, MUCH PRESSURE. quantity, or volume |
| **MUCH (adv)** | To a great degree or BE CAREFUL THAT extent YOU DO NOT TURN THE INNER RACES TOO MUCH. |
| **MULTIPLY (v)** | , To use multiplication to MULTIPLY THE MULTIPLIES, get a result INDICATOR VALUE BY MULTIPLIED, THE SCALE VALUE. For other MULTIPLIED meanings, use: |
| **INCREASE (v)** | THE NUMBER OF Cracks can multiply. CRACKS CAN INCREASE. |
| **MUST (v)** | Auxiliary modal verb that THE BAT 1 SWITCH shows obligation MUST BE IN THE ON POSITION. |

# Page 315 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **NAME (n)** | The identification you PUSH THE BUTTON give to a person or an ADJACENT TO THE object NAME OF THE SYSTEM. WRITE YOUR NAME ON THE REGISTRATION FORM. |
| **NEAR (adj)** | At or to a relatively short PUT THE SYRINGE ON (NEARER, distance THE NEAREST NEAREST) SURFACE OF THE EXAMINATION TABLE. |
| **NEAR (prep)** | Approaching in space or BALANCE THE condition ELEVATOR NEAR ITS MAXIMUM LIMIT. MAKE SURE THAT THE COMPUTER SCREEN IS NOT NEAR THE WINDOW. |
| **nearly (adv) — UNNAPROVED** | ALMOST (adv) MOVE THE POINTER Move the pointer until UNTIL IT IS ALMOST IN nearly in the green band. THE GREEN BAND. |
| **NECESSARY (adj)** | That must be TWO HOURS ARE NECESSARY TO COMPLETE THE EXAM. |
| **need (v) — UNNAPROVED** | NECESSARY (adj) DURING THIS The backing rings do not PROCEDURE, IT IS need to be replaced NOT NECESSARY TO during this procedure. REPLACE THE BACKING RINGS. |
| **neither (adj) — UNNAPROVED** | TWO (TN) … NOT THE TWO UNITS MUST Neither unit must NOT OPERATE. operate. |
| **neither (pron) — UNNAPROVED** | TWO (TN) … NOT THE TWO UNITS MUST Neither of the units must NOT OPERATE. operate. |
| **NEUTRAL (adj)** | 1. That has no effect MAKE SURE THAT THE CONTROLS ARE IN THE NEUTRAL POSITION. 2. That is not acid or CLEAN THE SCREEN alkaline WITH A NEUTRAL SOLUTION. |

# Page 316 of 434

ASD-STE100 Simplified Technical English
Word Approved meaning/
(part of speech) ALTERNATIVES STE EXAMPLE Non-STE example

| Word (POS) | Meaning & Examples |
|------------|-------------------|
| **neutralize (v) — UNNAPROVED** | NEUTRAL (adj) MAKE THE BASIC Neutralize the basic ELECTROLYTE electrolyte with vinegar NEUTRAL WITH or boric acid. VINEGAR OR BORIC ACID. |
| **never (adv) — UNNAPROVED** | DO NOT DO NOT LET THE Never allow the level in LEVEL IN THE TANK the tank to drop below DECREASE TO LESS half. THAN HALF. |
| **NEW (adj)** | Not used before INSTALL A NEW (NEWER, GASKET ON THE NEWEST) FLANGE. |
| **NEXT (adj)** | The first occurrence that REMOVE THE UNIT follows immediately after BEFORE THE NEXT in time or sequence. OPERATING CYCLE. |
| **next (adv) — UNNAPROVED** | THEN (adv) HOLD THE FLANGE IN Hold the flange in its ITS POSITION. THEN, position. Next, install the INSTALL THE BOLT. bolt. |
| **next to (prep) — UNNAPROVED** | ADJACENT TO (prep) THE PUMP IS The pump is next to the ADJACENT TO THE central rib. CENTRAL RIB. |
| **NO (adj)** | Not any MAKE SURE THAT THERE IS NO FUEL LEAKAGE. |
| **NO (adv)** | Function word that DOES THE LIGHT shows the negative COME ON? answer to a question YES OR NO? |
| **NOISE (n)** | An unwanted sound WHILE THE ENGINE CONTINUES TO TURN, LISTEN FOR UNUSUAL NOISES. |
| **noisy (adj) — UNNAPROVED** | NOISE (n) IF THERE IS NOISE If pump operation is WHEN THE PUMP noisy, check the pump OPERATES, EXAMINE filter for unwanted THE FILTER FOR particles. UNWANTED PARTICLES. |
| **NONE (pron)** | Not one, not anyone IF NONE OF THE BRACKETS ARE DAMAGED, CONTINUE THE INSPECTION. |
