# Page 361–364 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 361–364 of 434

# Page 361 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **secure (adj) — UNNAPPROVED** | TIGHT (adj) | MAKE SURE THAT THE<br>BOLTS ARE TIGHT. | Make sure that the bolts<br>are secure. |
|  | SAFE (adj) | BEFORE YOU LIFT<br>THE PLATFORM, MAKE<br>SURE THAT IT IS<br>SAFE. | Make sure that the<br>platform is secure before<br>you lift it. |
|  | CORRECTLY (adv) | MAKE SURE THAT THE<br>BRACKETS ARE<br>CORRECTLY<br>ATTACHED. | Check the brackets for<br>secure attachment. |
| **secure (v) — UNNAPPROVED** | ATTACH (v) | REMOVE THE BOLTS<br>THAT ATTACH THE<br>UNIT. | Remove the bolts that<br>secure the unit. |
|  | SAFETY (v) | SAFETY THE PULLEY<br>GUARD PINS WITH<br>SPLIT PINS. | Secure the pulley guard<br>pins with split pins. |
| **securely (adv) — UNNAPPROVED** | CORRECTLY (adv) | MAKE SURE THAT THE<br>BRACKETS ARE<br>CORRECTLY<br>ATTACHED. | Make sure that the<br>brackets are securely<br>attached. |
|  | SAFELY (adv) | MAKE SURE THAT THE<br>LADDER IS SAFELY<br>ATTACHED. | Make sure the ladder is<br>securely attached. |
|  | TIGHT (adj) | MAKE SURE THAT THE<br>BOLTS ARE TIGHT. | Make sure that the bolts<br>are securely installed. |
| **security (n) — UNNAPPROVED** | CORRECTLY (adv) | MAKE SURE THAT THE<br>COMPONENTS ARE<br>CORRECTLY<br>ATTACHED. | Check the security of the<br>components. |

# Page 362 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **SEE (v),**<br>**SEES,**<br>**SAW,**<br>**SEEN** | To know with the eyes | MAKE SURE THAT<br>YOU CAN SEE THE<br>CABLE THROUGH THE<br>INSPECTION HOLE. |  |
|  | For other<br>meanings, use:<br>REFER (v) | REFER TO TABLE 8001<br>FOR THE APPLICABLE<br>TORQUE VALUES. | See Table 8001 for the<br>applicable torque values. |
|  | EXAMINE (v) | EXAMINE THE<br>MEMBRANE FOR<br>HOLES. | Check the membrane to<br>see if there are holes. |
|  | MAKE SURE (v) | MOVE THE TUBE TO<br>MAKE SURE THAT ITS<br>INNER CONNECTION<br>IS TIGHT. | Move the tube to see if<br>its inner connection is<br>tight. |
| **seek (v) — UNNAPPROVED** | GET (v) | GET MEDICAL AID<br>IMMEDIATELY. | Seek medical attention<br>immediately. |
| **seepage (n) — UNNAPPROVED** | LEAKAGE (n) | CLEAN THE AREAS<br>WHERE THERE IS<br>HYDRAULIC FLUID<br>LEAKAGE. | Clean the areas where<br>there is hydraulic fluid<br>seepage. |
| **seized (adj) — UNNAPPROVED** | CATCH (v) | IF THE CONTROL<br>CABLE IS CAUGHT IN<br>THE PULLEY,<br>RELEASE THE CABLE<br>TENSION. | If the control cable is<br>seized in the pulley,<br>release the cable<br>tension. |
|  | MOVE (v) | IF YOU CANNOT MOVE<br>THE BOLTS, APPLY<br>SOME PENETRATING<br>OIL. | If the bolts are seized,<br>apply some penetrating<br>oil. |
|  | TURN (v) | IF THE FLAP CONTROL<br>MOTOR CANNOT<br>TURN, USE THE<br>ALTERNATIVE MODE. | If the flap control motor<br>is seized, use the<br>alternate mode. |

# Page 363 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **SELECT (v),**<br>**SELECTS,**<br>**SELECTED,**<br>**SELECTED** | To make a choice | SELECT THE<br>HYDRAULIC SYSTEM<br>THAT YOU WILL<br>PRESSURIZE. |  |
|  | SELECT A LANGUAGE<br>FROM THE MENU. |  |  |
|  | Do not use this<br>word as a<br>synonym for<br>SET (v). | SET THE SWITCH TO<br>"TEST." | Select the switch to<br>TEST. |
| **SELECTION (n)** | The action or result of<br>choosing | THE OPERATION OF<br>THE INDICATOR DOES<br>NOT PREVENT THE<br>SELECTION OF<br>SYSTEM 1. |  |
| **SEMICIRCULAR**<br>**(adj)** | That has the shape of<br>half a circle | THE VALVE FLAPS<br>ARE SEMICIRCULAR. |  |
| **SEND (v),**<br>**SENDS,**<br>**SENT,**<br>**SENT** | To cause to go | SEND THE FILTER<br>ELEMENT TO THE<br>MAINTENANCE SHOP<br>FOR THE NECESSARY<br>INSPECTION. |  |
| **SENSE (v),**<br>**SENSES,**<br>**SENSED,**<br>**SENSED** | To get an input<br>automatically | THE TEMPERATURE<br>BULB SENSES THE<br>EXTERNAL AIR<br>TEMPERATURE. |  |
| **SENSITIVE (adj)** | That can sense small<br>changes | THE CAPSULE IS<br>SENSITIVE TO<br>PRESSURE CHANGES. |  |
| **separable (adj) — UNNAPPROVED** | DISASSEMBLE (v) | YOU CAN<br>DISASSEMBLE THIS<br>UNIT INTO TWO<br>PARTS. | This unit is separable<br>into two parts. |
|  | DISCONNECT (v) | YOU CAN<br>DISCONNECT THESE<br>LINE FITTINGS. | These line fittings are<br>separable. |

# Page 364 of 434

| Word (part of speech) | Approved meaning/ALTERNATIVES | STE EXAMPLE | Non-STE example |
|---|---|---|---|
| **separate (adj) — UNNAPPROVED** | ISOLATED (adj) | EACH HYDRAULIC<br>SYSTEM IS FULLY<br>ISOLATED. | All hydraulic systems are<br>completely separate. |
|  | DIFFERENT (adj) | PUT THE REMAINING<br>PARTS IN A<br>DIFFERENT<br>CONTAINER. | Put the remaining parts<br>in a separate container. |
|  | NOT CONNECTED | THESE TWO TRACKS<br>ARE NOT CONNECTED<br>TO THE OTHER TWO. | These two tracks are<br>separate from the other<br>two. |
|  | NOT ATTACHED | THE CAP IS NOT<br>ATTACHED TO THE<br>COUPLING. | The cap is separate from<br>the coupling. |
| **separate (v) — UNNAPPROVED** | DISCONNECT (v) | DISCONNECT THE<br>LINE FITTINGS. | Separate the line fittings. |
|  | DIVIDE (v) | YOU CAN DIVIDE THE<br>DRAINS INTO THREE<br>GROUPS. | You can separate the<br>drains into three groups. |
| **separately (adv) — UNNAPPROVED** | INDEPENDENTLY (adv) | THE SYSTEM<br>MONITORS THE<br>CONDITION OF THE<br>PARTS<br>INDEPENDENTLY. | The system monitors the<br>condition of the parts<br>separately. |
| **SEPARATION (n)** | The action or result of<br>separating | SEPARATION OF<br>THESE PARTS IS NOT<br>EASY. |  |
| **SEQUENCE (n)** | The relation of items that<br>follow one after the other<br>in a list or the relation of<br>steps or events that<br>occur one after the other<br>in time | TIGHTEN THE BOLTS<br>IN THE SEQUENCE<br>THAT IS GIVEN IN<br>FIGURE 3. |  |
| **serious (adj) — UNNAPPROVED** | IMPORTANT (adj) | VIRUS<br>CONTAMINATION IS<br>AN IMPORTANT<br>PROBLEM. | Virus contamination is a<br>serious problem. |
|  | DANGEROUS (adj) | HYDRAULIC FLUID IS<br>DANGEROUS FOR<br>YOUR EYES. | Hydraulic fluid can cause<br>serious eye injury. |
