# Page 217 of 434

**Page 2-1-D19**

**ASD-STE100 Simplified Technical English**

**#<u>Non-STE example</u>**

**Word Approved meaning/** **<u>(part of speech) ALTERNATIVES STE EXAMPLE</u>**

Blank Page

# Page 218 of 434

**Page 2-1-D20**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**EACH (adj)**|Every one of two or<br>more objects or persons,<br>seen together as a group<br>but identified separately|MAKE SURE THAT THE<br>SWITCH IN EACH<br>PANEL IS SET TO<br>“OFF.”|
||**EACH (pron)**|Every one of two or<br>more objects or persons,<br>seen together as a group<br>but identified separately|INSTALL TWO<br>SPACERS, EACH<br>WITH A THICKNESS<br>OF 3.5 mm.|
||**EACH OTHER**<br>**(pron)**|Each of two or more in<br>reciprocal action or<br>relation|WHEN YOU REMOVE<br>THE PROBES, DO NOT<br>LET THEM TOUCH<br>EACH OTHER.|
||**early (adj) — UNNAPPROVED**|SHORT (adj)|IF THE FILTERS<br>BECOME CLOGGED<br>AFTER AN<br>UNUSUALLY SHORT<br>TIME, SEND THEM TO<br>THE LABORATORY<br>FOR ANALYSIS OF<br>THE CONTAMINATION.|If the filters clog at an<br>unusually early stage,<br>send them to the<br>laboratory for analysis of<br>the contamination.|
||**earth (n) — UNNAPPROVED**|GROUND (n)|MAKE SURE THAT THE<br>ELECTRICAL SUPPLY<br>GOES TO GROUND.|Make sure the electric<br>supply goes to earth.|
||**earth (v) — UNNAPPROVED**|GROUND (v)|MAKE SURE THAT THE<br>FUEL TANKS ARE<br>CORRECTLY<br>GROUNDED.|Make sure the fuel tanks<br>are correctly earthed.|
||**ease (n) — UNNAPPROVED**|EASILY (adv)|MAKE SURE THAT<br>YOU CAN MOVE THE<br>HANDLE EASILY.|The handle must move<br>with ease.|
|||EASY (adj)|MAKE SURE THAT IT<br>IS EASY TO MOVE THE<br>HANDLE.|The handle must move<br>with ease.|
||**ease (v) — UNNAPPROVED**|CAREFULLY REMOVE|CAREFULLY REMOVE<br>THE TRIM COVER<br>FROM THE ADHESIVE<br>TAPE.|Ease the trim cover from<br>the adhesive tape.|
|||CAREFULLY MOVE|CAREFULLY MOVE<br>THE PIPE INTO THE<br>CORRECT POSITION.|Ease the pipe into the<br>right position.|

**Issue 9 2025-01-15**

**Part 2 - Dictionary**

# Page 219 of 434

**Page 2-1-E1**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**EASILY (adv)**|Without difficulty|OXIDATION OCCURS<br>VERY EASILY.|
||**EASY (adj)**<br>**(EASIER,**<br>**EASIEST)**|Without difficulty|USE THE LEFT<br>OPENING FOR EASY<br>ACCESS.|
||**EAT (v),**<br>**EATS,**<br>**ATE**|To consume food|DO NOT EAT IN THE<br>WORK AREA.|
||No other verb<br>forms.|For safety<br>instructions, use:|
|||SWALLOW (v)|DO NOT SWALLOW<br>THE POTTING<br>COMPOUND.|Do not eat the potting<br>compound.|
||**EDGE (n)**|A line that is the<br>intersection of two<br>surfaces of a solid object|THE DISTANCE<br>BETWEEN THE EDGE<br>OF THE PANEL AND<br>THE PARTITION MUST<br>NOT BE MORE THAN<br>0.05 mm.|
||**EFFECT (n)**|The result of a cause|WHEN DUST MIXES<br>WITH OIL, IT HAS AN<br>ABRASIVE EFFECT.|
||**effect (v) — UNNAPPROVED**|DO (v)|DO THE TIGHTENING<br>PROCEDURE.|Effect the tightening<br>procedure.|
||**effective (adj) — UNNAPPROVED**|GOOD (adj)|THIS MATERIAL GIVES<br>GOOD PROTECTION<br>FROM CORROSION.|This material provides<br>effective protection from<br>corrosion.|
||**efficacious (adj) — UNNAPPROVED**|GOOD (adj)|THIS IS A GOOD<br>PROCEDURE TO<br>REMOVE PAINT.|This is an efficacious<br>way to remove paint.|
||**efficient (adj) — UNNAPPROVED**|SATISFACTORY (adj)|THE TRANSMISSION<br>CONTROL PROTOCOL<br>IS NOT SATISFACTORY<br>FOR THE<br>TRANSMISSION OF<br>INTERACTIVE<br>TRAFFIC.|<br>The Transmission<br>Control Protocol is not<br>efficient for the<br>transmission of<br>interactive traffic.|

# Page 220 of 434

**Page 2-1-E2**

**Part 2 - Dictionary**

**Issue 9 2025-01-15**

**ASD-STE100 Simplified Technical English**

||**Word**<br>**(part of speech)**|**Approved meaning/**<br>**ALTERNATIVES**|**STE EXAMPLE**|**Non-STE example**|
||---|---|---|---|
||**efficiently (adv) — UNNAPPROVED**|SATISFACTORILY (adv)|MAKE SURE THAT THE<br>UNIT OPERATES<br>SATISFACTORILY.|Make sure the unit<br>operates efficiently.|

||**efflux (n) — UNNAPPROVED**|EXHAUST (n)|MAKE SURE THAT<br>THERE ARE SAFETY<br>BARRIERS AROUND<br>THE ENGINE EXHAUST<br>AREA.|Ensure that there are<br>safety barriers around<br>the engine efflux area.

||**effort (n) — UNNAPPROVED**|FORCE (TN)|DO NOT TIGHTEN THE<br>BOLTS WITH TOO<br>MUCH FORCE.|Do not use too much<br>effort to tighten the bolts.|
|||TRY (v)|FIRST, TRY TO TURN<br>THE SHAFT WITH<br>YOUR HANDS.|First, make an effort to<br>turn the shaft with your<br>hands.|
||**either (adj) — UNNAPPROVED**|ONE (TN) OF THE TWO<br>(TN)|IF THERE IS MERCURY<br>CONTAMINATION IN<br>ONE OF THE TWO<br>COMPARTMENTS,<br>CLEAN THE AREA<br>IMMEDIATELY.|If there is mercury<br>spillage in either<br>compartment, clean the<br>area immediately.|
||**either (conj) — UNNAPPROVED**|OR (conj)|YOU CAN USE A RED<br>PEN OR A GREEN PEN.|You can use either a red<br>pen or a green pen.|
||**either (pron) — UNNAPPROVED**|ONE (TN) OR THE<br>OTHER|THERE ARE TWO<br>SOLENOIDS. YOU CAN<br>SUPPLY ELECTRICAL<br>POWER TO ONE OR<br>THE OTHER.|There are two solenoids.<br>You can supply electrical<br>power to either.|
||**EJECT (v),**<br>**EJECTS,**<br>**EJECTED,**<br>**EJECTED**|To move or to cause a<br>person or item to move<br>from an aircraft or<br>equipment with force|IF YOU PULL THE<br>EJECTION SEAT<br>HANDLE, THE SEAT<br>WILL EJECT.|

||**ejection (n) — UNNAPPROVED**|EJECT (v)|PUSH THE<br>APPLICABLE BUTTON<br>TO EJECT THE DISK<br>DRIVE.|Push the applicable<br>button for disk drive<br>ejection.

**Issue 9 2025-01-15**

**Part 2 - Dictionary**
