# Page 229–232 of 434

> **Source:** ASD-STE100 Issue 9, January 2025
> **Pages:** 229–232 of 434

# Page 229 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| exactly (adv) — UNNAPPROVED | ACCURATELY (adv) | PUT THE REPAIR SHEET ACCURATELY ON THE DAMAGED AREA. | Put the repair sheet exactly on the damaged area. |
| exactly (adv) — UNNAPPROVED | FULLY (adv) | FIND THE BOLT HOLE THAT ALIGNS FULLY WITH ONE OF THE OUTER SLOTS. | Find the bolt hole that aligns exactly with one of the outer slots. |
| exactly (adv) — UNNAPPROVED | CORRECT (adj) | THE SEAL MUST BE OF THE CORRECT DIMENSION FOR THE GROOVE. | The seal must fit the groove exactly. |
| examination (n) — UNNAPPROVED | EXAMINE (v) | EXAMINE THE BLADE FOR CRACKS. | Do an examination of the blades for cracks. |
| examination (n) — UNNAPPROVED | FIND (v) | IF YOU FIND CORROSION, REMOVE IT WITH THE SPECIFIED MATERIAL. | If the examination reveals corrosion, it must be removed with the specified material. |
| EXAMINE (v), EXAMINES, EXAMINED, EXAMINED | To look carefully at | EXAMINE THE COMPUTER FOR DAMAGE. | |
| EXAMPLE (n) | Something from a group which has the same qualities as the group | FIGURE 2 IS AN EXAMPLE OF A REPAIR PROCEDURE FOR A DAMAGED WEB. | |
| exceed (v) — UNNAPPROVED | MORE THAN | MAKE SURE THAT THE INDICATION IS NOT MORE THAN 400 KNOTS. | Ensure that the indication does not exceed 400 knots. |
| except (prep) — UNNAPPROVED | To replace this word, use a different construction. Be accurate. | KEEP ALL THE PARTS THAT ARE SERVICEABLE AND DISCARD THOSE THAT ARE BROKEN. | Keep all parts except those that are broken. |
| except (prep) — UNNAPPROVED | | REMOVE ALL SCREWS, BUT NOT THE ONE ON THE LEFT SIDE OF THE FLANGE. | Remove all screws except the one on the left side of the flange. |

# Page 230 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| exception (n) — UNNAPPROVED | To replace this word, use a different construction. Be accurate. | KEEP ALL THE PARTS THAT ARE SERVICEABLE AND DISCARD THOSE THAT ARE BROKEN. | Keep all parts with the exception of those that are broken. |
| exception (n) — UNNAPPROVED | | REMOVE ALL SCREWS, BUT NOT THE ONE ON THE LEFT SIDE OF THE FLANGE. | Remove all screws with the exception of the one on the left side of the flange. |
| exceptional (adj) — UNNAPPROVED | UNUSUAL (adj) | IF IT IS NECESSARY TO APPLY UNUSUAL FORCE TO OPEN THE UNIT, EXAMINE THE CONTROL LINKAGE. | If exceptional force is needed to open the unit, examine the control linkage. |
| exceptionally (adv) — UNNAPPROVED | UNUSUALLY (adv) | IF THE TIRE PRESSURE IS UNUSUALLY HIGH, OPEN THE VALVE. | If the tire pressure is exceptionally high, open the valve. |
| excess (adj) — UNNAPPROVED | TOO MUCH | DO NOT APPLY TOO MUCH ADHESIVE ON THE GASKET. | Do not apply excess adhesive on the gasket. |
| excess (adj) — UNNAPPROVED | MORE THAN | DO NOT PUT MORE THAN THE PERMITTED WEIGHT ON THE TROLLEY. | Do not put excess weight on the trolley. |
| excess (adj) — UNNAPPROVED | UNWANTED (adj) | REMOVE UNWANTED COMPOUND FROM THE GASKET. | Wipe excess compound from the gasket. |
| excess (adj) — UNNAPPROVED | NOT NECESSARY | REMOVE ALL REMAINING SEALANT THAT IS NOT NECESSARY. | Remove all the excess sealant. |
| excess (n) — UNNAPPROVED | TOO MUCH | IF YOU USE TOO MUCH PAINT, THE FINISH WILL BE UNSATISFACTORY. | An excess of paint will give a poor finish. |
| excess (n) — UNNAPPROVED | MORE THAN | THE HYDRAULIC PRESSURE MUST NOT BE MORE THAN 200 bar. | The hydraulic pressure must not be in excess of 200 bar. |

# Page 231 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| excessive (adj) — UNNAPPROVED | TOO MUCH | TOO MUCH FORCE CAN CAUSE DAMAGE TO THE SEAL. | Excessive force can damage the seal. |
| excessive (adj) — UNNAPPROVED | MORE THAN | IF THE PRESSURE IS MORE THAN 1000 kPa, STOP THE TEST. | If the pressure is excessive, stop the test. |
| excessively (adv) — UNNAPPROVED | TOO MUCH | BE CAREFUL NOT TO TURN THE INNER RACES TOO MUCH. | Be careful not to excessively rotate the inner races. |
| excessively (adv) — UNNAPPROVED | MORE THAN | IF THE OIL LEAKAGE IS MORE THAN FIVE DROPS A MINUTE, REJECT THE UNIT. | If oil leaks excessively, reject the unit. |
| exchange (v) — UNNAPPROVED | INTERCHANGE (v) | INTERCHANGE THE No. 1 AND No. 2 COMPUTERS. THEN DO THE TEST AGAIN. | Exchange the No. 1 and No. 2 computers. Then do the test again. |
| exchange (v) — UNNAPPROVED | REPLACE (v) | REPLACE THE O-RINGS. | Exchange the O-rings. |
| exclude (v) — UNNAPPROVED | NOT INCLUDE | THIS PROCEDURE DOES NOT INCLUDE THE REMOVAL OF THE PISTON. | This procedure excludes the removal of the piston. |
| exclude (v) — UNNAPPROVED | NOT USE | DO NOT USE OXYGEN. | Exclude the use of oxygen. |
| excluding (prep) — UNNAPPROVED | WITHOUT (prep) | THE WEIGHT OF THE UNIT, WITHOUT THE MOTOR, IS 10 kg. | The weight of the unit, excluding the motor, is 10 kg. |
| execute (v) — UNNAPPROVED | DO (v) | DO THESE STEPS. | Execute the following operations. |
| exempt (adj) — UNNAPPROVED | NO (adj) | MAKE SURE THAT THERE ARE NO METAL PARTICLES IN THE OIL. | Ensure the oil is exempt from metal particles. |
| exempt (adj) — UNNAPPROVED | NOT SHOW | MAKE SURE THAT THE SEALS DO NOT SHOW SIGNS OF DETERIORATION. | Ensure the seals are exempt from signs of deterioration. |

# Page 232 of 434

| Word (POS) | Approved meaning / ALTERNATIVES | STE example | Non-STE example |
|------------|--------------------------------|-------------|-----------------|
| exercise (v) — UNNAPPROVED | MAKE SURE (v) | MAKE SURE THAT YOU DO NOT GET ACID ON YOUR SKIN. | Exercise caution not to allow acid to contact skin. |
| exercise (v) — UNNAPPROVED | CAREFUL (adj) | BE CAREFUL THAT YOU DO NOT GET ACID ON YOUR SKIN. | Exercise caution not to allow acid to contact skin. |
| exert (v) — UNNAPPROVED | APPLY (v) | APPLY A LIGHT FORCE TO THE PEDALS. | Exert a light force on the pedals. |
| exert (v) — UNNAPPROVED | PUT (v) | PUT PRESSURE ON THE WOUND. | Exert pressure on the wound. |
| exhale (v) — UNNAPPROVED | BREATHE (v) | BREATHE INTO THE OXYGEN MASK. | Exhale into the oxygen mask. |
| EXHAUST (n) | The gas from an engine | THE EXHAUST FROM THE APU IS DANGEROUS. | |
| exhaust (v) — UNNAPPROVED | REMOVE (v) | USE A FAN TO REMOVE THE GASES. | Exhaust the gases using a fan. |
| exhaust (v) — UNNAPPROVED | DECREASE (v) | DECREASE THE NITROGEN PRESSURE TO 120 psi. | Exhaust the nitrogen pressure to 120 psi. |
| exhaust (v) — UNNAPPROVED | RELEASE (v) | RELEASE THE HYDRAULIC PRESSURE IN THE ACCUMULATOR. | Exhaust all the hydraulic pressure in the accumulator. |
| exhaustive (adj) — UNNAPPROVED | ALL (adj) | ALL THE TEST CONDITIONS ARE GIVEN IN PARAGRAPH 2.0. | An exhaustive list of test conditions is given at paragraph 2.0. |
| exhaustive (adj) — UNNAPPROVED | FULL (adj) | THIS IS NOT A FULL LIST. | The list is not exhaustive. |
| exist (v) — UNNAPPROVED | BE (v) | THERE ARE TWO DIFFERENT PROCEDURES FOR THIS REPAIR. | Two different procedures exist for this repair. |
| EXIT (n) | An opening to go out of a space | MAKE SURE THAT ALL THE EMERGENCY EXITS ARE CLEAR OF UNWANTED OBJECTS. | |
