# Jorne WL keyboard

This revision is based on the Corne V3 and is optimised for wireless use.

- LEDs are removed
- Supports MX/Alps/MX hotswap
- Uses MSK12C01 power switches (outward is off, inward is on)
- Has through-hole battery contacts (square is ground, circle is RAW)
- Battery contacts are wired through the power switch
- Pinky keys can be broken off