# Solar-Log Binding

The [Solar-Log Family](https://www.solar-log.com/en/) of monitoring devices for PV installations provide a MODBUS (TCP) and JSON-based API to access a number of internal data related to power generation and consumption. This binding implements access to the data via the JSON API.

## Usage

The Solar-Log is exposed as one Thing with a number of channels that can be used to read the values for different aspects of your Solar-Log installation.

## Configuration

You can either configure the Thing via the openHAB UI or via a `*.things` file, according to the following example:

`Thing solarlog:meter:pv "Solar-Log 300" @ "Utility Room" [ url="http://solar-log", refreshInterval=15 ]`

The parameters to be used are simple:

- `url` denotes the URL of your Solar-Log. If you have not changed anything, this defaults to `http://solar-log`.
- `refreshInterval` is the interval to fetch new data. Solar-Log updates its data every 15–60 seconds. `15` is the default value. Values lower than this will return the same result within the last 15-second period. Values lower than this cannot be set in the UI.

Currently, the binding does not support authenticated access to the Solar-Log JSON API (which was introduced with newer firmware). You must set the API access to `Open` in the Solar-Log configuration in order for the binding to work.

## Available channels

The following table is taken from the official manual and contains all available channels. If you want to manually define Items, this can for example be done as follows:

`Number solarlog_meter_pv_yieldday "Yield Day [% W]" (gSolarLog, gUtilityRoom) { channel="solarlog:meter:pv:yieldday" }`

| Data point         | Unit                                           | Index Description                                                          |
| ------------------ | ---------------------------------------------- | -------------------------------------------------------------------------- |
| lastupdate         | Time in the format dd.mm.yy; hh.minmin, secsec | 100 Time                                                                   |
| pac                | W                                              | 101 Total output PAC from all of the inverters and meters in inverter mode |
| pdc                | W                                              | 102 Total output PDC from all of the inverters                             |
| uac                | V                                              | 103 Average voltage UAC from the inverter                                  |
| udc                | V                                              | 104 Average voltage UDC from the inverter                                  |
| yieldday           | Wh                                             | 105 Total yield for the day from all of the inverters                      |
| yieldyesterday     | Wh                                             | 106 Total yield for the previous day from all of the inverters             |
| yieldmonth         | Wh                                             | 107 Total yield for the month from all of the inverters                    |
| yieldyear          | Wh                                             | 108 Total yield for the year from all of the inverters                     |
| yieldtotal         | Wh                                             | 109 Total yield from all of the inverters                                  |
| conspac            | W                                              | 110 Current total consumption PAC from all of the consumption meters       |
| consyieldday       | Wh                                             | 111 Total consumption from all of the consumption meters                   |
| consyieldyesterday | Wh                                             | 112 Total consumption for the previous day; all of the consumption meters  |
| consyieldmonth     | Wh                                             | 113 Total consumption for the month; all of the consumption meters         |
| consyieldyear      | Wh                                             | 114 Total consumption for the year; all of the consumption meters          |
| consyieldtotal     | Wh                                             | 115 Accumulated total consumption, all Consumption meter                   |
| totalpower         | Wp                                             | 116 Installed generator power                                              |

## More information

More information about the Solar-Log Data interfaces and the exact meaning of the various channels and the documentation of the JSON API can be found in the [Manual](https://www.solar-log.com/manuals/manuals/en_GB/SolarLog_Manual_3x_EN.pdf).
