## ⚡ Hardware Performance

Performance ℹ️

## 🌐 Grid Configuration

## ⚛️ Physics & Time

Estimate the global timestep size, based on the CFL condition at the finest level. The timestep is estimated using the formula `dt = CFL * dx / vmax` at the finest level, where `dx = (Lx / Nxbase) / 2levelmax`.
Box Size X (pc) ℹ️
vmax (km/s) ℹ️
CFL ℹ️
Enter Max Steps Manually
tstop
Max Steps

## 🖥️ Resources

Number of GPUs
SU per GPU-Hour

## Estimation Results

Total Active Cells -
Finest Resolution (dx) -
Time Step (dt) -
Total Steps -
Physical Runtime
0 Days
0 Hours
0 Seconds
Total Resource Cost
0 SU
0 GPU-Hours