Note that option order is significant: An option only 
applies to subsequent input files. So if you are using splitter, you probably 
want to put most of your options before '-c template.args'.


=== General options ===

;--help=topic
: 	Print help on the given topic.  If the topic is omitted then a
list of all the help topics is printed instead.

;--version 
: 	Output program version to stderr.

=== File options ===

;--input-file=filename
: 	Read input data from the give file.  This option (or just a
filename) may be given more than once. Make sure to set all 
wanted options before using this.

;--gmapsupp
: 	Create a gmapsupp.img file that can be uploaded to a Garmin or
placed in "/Garmin" in a microSD card (such as by mounting the
device in USB mass storage mode).  It can be used on ready
compiled img files, if the input files are not already compiled
then they are compiled first and then the gmapsupp is created.

;--gmapi
: 	Create a directory in the "gmapi" format required by Mac applications. Can 
also be used for Windows programs.

;-c filename
;--read-config=filename
: 	Each line of the named file contains a command option in the form
option=value or option:value.  The options are included as arguments of
the executed command as if they had been specified on the command line.
Lines beginning with a # character are ignored and can be used as
comments.  Any command line option can be specified, however the
leading '--' must be omitted.  The short option names with a single
'-' cannot be used, simply use the long name instead. 
<p>
;--output-dir=directory
:	Specify the directory in which all output files are written. It defaults
to the current working directory, i.e. the directory the command is
executed from.
<p>
;-n name
;--mapname=name
: 	Set the name of the map. Garmin maps are identified by an 8 digit
number.  The default is 63240001.  It is best to use a different
name if you are going to be making a map for others to use so
that it is unique and does not clash with others.
<p>
;--description=text
: 	Set the descriptive text for the map. This may be displayed in
QLandkarte, MapSource or on a GPS, where it is normally shown
below the family name. Example: --description="Germany, Denmark"
Please note: if you use splitter.jar to build a template.args file
and use -c template.args, then that file may contain a
"description" that will override this option for each single
tile. Make sure to set the description for the gmapsupp.img after
"-c template.args".
<p>
;--country-name=name
: 	Set the map's country name. The default is "COUNTRY".
<p>
;--country-abbr=abbreviation
: 	Set the map's abbreviated country name. The default is "ABC".
<p>
;--region-name=name
: 	Set the map's region name. By default, the map has no region name.
<p>
;--region-abbr=abbreviation
: 	Set the map's abbreviated region name. By default, the map has
no abbreviated region name.
<p>
=== Label options ===

;--code-page=number
:     Specify which international character set is to be used. Only 8 bit
character sets are supported so you have to specify which code page you
want to use.
It is entirely dependent on the device firmware which code pages are
supported.
<p>
;--latin1
: 	This is equivalent to --code-page=1252.
<p>
;--unicode
: 	This is equivalent to --code-page=65001. Note that some devices don't support 
Unicode maps produced by mkgmap.
<p>
;--lower-case
: 	Allow labels to contain lower case letters.  Note that many
Garmin devices are not able to display lower case letters at an angle.
<p>
=== Address search options ===
;--index
: 	Generate a global address search index. If the --gmapsupp option is
also given, then the index is generated within the resulting
gmapsupp.img file so that address search will work on a GPS
device.
<p>
If instead the --tdbfile option is given then the index consists
of two files named osmmap.mdx and osmmap_mdr.img which can be used
with MapSource.  The --overview-mapname option can be used to change
these names.  (For compatibility, you do not need the tdbfile
option if gmapsupp is not given).
<p>
If both the --gmapsupp and --tdbfile options are given alongside
the --index option, then both indexes will be created. Note that
this will require roughly twice as much memory.
<p>
If the map is sent to the device by MapSource, it will enable
find by name and address search on the GPS.

: The address fields are assigned by special mkgmap address
tags using the style file:

  mkgmap:country
  mkgmap:region
  mkgmap:city
  mkgmap:postal_code
  mkgmap:street
  mkgmap:housenumber
  mkgmap:phone
  (mkgmap:is_in - used by location-autofill=is_in)

: If the index is created from previously compiled .img files, then the
same code page and sorting options (e.g. --code-page, --latin1) must
be used as were used to compile the individual map tiles.

;--split-name-index
:     Index each part of a street name separately.
For example, if the street is "Aleksandra Gryglewskiego" then you will be able to
search for it as both "Aleksandra" and "Gryglewskiego".  It will also increase the
size of the index.  Useful in countries where searching for the first word in name
is not the right thing to do. Words following an opening bracket '(' are ignored. 
:	See also option road-name-config.  
<p>
;--road-name-config=filename
:	Provide the name of a file containing commonly used road name prefixes
and suffixes.
This option handles the problem that some countries have road names which 
often start or end with very similar words, e.g. in France the first word
is very often 'Rue', often followed by a preposition like 'de la' or 'des'.
This leads to rather long road names like 'Rue de la Concorde' where only
the word 'Concorde' is really interesting. In the USA, you often have names
like 'West Main Street' where only the word 'Main' is important.  
Garmin software has some tricks to handle this problem. It allows the use
of special characters in the road labels to mark the beginning and end of 
the important part. In combinarion with option split-name-index
only the words in the important part are indexed.
<p>
:There are two effects of this option:
::	- On the PC, when zooming out, the name 'Rue de la Concorde' is only
rendered as 'Concorde'.
::	- The index for road names only contains the important part of the name.
You can search for road name Conc to find road names like 'Rue de la Concorde'.
However, a search for 'Rue' will not list 'Rue de la Concorde' or
'Rue du Moulin'. It may list 'Rueben Brookins Road' if that is in the map.
Only MapSource shows a corresponding hint.
<p>
::	Another effect is that the index is smaller. 
:	See comments in the sample roadNameConfig.txt for further details.
<p>
;--mdr7-excl=name[,name...]
:	Specify words which should be omitted from the road index.
It was added before option road-name-config and is probably no longer needed.
:	Example usage: --x-mdr7-excl="Road, Street, Straße, Weg"
<p>
;--mdr7-del=name[,name...]
:	Use this option if your style adds strings to the labels of roads which you
want to see in the map but which should not appear in the result list
of a road name / address search. The list is used like this:
For each road label, mkgmap searches for the last blank. If one is found, it checks
if the word after it appears in the given list. If so, the word is removed
and the search is repeated. The remaining string is used to create the index.
:	Example: Assume your style adds surface attributes like 'pav.' or 'unp.' to a road
label. You can use --mdr7-del="pav.,unp." to remove these suffixes from the index.
<p>
;--poi-excl-index=poi[-poi][,poi[-poi]...]
:	By default, mkgmap indexes the following POI types with a non-empty label:
::	- 0x00 .. 0x0f (cities, sub type 0, type <= 0xf)
::	- 0x2axx..0x30xx (Food & Drink, Lodging, ...)
::	- 0x28xx (no category ?)
::	- 0x64xx .. 0x66xx (attractions)   
:	This option allows the exclusion of POI types from the index. 
The excluded types are not indexed, but may still be searchable on a device 
as some devices seem to ignore most of the index, e.g. an Oregon 600 with 
firmware 5.00 only seems to use it for city search.
If your device finds a POI name like 'Planet' when you search for 'Net',
it doesn't use the index because the index created by mkgmap cannot help for 
that search.
<p> 
:	So, this option may help when you care about the size of the index or the
memory that is needed to calculate it.    
The option expects a comma separated list of types or type ranges. A range is 
given with from-type-to-type, e.g. 0x6400-0x6405. First and last type are both 
excluded.  A range can span multiple types, e.g. 0x6400-0x661f.  
:	Examples for usage: 
::	- Assume your style adds a POI with type 0x2800 for each addr:housenumber.
It is not useful to index those numbers, so you can use --poi-excl-index=0x2800
to exclude this.
::	- For the mentioned Oregon you may use --poi-excl-index=0x2a00-0x661f
to reduce the index size.
<p>
;--bounds=directory|zipfile
:     Specify a directory or zip file containing the preprocessed bounds files. 
Bounds files in a zip file must be located in the zip file's root directory.
<p>
The preprocessed boundaries are used to add special tags to all elements 
(points, lines and polygons) containing the elements location information.
The style file can be used to assign the address tags mkgmap:country,
mkgmap:region etc. using these values.
<p>
The following special tags are added:          
<pre>
  mkgmap:admin_level2 : Name of the admin_level=2 boundary 
  mkgmap:admin_level3 : Name of the admin_level=3 boundary
  ..
  mkgmap:admin_level11
  mkgmap:postcode : the postal_code value
</pre>
Preprocessed bounds can be created with the following command:
<pre>
  java -cp mkgmap.jar 
    uk.me.parabola.mkgmap.reader.osm.boundary.BoundaryPreprocessor
    <inputfile> <boundsdir>
</pre>
The input file must contain the boundaries that should be preprocessed. 
It can have OSM, PBF or O5M file format. It is recommended that it 
contains the boundary data only to avoid very high memory usage.
The boundsdir gives the directory where the processed files are stored.
This directory can be used as --bounds parameter with mkgmap.               
<p>
;--location-autofill=[option1,[option2]]
: 	Controls how the address fields for country, region, city and zip info 
are gathered automatically if the fields are not set by using the special 
mkgmap address tags (e.g. mkgmap:city - see option index).
Warning: automatic assignment of address fields is somehow a best guess.
:;is_in
::     The is_in tag is analyzed for country and region information.
<p>
:;nearest
::	The city/hamlet points that are closest to the element are used 
to assign the missing address fields. Beware that cities located 
in the same tile are used only. So the results close to a tile 
border have less quality.  

;--housenumbers
:   Enables house number search for OSM input files. 
All nodes and polygons having addr:housenumber set are matched 
to streets. A match between a house number element and a street is created if
the street is located within a radius of 150m and the addr:street tag value of 
the house number element equals the mgkmap:street tag value of the street. 
The mkgmap:street tag must be added to the street in the style file.
For optimal results, the tags mkgmap:city and mkgmap:postal_code should be
set for the housenumber element. If a street connects two or more cities
this allows to find all addresses along the road, even they have the same
number.
: Example for given street name: 
:: Node -  addr:street=Main Street addr:housenumber=2
:: Way 1 - name=Main Street
:: Way 2 - name=Main Street, mkgmap:street=Main Street
:: Way 3 - mkgmap:street=Mainstreet
:: Way 4 - name=Main Street [A504]
: The node matches to Way 2. It has mkgmap:street set with a value equal to
the addr:street tag value of the house number node.
<p>
If the street is not given with addr:housenumber, mkgmap uses heuristics
to find the best match.

=== Overview map options ===
;--overview-mapname=name
: 	If --tdbfile is enabled, this gives the name of the overview
.img and .tdb files. The default map name is osmmap.
<p>
;--overview-mapnumber=8 digit number
: 	If --tdbfile is enabled, this gives the internal 8 digit
number used in the overview map and tdb file.  The default
number is 63240000.
<p>
;--overview-levels=level:resolution[,level:resolution...]
:   Like levels, specifies additional levels that are to be written to the
overview map. Counting of the levels should continue. Up to 8 additional 
levels may be specified, but the lowest usable resolution with MapSource 
seems to be 11. The hard coded default is empty.
:	See also option --overview-dem-dist.      
<p>
;--remove-ovm-work-files
:   If overview-levels is used, mkgmap creates one additional file 
with the prefix ovm_ for each map (*.img) file. 
These files are used to create the overview map.
With option --remove-ovm-work-files=true the files are removed 
after the overview map was created. The default is to keep the files.  
<p>
=== Style options ===
;--style-file=filename
: 	Specify an external file to obtain the style from.  "file" can
be a directory containing files such as info, lines, options
(see resources/styles/default for an example).  The directory
path must be absolute or relative to the current working
directory when mkgmap is invoked.
<p>
The file can be a zip file containing the files instead of a
directory.
<p>
The files can be at the top level or contained in a folder within
the zip file.  If the zip file contains more than one top level
folder then each folder is the name of a style that can be selected
with the --style option.
<p>
The argument can also be a URL that specifies the location of a
style file.
<p>
;--style=name
: 	Specify a style name. Must be used if --style-file points to a 
directory or zip file containing multiple styles. If --style-file 
is not used, it selects one of the built-in styles. 
<p>
;--style-option=tag[=value][;tag[=value]...]
: 	Provide a semicolon separated list of tags which can be used in the style.
The intended use is to make a single style more flexible, e.g.
you may want to use a slightly different set of rules for a map of
a whole continent. The tags given will be prefixed with "mkgmap:option:".
If no value is provided the default "true" is used.  
This option allows to use rules like
mkgmap:option:light=true & landuse=farmland {remove landuse}
Example: -- style-option=light;routing=car
will add the tags mkgmap:option:light=true and mkgmap:option:routing=car
to each element before style processing happens. 
<p>                                                            
;--list-styles
: 	List the available styles. If this option is preceded by a style-file
option then it lists the styles available within that file.
<p>
;--check-styles
: 	Perform some checks on the available styles. If this option is 
preceded by a style-file option then it checks the styles 
available within that file. If it is also preceded by the style
option it will only check that style.
<p>
;--levels=level:resolution[,level:resolution...]
: 	Change the way that the levels on the map correspond to the zoom
levels in the device. See customisation help. The hard coded default is:
"0:24, 1:22, 2:20, 3:18, 4:16", although each style can have
its own default. The default style for example overwrites it with
"0:24, 1:22, 2:20, 3:18". Up to 8 levels may be specified.
<p>
;--name-tag-list=tag[,tag...]
: 	Specify the tag that will be used to supply the name.  Useful for
language variations.  You can supply a list of tags and the first one
found will be used.  e.g. --name-tag-list=name:en,int_name,name
<p>
===Product description options===

;--family-id=integer
: 	This is an integer that identifies a family of products.
Range: [1..9999]
Mkgmap default: 6324
<p>
;--family-name=name
: 	If you build several maps, this option describes the
family name of all of your maps. Garmin will display this
in the map selection screen.
<p>
Example: --family-name="OpenStreetmap mkgmap XL 2019"
<p>
;--product-id=integer
: 	This is an integer that identifies a product within a family.
It is often just 1, which is the default.
<p>
;--product-version=integer
: 	The version of the product. Default value is 100 which means version 1.00.
<p>
;--series-name=name
: 	This name will be displayed in MapSource in the map selection
drop-down. The default is "OSM map".
<p>
;--area-name=name
:   Area name is displayed on Garmin units (or at least on eTrex) as the second 
part of the mapname in the list of the individual maps.
<p>
;--copyright-message=text
: 	Specify a copyright message for files that do not contain one.
<p>
;--copyright-file=filename
: 	Specify copyright messages from a file.
Note that the first copyright message is not displayed on a device, but is 
shown in BaseCamp. The copyright file must include at least two lines and
be UTF-8 encoded. The following symbols will be substituted by mkgmap:
$MKGMAP_VERSION$, $JAVA_VERSION$, $YEAR$, $LONG_DATE$, $SHORT_DATE$ and $TIME$.
Time and date substitutions use the local date and time formats.
<p>
;--license-file=filename
: 	Specify a file which content will be added as license.
The license file must be UTF-8 encoded.
The following symbols will be substituted by mkgmap:
$MKGMAP_VERSION$, $JAVA_VERSION$, $YEAR$, $LONG_DATE$, $SHORT_DATE$ and $TIME$.
Time and date substitutions use the local date and time formats.
All entries of all maps will be merged in the overview map.
<p>
=== Optimization options ===

;--reduce-point-density=NUM
: 	Simplifies the ways with the Douglas Peucker algorithm.
NUM is the maximal allowed error distance, by which the resulting
way may differ from the original one.
This distance gets shifted with lower zoom levels. 
Recommended setting is 4, this should lead to only small differences
(Default is 2.6, which should lead to invisible changes)
<p>
;--reduce-point-density-polygon=NUM
: 	Allows you to set the maximal allowed error distance for the DP algorithm
to be applied against polygons. Recommended setting is 8.
<p>
;--merge-lines
: 	Try to merge lines. This helps the simplify filter to straighten out
longer chunks at lower zoom levels. Decreases file size more.
Increases paint speed at low zoom levels.
Default is enabled, use --no-merge-lines to disable.
<p>
;--min-size-polygon=NUM
:   Removes all polygons smaller than NUM from the map.
This reduces map size and speeds up redrawing of maps. 
Recommended value is 8 to 15, default is 8.
:	See also polygon-size-limits.
<p>
;--polygon-size-limits=resolution:value[,resolution:value...]
:   Allows you to specify different min-size-polygon values for each resolution.
Sample:  
--polygon-size-limits="24:12, 18:10, 16:8, 14:4, 12:2, 11:0"
If a resolution is not given, mkgmap uses the value for the next higher 
one. For the given sample, resolutions 19 to 24 will use value 12,
resolution 17 and 18 will use 10, and so on.
Value 0 means to not apply the size filter. 
Note that in resolution 24 the filter is not used.
The following options are equivalent:
 --min-size-polygon=12
 --polygon-size-limits=24:12
 --polygon-size-limits=24:0,23:12
 --polygon-size-limits=24:0,23:12,22:12,21:12,16:12
<p>
=== Hill Shading (DEM) options ===
:   Hill Shading is rendered by PC programs (MapSource or BaseCamp) or GPS devices 
when the map includes a Digital Elevation Model (DEM). Use the following options 
to add a DEM to the map and control its characteristics. DEM creation requires 
files containing height information for the area covered by the map, the so 
called hgt files, which typically cover 1 degree latitude * 1 degree longitude 
and are named by the coordinates of their bottom left corner (eg. N53E009). They 
contain height information in a grid of points. Typical hgt files contain either 
1'' or 3'' data. 3'' files have 1201 * 1201 points, which gives 
2 * 1201 * 1201 = 2.884.802 bytes. 1'' files have 3601 * 3601 points, which gives 
2 * 3601 * 3601 = 25.934.402 bytes. Other files are supported as long as the 
formular sqrt(size/2) gives an integer value.
<p>
;--dem=path[,path...]
:   The option expects a comma separated list of paths to directories or zip 
files containing *.hgt files. Directories are searched for *.hgt files 
and also for *.hgt.zip and *.zip files
:   The list is searched in the given order, so if you want to use 1'' files 
make sure that they are found first. There are different sources for *.hgt 
files, some have so called voids which are areas without data. Those should be 
avoided.
<p>
;--dem-dists=number[,number...]
:   If given, the option specifies the resolution(s) or zoom level for the DEM 
data. If not given, mkgmap tries to determine a reasonable value based on the 
resolution found in the *.hgt files. For desktop programs like MapSource or 
Basecamp you only need one zoom level, for GPS devices you need one for each 
resolution given with the --levels option. The actual values are given as 
distance between two DEM points and should be a multiple or submultiple of the 
distance between two points in the hgt file, that is 3314 for 1'' and 9942 for 
3''. Higher distances mean lower resolution and thus fewer bytes in the map. 
Reasonable values for the highest resolution should not be much smaller than 
50% hgt resolution, that is somewhere between 1648 and 5520 for 1'' hgt input 
files (3312 is often used), and 5520 to 9942 for 3'' hgt input files.
:	Example which should work with levels="0:24, 1:22, 2:20, 3:18":
:	--dem-dists=3312,13248,26512,53024
:	This was found in a Garmin Demo map for transalpin data created 2009.
<p>
;--dem-interpolation=auto|bicubic|bilinear
:   Use this option to specify the method that is used to interpolate data from 
hgt raster to the DEM raster. The value bicubic gives the highest precision 
but is slower, bilinear is faster but less precise, it tends to smooth the 
profile and thus also reduces DEM size compared to bicubic. The value auto 
means that bicubic is used where is seems appropriate according to hgt 
resolution and dem-dist value, else bilinear is used. The default is auto.
<p>
;--dem-poly=filename
:   If given, the filename should point to a *.poly file in osmosis polygon 
file format. The polygon described in the file is used to determine the area
for which DEM data should be added to the map. If not given, the DEM data will
cover the full tile area.
<p>   
;--overview-dem-dist=integer
:   If given, the option specifies the resolution(s) for the DEM data in the
overview map. If not given or 0, mkgmap will not add DEM to the overview map.
Reasonable values depend on the size of the area and the lowest resolution
used for the single tiles, good compromises are somewhere between 55000 
and 276160.  
<p>
=== Miscellaneous options ===

;--max-jobs[=integer]
: 	Specify the number of threads to be used for concurrent processing.
Increasing max-jobs will reduce the execution time, providing sufficient
memory is available and the value is not greater than the number of cores
in the CPU. If no value is specified, the limit is set to the number of CPU
cores. The default is for the limit to be automatically set to a reasonable
value based on the amount of memory allocated to the Java runtime and the
amount used in processing the first tile. To optimise mkgmap to use all
available CPU cores, you may need to use the Java -Xmx option to increase
the amount of available heap storage.
<p>
;--keep-going
: 	Don't quit whole application if an exception occurs while
processing a map - continue to process the other maps.
<p>
;--block-size=integer
: 	Changes the block size that is used in the generated map. This
option is not usually needed, but sometimes an error message
will ask you to try a value for this option.
<p>     
;--net
: 	Tells mkgmap to write NET data, which is needed for address search
and routing. Use this option if you want full address search, but do
not need a map that supports routing.
<p>                                                            
;--route
: 	Tells mkgmap to write NET and NOD data, which are needed in maps 
that support routing. If you specify this option, you do not need
to specify --net.
<p>
;--add-boundary-nodes-at-admin-boundaries=NUM	
: 	This option controls how mkgmap calculates special routing nodes which
are needed by Garmin software to allow routing between different map tiles.
These nodes are written to section 3 and 4 in the NOD file.
When a road crosses the tile boundary (bbox), the road is split at this
point and such a special node is written. This allows routing between
one set of tiles produced by splitter.jar. However, if you create a map
from different sets of tiles, those tiles are likely to overlap.
For the overlapping tiles, none of the entries in NOD3 match and thus
routing across tile border doesn't work when the route is not fully
covered by one of the tiles.
The option tells mkgmap to add special nodes whereever a road touches or
crosses an administratve boundary. The NUM parameter specifies a filter
for the admin_level. Boundaries with a higher admin_level value are ignored.
The default value is 2 (country borders). Another reasonable value might
be 4. A value less or equal to 0 tells mkgmap to ignore intersections at 
administrative boundaries.
<p>	
;--drive-on=left|right|detect|detect,left|detect,right
: 	Explicitly specify which side of the road vehicles are
expected to drive on. 
If the first option is detect, the program tries 
to find out the proper flag. If that detection
fails, the second value is used (or right if none is given).
With OSM data as input, the detection tries to find out  
the country each road is in and compares the number
of drive-on-left roads with the rest.
Use the --bounds option to make sure that the detection 
finds the correct country. 
<p>

;--check-roundabouts
: 	Check that roundabouts have the expected direction (clockwise
when vehicles drive on the left). Roundabouts that are complete
loops and have the wrong direction are reversed. Also checks
that the roundabouts do not fork or overlap other roundabouts
and that no more than one connecting highway joins at each node.
<p>
;--check-roundabout-flares
: 	Check that roundabout flare roads point in the correct
direction, are one-way and don't extend too far.
<p>
;--max-flare-length-ratio=NUM
: 	When checking flare roads, ignore roads whose length is
greater than NUM (an integer) times the distance between the
nodes on the roundabout that the flare roads connect to. Using
this option with a value of at least 5 will cut down the
number of legitimate roads that are flagged as flare road
problems. Default value is 0 (disabled) because it's not a
completely reliable heuristic.
<p>
;--ignore-turn-restrictions
: 	When reading OSM files, ignore any "restriction" relations.
<p>
;--ignore-osm-bounds
: 	When reading OSM files, ignore any "bounds" elements.
With this option selected generate-sea sometimes works better,
but routing across tiles will not work.
<p>
;--preserve-element-order
: 	Process the map elements (nodes, ways, relations) in the order
in which they appear in the OSM input. Without this option,
the order in which the elements are processed is not defined.
<p>
Optional BITMASK (default value 3) allows you to specify which
adjustments are to be made (where necessary):
<p>
:* 1 = increase angle between side road and outgoing main road
:* 2 = increase angle between side road and incoming main road
<p>
;--cycle-map
: 	Tells mkgmap that the map is for cyclists. This assumes that
different vehicles are different kinds of bicycles, e.g. a way
with mkgmap:car=yes and mkgmap:bicycle=no may be a road that is 
good for racing bikes, but not for other cyclists.
This allows the optimisation of sharp angles at junctions of those roads. 
Don't use with the default style as that is a general style!
<p>
;--report-similar-arcs
: 	Issue a warning when more than one arc connects two nodes and
the ways that the arcs are derived from contain identical
points. It doesn't make sense to use this option at the same
time as using the cycleway creating options.
<p>
;--report-dead-ends=LEVEL
: 	Set the dead end road warning level. The value of LEVEL (which
defaults to 1 if this option is not specified) determines
those roads to report: 0 = none, 1 = multiple one-way roads
that join together but go nowhere, 2 = individual one-way roads
that go nowhere.
<p>
;--add-pois-to-lines
: 	Generate POIs for lines. For each line (must not be closed) POIs are
created at several points of the line. Each POI is tagged with the
same tags like the line and additional tags added by mkgmap:
mkgmap:line2poi=true and tag mkgmap:line2poitype having
the following values:
:* start  - The first point of the line
:* end    - The last point of the line
:* inner  - Each point of the line except the first and the last 
:* mid    - The middle point
;--add-pois-to-areas
: 	Generate a POI for each polygon and multipolygon. The POIs are created 
after the relation style but before the other styles are applied. Each 
POI is tagged with the same tags of 
the area/multipolygon. Additionally the tag mkgmap:area2poi=true is 
set so that it is possible to use that information in the points style
file. Artifical polygons created by multipolyon processing are not used.
The POIs are created at the following positions (first rule that applies):
:;polygons: 
::First rule that applies of
::* the first node tagged with a tag defined by the pois-to-areas-placement option
::* the centre point  
:; multipolygons:
::First rule that applies of
::* the node with role=label
::* the centre point of the biggest area
;--pois-to-areas-placement=tag=value[;tag=value...]
:     A POI is placed at the first node of the polygon tagged with the first tag/value
pair. If none of the nodes are tagged with the first tag-value pair the first node
tagged with the second tag-value pair is used and so on. If none of the tag-value pairs
matches or the taglist is empty, the centre of the polygon is used.
It is possible to define wildcards for tag values like entrance=*.
<p>Default: entrance=main;entrance=yes;building=entrance
<p>
;--precomp-sea=directory|zipfile
:     Defines the directory or a zip file that contains precompiled sea tiles. 
Sea files in a zip file must be located in the zip file's root directory or in 
a sub directory sea. When this option is defined all natural=coastline tags 
from the input OSM tiles are removed and the precompiled data is used instead. 
This option can be combined with the generate-sea options multipolygon, polygons 
and land-tag. The coastlinefile option is ignored if precomp-sea is set.      
<p>
;--coastlinefile=filename[,filename...]
: 	Defines a comma separated list of files that contain coastline 
data. The coastline data from the input files is removed if 
this option is set. Files must have OSM or PBF fileformat.	
<p>
;--generate-sea[=ValueList]
: 	Generate sea polygons. ValueList is an optional comma
separated list of values:
<p>
:;multipolygon
:: generate the sea using a multipolygon (the default behaviour so this really doesn't need to be specified).

:;polygons | no-mp
:: don't generate the sea using a multipolygon - instead,
generate a background sea polygon plus individual land
polygons with tag natural=land. This requires a
suitable land polygon type to be defined in the style
file (suggested type is 0x010100) and the polygon must
be defined in the TYP file as having a higher drawing
level than the sea polygon type.

:;no-sea-sectors
:: disable the generation of "sea sectors" when the
coastline fails to reach the tile's boundary.
:;extend-sea-sectors
:: same as no-sea-sectors. Additional adds a point so coastline reaches the nearest tile boundary.

:;land-tag=TAG=VAL
:: tag to use for land polygons (default natural=land).
:;close-gaps=NUM
:: close gaps in coastline that are less than this distance (metres)

:;floodblocker 
:: enable the flood blocker that prevents a flooding of
land by checking if the sea polygons contain streets
(works only with multipolygon processing)		

:;fbgap=NUM           
:: flood blocker gap in metre (default 40)
points that are closer to the sea polygon do not block 
:;fbthres=NUM
:: at least so many highway points must be contained in 
a sea polygon so that it may be removed by the flood
blocker (default 20)

:; fbratio=NUM
:: only sea polygons with a higher ratio 
(highway points * 100000 / polygon size) are removed 
(default 0.5)

:; fbdebug
:: switches on the debugging of the flood blocker
generates GPX files for each polygon checked by
the flood blocker

;--make-poi-index
:	Generate a POI index in each map tile. Probably not used by modern devices,
but still supported.
<p>
;--nsis
: 	Write a .nsi file that can be used with the Nullsoft Scriptable Install System
(NSIS) to create a Windows Mapsource Installer.
<p>
;--make-opposite-cycleways
: 	Some one-way streets allow bicycle traffic in the reverse
direction and this option makes a way with the same points as
the original that allows bicycle traffic (in both directions).
;--link-pois-to-ways
:     This option may copy some specific attributes of a POI 
to a small part of the way the POI is located on. This can be used
to let barriers block a way or to lower the calculated speed
around traffic signals.
POIs with the tags highway=* (e.g. highway=traffic_signals)  
or barrier=* (e.g. barrier=cycle_barrier) are supported.
The style developer must add at least one of the access tags
(mkgmap:foot, mkgmap:car etc.), mkgmap:road-speed and/or 
mkgmap:road-class to the POI. 
The access tags are ignored if they have no effect for the way, 
else a route restriction is added at the POI so that only 
allowed vehicles are routed through it. 
The tags mkgmap:road-speed and/or mkgmap:road-class are 
applied to a small part of the way around the POI, typically
to the next junction or a length of ~25 m. The tags
are ignored for pedestrian-only ways.      
<p>
;--process-destination
: 	Splits all motorway_link, trunk_link, primary_link, secondary_link,
and tertiary_link ways tagged with destination into two or three parts where 
the second part is additionally tagged with mkgmap:dest_hint=*.
The code checks for the tags destination, destination:lanes, 
destination:street and some variants with :forward/:backward like
destination:forward or destination:lanes:backward. If a value for
destination is found, the special tag mkgmap:dest_hint is set to  
it  and the way is split.
This happens before the style rules are processed.
This allows to use any routable Garmin type (except 0x08 and 0x09)
for that part so that the Garmin device tells the name of
this part as hint which destination to follow.
:	See also --process-exits.
<p>
;--process-exits
:     Usual Garmin devices do not tell the name of the exit on motorways 
while routing with mkgmap created maps. This option splits each
motorway_link, trunk_link, primary_link, secondary_link, and 
tertiary_link way into three parts. 
All parts are tagged with the original tags of the link. 
Additionally the middle part is tagged with the following tags:
<pre>
  mkgmap:exit_hint=true
  mkgmap:exit_hint_ref=<ref tag value of the exit>
  mkgmap:exit_hint_name=<name tag value of the exit>
  mkgmap:exit_hint_exit_to=<exit_to tag value of the exit>
</pre>
Adding a rule checking the mkgmap:exit_hint=true makes it possible
to use any routable Garmin type (except 0x08 and 0x09) for the middle 
part so that the Garmin device tells the name of this middle part as 
hint where to leave the motorway/trunk.
The first part must have type 0x08 or 0x09 so that Garmin uses the hint. 

;--delete-tags-file=filename
: 	Names a file that should contain one or more lines of the form
TAG=VALUE or TAG=*. Blank lines and lines that start with
a # or ; are ignored. All tag/value pairs in the OSM input are
compared with these patterns and those that match are deleted.
<p>
;--ignore-fixme-values
: 	Ignore all tags for which the value matches the pattern "(?i)fix[ _]?+me".	
<p>
;--tdbfile
: 	Write files that are essential to running with MapSource, a .tdb file and
an overview map.
<p>
;--show-profiles=1
: 	Sets a flag in tdb file. The meaning depends on the availability of DEM 
data (see "Hill Shading (DEM) options"). 
: 	Without DEM data the flag enables profile calculation in MapSource or 
Basecamp based on information from contour lines. 
: 	If DEM data is available the profile is calculated with that 
information and the flag only changes the status line to show the height when 
you hover over an area with valid DEM data. 
: 	The default is show-profiles=0.
<p>
;--transparent
: 	Make the map transparent, so that if two maps covering the same area are
loaded, you can see through this map to see details from the other map too.
Typically used for maps containing just contour lines. See --draw-priority
as well.
<p>
;--draw-priority=integer
: 	When two maps cover the same area and both are enabled in the device, this
option controls the order in which they are drawn in and therefore which map
is on top.  Higher priorities are drawn "on top" of lower priorities.
The map drawn on top must be transparent for the one underneath to be seen.
The default value is 25.
<p>
;--custom
: 	Write a different TRE header. With this option, mkgmap writes the bytes
0x170401 instead of the default 0x110301 at offset 43. Useful for marine maps.	
<p>
;--hide-gmapsupp-on-pc
: 	Set a bit in the gmapsupp.img that tells PC software that the file is
already installed on the PC and therefore there is no need to read it 
from the device.
<p>
;--poi-address
: 	Enable address / phone information to POIs. Address info is
read according to the "Karlsruhe" tagging schema. Automatic
filling of missing information could be enabled using the
"location-autofill" option.
Default is enabled, use --no-poi-address to disable.
<p>
;--verbose
: 	Makes some operations more verbose. Mostly used with --list-styles.
<p>
;--order-by-decreasing-area
:	Puts area/polygons into the map in decreasing size order, so
that smaller features are rendered over larger ones
(assuming _drawOrder is equal).
The tag mkgmap:drawLevel can be used to override the
natural area of a polygon, so forcing changes to the rendering order. 

=== Deprecated and Obsolete Options ===
<p>
;--drive-on-left
;--drive-on-right
: 	Deprecated; use drive-on instead.
The options are translated to drive-on=left|right. 
<p>
;--make-all-cycleways
:   Deprecated; use --make-opposite-cycleways instead. Former meaning: 
<div class=preserve><nowiki>
Turn on all of the options that make cycleways.
</nowiki></div>
<p>
;--charset=name
: 	Obsolete; use --code-page instead.
<p>
;--map-features=filename
: 	Obsolete; use --style-file instead.
<p>
;--ignore-maxspeeds
: 	Obsolete; former usage:
When reading OSM files, ignore any "maxspeed" tags.
<p>
;--ignore-builtin-relations
: 	Obsolete; former usage:
When reading OSM files, skip the built-in processing of
relations. This speeds up the processing non-routable map
layers that do not contain multipolygons. This implies
--ignore-turn-restrictions.
<p>
;--road-name-pois[=GarminCode]
: 	Obsolete; former usage:
Generate a POI for each named road. By default, the POIs'
Garmin type code is 0x640a. If desired, a different type code
can be specified with this option.  This is a workaround for not
being able to search for roads.
0x2f15: a blue dot in the middle of the road, and if you select,
or 'hover' over it, the street name appears.
<p>
;--make-cycleways
:   Obsolete; former meaning:
<div class=preserve><nowiki>
Some streets have a separate cycleway track/lane just for
bicycle traffic and this option makes a way with the same
points as the original that allows bicycle traffic. Also,
bicycle traffic is prohibited from using the original way
(unless that way's bicycle access has been defined).
</nowiki></div>