# SDL_HINT_LINUX_DIGITAL_HATS

A variable controlling whether joysticks on Linux will always treat 'hat' axis inputs (ABS_HAT0X - ABS_HAT3Y) as 8-way digital hats without checking whether they may be analog.

## Header File

Defined in [SDL_hints.h](https://github.com/libsdl-org/SDL/blob/SDL2/include/SDL_hints.h)

## Syntax

```c
#define SDL_HINT_LINUX_DIGITAL_HATS "SDL_LINUX_DIGITAL_HATS"
```

## Remarks

This variable can be set to the following values:

- "0": Only map hat axis inputs to digital hat outputs if the input axes
  appear to actually be digital (the default)
- "1": Always handle the input axes numbered ABS_HAT0X to ABS_HAT3Y as
  digital hats

----
[CategoryAPI](CategoryAPI), [CategoryAPIMacro](CategoryAPIMacro), [CategoryHints](CategoryHints)

