U9 footprint doesn't match whatever part I ordered for it.
The footprint used by U7 will work for U9.

U2 & U3 (RS485) pads are too far spaced from each other... the LTC chip has to 'stretch' across the pads.


...
Verified fixed on RevB