Resistor R5 needs to move left, for additional clearance from Arduino MEGA USB connector.

Workaround: Manually verify no short, then apply conformal coating.

/////////////////////////////////////////////////////////////////////////////////

Solution:
Moved R5 below D4

Done