Move grid charger harness holes down so they don't hit the IMA bay's top plastic rib.

/////////////////////////////////////////////////////////////////////////////////

Solution:
Move grid charger holes down as far as possible.