RevC Assembly Notes:
R130 should be 1206
R353 silkscreen
Move middle (rear) temp connector so it doesn't hit ribbon cable's locking tab
Move beeper and Cherry switch up ~1mm
Silkscreen text overlaps near (right of) C95.

/////////////////////////////////////////////////////////////////////////////////

Solution:
R130 changed to 1206
Fixed silkscreen issues
Didn't move temp connector, beeper, or cherry switch

Done