Simplest method to prevent backfeeding 5V into USB is to remove FET "T1" between  USBVCC & +5V (on Arduino).

Still need to verify this still allows USB to work... it should, but should test it.

...
Deferred to RevB V&V for solution.