# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Stop

Stops execution on the target. A break event will be sent when the target is stopped.

Table 108. Stop command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_STOP | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Level | 1 byte | 0x01: stop immediately 0x02: stop at next symbol (deprecated)

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |