# Atmel EDBG-based Tools Protocols
Serial trace commands

Sidebar | Prev | Up | Next

### Get status

Reads out status information.

Table 23. Get status

Field | Size | Description
--- | --- | ---
SERIAL_TRACE | 1 byte | 0x87
GET_STATUS | 1 byte | 0x09

Response:

Table 24. Get status response

Field | Size | Description
--- | --- | ---
SERIAL_TRACE | 1 byte | 0x87
GET_STATUS | 1 byte | 0x09
STATUS | 1 byte | Status encoding Bit 7: overrun error (buffer not read fast enough) Bit 6: receive error (framing or baud rate error) Bit 1: receive disabled (receiver has been disabled)
BYTES | 2 byte, MSB first | Number of bytes available to read

Prev | Up | Next
| Home |