# Atmel EDBG-based Tools Protocols
Hints and tips:

Sidebar | Prev | Up | Next

### Flow control

The following flow control functions are supported:

- RESET: resets the target and stops it at the reset vector address.

- STOP: stops the target at the next instruction (low-level stop).

- RUN: puts the target into run mode unconditionally.

- STEP: performs a single instruction step on the target. Instruction-level stepping must be used repetitively to perform statement-level stepping.

- PC read/write: reads and adjusts the program counter

- Erase: performs an erase on the target. To be used in programming mode only.

- CRC: performs a CRC calculation on the target (XMEGA only).

- Memory Read and Write: provides access to memory areas in programming mode and when stopped in a debug session. Rules are provided per memory-type in the communication protocol specification.

- Hardware breakpoint set / clear: Provides access to add and remove hardware breakpoints. Resources are family / OCD specific.

- Software breakpoint set / clear: Inserts and removed software breakpoints from a control table in the tool. On the next flow control command executed, the flash memory on the target is updated.

- Software breakpoints clear all: Immediately restores all software breakpoints to their original values.

All flow control functions will return a success or failure based on the ability to perform that command. The target state is assumed to be running until a BREAK event is received, indicating the transition to a stopped state.

Prev | Up | Next
| Home |