# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Erase

Performs an erase on the target. Functionality varies according to target family.

Table 117. Erase command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_ERASE | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Mode | 1 byte | 0x00 = Chip erase 0x01 = Application erase 0x02 = Boot section erase 0x03 = EEPROM erase 0x04 = Applicaton page erase 0x05 = Boot page erase 0x06 = EEPROM page erase 0x07 = User signature erase
Address | 4 bytes | Start address of section to erase (byte address)

Note: tinyAVR and megaAVR (debugWIRE) does not support any erase functionlity - flash pages are erased automatically before programming.

Note: megaAVR (JTAG) support only chip erase mode - Mode and Address parameters are ignored.

Note: AVR XMEGA requires Mode and Address parameters.

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |