# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Memory Read masked

Reads memory on the target, skipping some locations by applying a mask. Can be used, for example, to prevent reading locations which are implemented as FIFO pointers which are altered by reading them.

Memories can only be accessed when the device is in STOPPED mode.

Table 120. Memory Read masked command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_MEMORY_READ | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Type | 1 byte | Memory type to access. For overview of memory types see the section called “Memory Types”.
Address | 4 bytes | Start address (byte address) of memory to access.
Bytes | 4 bytes | Number of bytes to access. Payload restrictions apply
Mask | n/8 bytes | Mask to apply while reading. 1 bit per location byte, 0 = skip location, 1 = read location

Responses:

- DATA

- FAILED

Prev | Up | Next
| Home |