# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Disable debugWIRE

Resets the target and temporarily disables the debugwire interface.

In this state the debugWIRE module will no longer be in control of the /RESET pin. The value of the DWEN fuse is unaffected. Cycling power in this state will cause the debugWIRE module to regain control of the /RESET pin

Table 116. Disable debugWIRE command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_DISABLE_DEBUGWIRE | 1 byte | Command ID
Version (0x00) | 1 byte | Command version

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |