# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Page Erase

Performs a page-erase on the target.

Note: This can only be done during debug mode, not programming mode, and only applies to megaAVR (JTAG)

Table 122. Page Erase command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_PAGE_ERASE | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Address | 4 bytes | Start address (byte address) of flash page to erase

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |