# Atmel EDBG-based Tools Protocols
Responses

Sidebar | Prev | Up | Next

### DATA

Data is returned

Table 131. DATA response format version 0

Field | Size | Description
--- | --- | ---
RSP_AVR8_DATA | 1 byte | Response ID
Version (0x01) | 1 byte | Response version
Data | n bytes | Data returned
Status code | 1 byte | Trailing status of the read operation indicating whether the data returned is in fact valid. 0x00 = OK.

Prev | Up | Next
| Home |