# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Get ID

Retrieves the ID of the target. The same ID is returned by Activate Physical command. Any previously read value is not cached, but re-read from the target.

Table 104. Get ID command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_GET_ID | 1 byte | Command ID
Version (0x00) | 1 byte | Command version

Responses:

- DATA

- FAILED

Prev | Up | Next
| Home |