# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Deactivate Physical

De-activates the physical interface and disconnects from the target. After this, the debugger has no connection to the target.

Note: This may be done implicitly by another command.

Table 103. Deactivate Physical command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_DEACTIVATE_PHYSICAL | 1 byte | Command ID
Version (0x00) | 1 byte | Command version

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |