# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Run To

Resumes execution on the target, with an internal breakpoint at the given location. A break event is sent when the target has reached the breakpoint. (This breakpoint cannot be accessed by any other means.)

Table 110. Run To command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_RUN_TO_ADDRESS | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Address | 4 bytes | Address to run to (word address)

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |