# Atmel EDBG-based Tools Protocols
Serial trace commands

Sidebar | Prev | Up | Next

### Stop

Stops the data capture

Table 19. Stop

Field | Size | Description
--- | --- | ---
SERIAL_TRACE | 1 byte | 0x87
STOP | 1 byte | 0x04

Response:

Table 20. Stop response

Field | Size | Description
--- | --- | ---
SERIAL_TRACE | 1 byte | 0x87
STOP | 1 byte | 0x04
Status | 1 byte | Status code 0x00: OK 0xFF: Error

Prev | Up | Next
| Home |