# Atmel EDBG-based Tools Protocols
SPI programming protocol commands

Sidebar | Prev | Up | Next

### SPI Load Address

Loads address to be used for SPI programming

Table 139. SPI Load Address command format

Field | Size | Description
--- | --- | ---
SPI_CMD_LOAD_ADDRESS | 1 byte | Command ID
Address | 4 bytes | Start address of next command. MSB first

Response:

Table 140. SPI Load Address response format

Field | Size | Description
--- | --- | ---
SPI_CMD_LOAD_ADDRESS | 1 byte | Command ID
Status | 1 byte | SPI_STATUS_CMD_OK

Prev | Up | Next
| Home |