# Atmel EDBG-based Tools Protocols
Protocol commands

Sidebar | Prev | Up | Next

### Reset

Resets the target

Table 79. Writes the target reset register

Field | Size | Description
--- | --- | ---
AVR32_CMD_RESET | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Action | 1 byte | Device specific bits for reset register depending upon the number of reset domains specified for the device.

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |