# Atmel EDBG-based Tools Protocols
Protocol commands

Sidebar | Prev | Up | Next

### Activate Physical

Activates the selected physical interface, if necessary, and makes contact with the target interface. If no interface is detected, a FAILED response is returned else the device ID is returned.

Table 74. Activate Physical command format

Field | Size | Description
--- | --- | ---
AVR32_CMD_ACTIVATE_PHYSICAL | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Reset | 1 bytes | 0x00: no NOT use external reset 0x01: apply external reset during activation

Responses:

- DATA containing the 32-bit device ID (JTAGID or aWireID)

- FAILED

Prev | Up | Next
| Home |