# Atmel EDBG-based Tools Protocols
Protocol commands

Sidebar | Prev | Up | Next

### Read

Read memory

Table 81. Read command format

Field | Size | Description
--- | --- | ---
AVR32_CMD_READ | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Memory type | 1 byte | Memory type to access; see the section called “Memory Types”
Address | 5 bytes | Memory type dependent, usually SAB address.
Bytes | 4 bytes | Number of bytes to read. Note that memory type might put restrictions on number of bytes.

Responses:

- DATA

- FAILED

Prev | Up | Next
| Home |