# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Software Breakpoint Set

Inserts a set of software breakpoints on the target. Breakpoints are only inserted to flash when the next flow control command is executed.

Table 125. Software Breakpoint Set command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_SW_BREAKPOINT_SET | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
n x Address | n x 4 bytes | Address (byte address) list to break at. Note: n > 0; n < MAX_SW_BREAKS payload restrictions apply

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |