# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### GET

Used to get parameters on the tool..

For lists of valid get / set paramters, see the section called “SET/GET parameters”.

Table 97. Get

Field | Size | Description
--- | --- | ---
GET (0x02) | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Get context | 1 byte | Context of the parameter to get
Address | 1 byte | Parameter ID / start address
Bytes | 1 byte | Number of bytes to read

Responses:

- DATA

- FAILED

Note: Getting multiple parameters in one set call can only be done when all fields are in the same context.

Prev | Up | Next
| Home |