# Atmel EDBG-based Tools Protocols
EDBG-specific vendor commands

Sidebar | Prev | Up | Next

#### Set configuration

Sets board configuration parameters. Will only work with devices with HHB suffix.

Table 9. Set configuration command

Field | Size | Description
--- | --- | ---
SET_CONFIG | 1 byte | 0x84
Count | 1 byte | Number of bytes to write
ConfigID | 1 byte | Configuration packet ID
Data | N bytes | Configuration data

Response:

Table 10. Set configuration response

Field | Size | Description
--- | --- | ---
SET_CONFIG | 1 byte | 0x84
Status | 1 byte | 0x00: success other values: failed

Prev | Up | Next
| Home |