# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### SET

Used to set parameters on the tool..

For lists of valid get / set paramters, see the section called “SET/GET parameters”

Table 96. Set

Field | Size | Description
--- | --- | ---
SET (0x01) | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Set context | 1 byte | Context of the parameter to set
Address | 1 byte | Parameter ID / start address
Bytes | 1 byte | Number of bytes to write
Data | N bytes | Data to write

Responses:

- OK

- FAILED

Note: Setting multiple parameters in one set call can only be done when all fields are in the same context.

Prev | Up | Next
| Home |