# Atmel EDBG-based Tools Protocols
Protocol Commands

Sidebar | Prev | Up | Next

### Reset

Resets the target and holds it stopped, in reset. A break event will be sent when the reset is done and the target is stopped.

Table 107. Reset command format

Field | Size | Description
--- | --- | ---
CMD_AVR8_RESET | 1 byte | Command ID
Version (0x00) | 1 byte | Command version
Level | 1 byte | 0x01: stop at boot reset vector 0x02: stop at main address (deprecated)

Responses:

- OK

- FAILED

Prev | Up | Next
| Home |