# Atmel EDBG-based Tools Protocols
Events

Sidebar | Prev | Up | Next

#### Event: external reset

Indicates target external reset status

Table 68. EXTERNAL RESET event format

Field | Size | Description
--- | --- | ---
EVT_HOUSEKEEPING_EXT_RESET | 1 byte | Event ID
Version (0x00) | 1 byte | Event version
State | 1 byte | 0x00 = External reset has been released (rising edge) 0x01 = External reset has been applied (falling edge)

Prev | Up | Next
| Home |