# Atmel EDBG-based Tools Protocols
SPI programming protocol commands

Sidebar | Prev | Up | Next

### SPI Get Baud

Reads the clock frequency used for SPI programming

Table 143. SPI Get Baud command format

Field | Size | Description
--- | --- | ---
SPI_CMD_GET_BAUD | 1 byte | Command ID

Response:

Table 144. SPI Get Baud response

Field | Size | Description
--- | --- | ---
SPI_CMD_GET_BAUD | 1 byte | Command ID
Baud | 2 bytes | Current baud (kbit/s)
Status | 1 byte | SPI_STATUS_CMD_OK

Prev | Up | Next
| Home |