# Atmel EDBG-based Tools Protocols
Protocol commands

Sidebar | Prev | Up | Next

### Get ID

Retrieves the ID of the target. The same ID is returned by Activate Physical command. Any previously read value is not cached, but re-read from the target.

Table 76. Get ID command format

Field | Size | Description
--- | --- | ---
AVR32_CMD_GET_ID | 1 byte | Command ID
Version | 1 byte | Command version

Responses:

- ID - 32-bit device ID (JTAGID or aWire ID)

- FAILED

Prev | Up | Next
| Home |